Overview: 
This is a Request for Proposal for a church domes cleaning project in the Saint Louis, MO Area.  The domes are arranged on two levels ranging from 20 to 30 feet above ground.  Domes spherical part is made of re-enforced fiberglass with vertical copper siding fascia. 

Scope of work is as follows:

· Thoroughly clean the Re-enforced Fiberglass dome surface with gentle power wash or other appropriate methods.  Contractor to provide submittal of the cleaning method and any chemical agents to be used for the cleaning process for approval.

· Remove Any Dirt and Dust off the copper portion of the domes, wash down thoroughly with fresh water.
· Remove the patina layer using chemicals that are eco-friendly, and will not react with the building structure.  Contractor to provide submittal of the cleaning method and any chemical agents to be used for the cleaning process for approval.
· Polish copper domes with “Clear Resin Coating” to inhibit tarnish and reformation of copper oxides “patina”.  Contractor to provide submittal of the cleaning method and any chemical agents to be used for the cleaning process for approval.
· Protect surrounding structure and surfaces from chemicals and paint droppings. 

Project address is 1843 Ross Ave

St Louis, MO 63146-3818

(314) 878-2072

