Open Solicitation - Summary Notice

	
	

	Date Issued: 

 10/3/2008 

Title of Document: 

 Heat Fused Preformed Thermoplastic Material 

Deadline: 

 10/29/2008  prior to 11:00 AM   E.D.T.

Requisition Number: 

  

Delivery Point: 

 Clinton Township, MI 

Delivery Date: 

 As Required  

Type of Purchase: 

 Term: Nov 1, 2008 - October 31, 2009  

Construction Related: 

 No 

Type of Response Allowed: 

 Hard Copy Only 




	 Solicitation Summary 


	Issuing Agency: 

 Road Commission of Macomb County 

Using Department: 

 Sign Department  

 

Special Notices: 

  FOB Destination

 

 

Summary of Specifications:  

The markings shall be highly durable retro reflective thermoplastic materials designed for transverse, longitudinal, legend and symbol markings subjected to high urban traffic volumes and particularly severe wear conditions such as repeated shear action from crossover or encroachment on typical configurations such as crosswalks, edge lines and lane lines. 



	



ITB #08-40PRIVATE 

ROAD COMMISSION OF MACOMB COUNTY
COMMISSIONERS





FINANCE DIRECTOR

Chairperson:

Fran Gillett



Michelle M. Mykytiak
Vice-Chair:

Thomas Raymus


PURCHASING DIRECTOR


Commissioner:

Robert Sawicki



JoAnna Strizic

Invitation to Bid on:
One (1) Year’s Requirements of Heat Fused 




Preformed Thermoplastic Material



Release & Delivery As Required November 1, 2008 to October 31, 2009
Sealed bids will be publicly opened at 11:00 o'clock A.M., E.S.T. on Wednesday, October 29, 2008 at the office of the Road Commission of Macomb County, in the Macomb County Administration Building, 117 S. Groesbeck, Mt. Clemens, Michigan, 48043 for the furnishing of the above materials, services, equipment, work and/or supplies in accordance with the terms, conditions and specifications as stated herein and hereto attached.

1.
The Board reserves the right to reject any and all bids, to waive any informality in bids and unless otherwise specified by the bidder, to accept any items in the bid.  In case of error in the extension of prices in the bid or other arithmetical error, the unit prices will govern.

2.
The bid must be delivered in person or sent by mail to the Road Commission of Macomb County, 117 S. Groesbeck, Mt. Clemens, Michigan, 48043.  It shall be in a sealed envelope marked with the name and address of the bidder on the outside of the envelope.  The above referenced bid number should also be highlighted on the outside of the envelope.  Facsimile and/or e-mail transmitted bids will not be accepted.
3.
The bidder shall assume full responsibility for delivery of bids prior to the appointed hour for opening same and shall assume the risk of late delivery or non-delivery regardless of the manner employed for the transmission thereof.  Bids shall be accepted by the Board at any time during the normal course of business only, said hours being 8:00 am to 4:30 pm, Monday through Friday, legal holidays excepted.  A bidder may withdraw their bid response by written request at any time prior to the scheduled bid opening.  Any bid received after the scheduled opening time will not be accepted and will be returned unopened.  No bid may be withdrawn, changed, or modified in any way for a period of sixty (60) calendar days from the date of the bid opening.

4.
IT IS UNDERSTOOD THAT THE BOARD OF MACOMB COUNTY ROAD COMMISSIONERS IS A GOVERNMENTAL UNIT AND AS SUCH IS EXEMPT FROM THE PAYMENT OF ALL STATE AND FEDERAL TAXES APPLYING ON THE ABOVE MENTIONED ITEM AND ALL PRICES QUOTED SHALL NOT INCLUDE ANY SUCH TAX.

5.
The total price quoted by the Bidder must be the total cost delivered to the location(s).  All goods are to be shipped F.O.B.  Shipments sent C.O.D. without the Road Commission’s consent will not be accepted and will, at the Contractor’s risk and expense, be returned.  Unauthorized shipments are subject to rejection and returned at the Contractor’s expense.


6.
The bidder by execution of the proposal thereby declares that the bid is made without collusion with any other person, firm or corporation making any other bid, or who otherwise would make a bid, and agrees to furnish all bid items in strict accordance with all Federal Regulatory Measures.

7.
All bids must be submitted on the Board's form of bid blank.  The bid shall be legibly prepared in ink or typewriter.  Erasures or alterations must be initialed by the bidder.

8.
Submission of a bid will be construed as a conclusive presumption that the bidder is thoroughly familiar with the Bid Proposal and Specifications and that he understands and agrees to abide by each and all of the stipulations and requirements contained therein.

9.
In the specifications, whenever an article or material is defined by brand name, the name and catalog number of a particular manufacturer, vendor or a limited description, the term “OR APPROVED EQUAL” is written.  Any reference to a particular manufacturer’s product either by brand name or limited description is only for purposes of setting a standard of performance, quality, composition, construction or size.

10.
The Board reserves the right to award the bid for the equipment which best fits our needs and appears to be in the best interest of the Road Commission at the time the bids are evaluated.
11.
Bidders aggrieved by an award of any resulting contract may file a written notice of protest with the Purchasing Director within seven (7) calendar days of the award by the Board of County Road Commissioners.
12.
When applicable, contractor shall furnish material safety data sheets for their products.

13.
BIDDERS ARE REQUIRED TO SUBMIT DATA AND DESCRIPTIVE LITERATURE COVERING THE ITEM PROPOSED TO BE FURNISHED.  BIDS SUBMITTED WITHOUT THE ABOVE DOCUMENTATION MAY BE CONSIDERED NON-RESPONSIVE AND REJECTED.

14.
THIS BID BY MUTUAL AGREEMENT OF BOTH PARTIES, may be extended for additional one (1) year periods, each year hereafter, but not to exceed a maximum of two (2) additional years.

15.
Prior to furnishing the requested products and services, it shall be the responsibility of the awarded vendor to obtain all licenses and permits required to complete this contractual service, at no cost to the Road Commission.  These licenses and permits shall be readily available for review by the Administration and Purchasing Personnel.

16.
Vendors will provide a general history, description and status of their company.  

17.
All applicable Federal and State laws and rules and regulation over the project shall apply to the project contract throughout and will be deemed to be included in the contract herein written out in full.
18.
The Road Commission of Macomb County adheres to Title VI related requirements as outlined in USDOT Regulation 49 CFR-Part 26, Appendix A of MDOT Bidding Specifications, and the RCMC Policy #440.  The Road Commission of Macomb County is an Equal Opportunity Agency.

19.
The Road Commission of Macomb County will not pay fuel surcharges.

20.
The only official document is available over the internet at www.rcmcweb.org or www.mitn.info.

JoAnna Strizic




Deborah Scully

Purchasing Director



I/C & Stockroom Supervisor

(586) 791-3348




(586) 791-3373

Copies of Bids and Bid Tabs are available on the following  websites:

www.mitn.info or www.rcmcweb.org/viewpage/bids.cgi 

PROPOSAL
WE, THE UNDERSIGNED, agree to furnish to the Road Commission of Macomb County One (1) Year’s Requirements of Heat Fused Preformed Thermoplastic Material Release & Delivery As Required November 1, 2008 to October 31, 2009, conforming to the attached specifications at the pricing indicated as noted.  F.O.B., 34592 Nova, Clinton Township, Michigan.

Part No.


Size/Color

Price Per Linear Foot
_________________
6" White

__________________ ft.
No Quantity Guaranteed

_________________
12" White

__________________ ft.
No Quantity Guaranteed

_________________
24" White

__________________ ft.
No Quantity Guaranteed

_________________
12" Yellow

__________________ ft.
No Quantity Guaranteed

_________________
24" Yellow

__________________ ft.
No Quantity Guaranteed

_________________
9’4” Straight Arrow
__________________ ea.
No Quantity Guaranteed

_________________
8’ Left Arrow

__________________ ea.
No Quantity Guaranteed

_________________
8’ Right Arrow

__________________ ea.
No Quantity Guaranteed

_________________
8’ Only Legend  

__________________ ea.
No Quantity Guaranteed

_________________
School Kit 

__________________ ea.
No Quantity Guaranteed

_________________
“R” Kit 2/Kit   
  
__________________ ea.
No Quantity Guaranteed

_________________
Sealer


__________________ gal.
No Quantity Guaranteed

All prices firm for duration of the contract:  ________yes     __________no

COMPANY NAME:____________________________ 
ADDRESS:______________________________

CITY:____________________________STATE:_____ 
ZIP:____________________________________

PRINTED NAME:______________________________
SIGNATURE:____________________________

TITLE:________________________________________
DATE:__________________________________

PHONE NO.:__________________________________
FAX NO.:_______________________________

E-MAIL ADDRESS:_____________________________   TERMS:_________________________________


ROAD COMMISSION OF MACOMB COUNTYPRIVATE 


Specifications for:


PREFORMED THERMOPLASTIC MATERIAL
CLASSIFICATION

The markings shall be highly durable retro reflective thermoplastic materials designed for transverse, longitudinal, legend and symbol markings subjected to high urban traffic volumes and particularly severe wear conditions such as repeated shear action from crossover or encroachment on typical configurations such as crosswalks, edge lines and lane lines.
	PRIVATE 
COMPLIES WITH SPECIFICATIONS
	YES
	NO
	EXPLAIN DEVIATIONS

	    MATERIALS
	
	
	

	The retro reflective markings must be a resilient white or yellow thermoplastic product with uniformly distributed glass beads throughout the entire cross sectional area.
	
	
	

	The preformed retro reflective markings shall upon application exhibit uniform adequate nighttime retro reflectivity.  The markings shall have a pre-applied average minimum intensity of 300 millicandelas and a post-applied average minimum intensity of 500 millicandelas for white as measured with a Mirolux 30 retroreflectometer.  
	
	
	

	For the yellow a pre-applied average minimum intensity of 200 millicandelas and a post-applied average minimum intensity of 300 millicandelas as measured with a Mirolux 30 retroreflectometer.
	
	
	

	Daylight reflectance shall not change significantly when the preformed retro reflective thermoplastic is properly applied to the roadway surface.
	
	
	

	The marking material shall be impervious to motor fuels, lubricants, hydraulic fluids, etc.  
	
	
	

	The preformed retro reflective markings shall be fusible to asphalt and Portland Cement Concrete pavements by means of the normal heat of a propane torch applied directly to the tape, not to the pavement.  No preheating of the pavement to a specified temperature shall be required.  Adhesives, primers or sealers are not necessary prior to the preformed marking application on asphalt and Portland Cement concrete pavements.  On Portland Cement concrete pavements, a compatible primer sealer may be applied before application to assure proper adhesion.
	
	
	

	The material shall be packaged flat in three (3) foot lengths.  All boxes shall be clearly marked on the package edges for easy identification of contents.
	
	
	

	The material must be supplied at a minimum thickness of 125 mils.
	
	
	

	The material shall be capable of being applied down to temperatures of 32(F (0(C) without special conditions pertaining to storage or treatment of the material before application.
	
	
	

	Heat indicators shall act as a visual cue during application that the material has reached a molten state so satisfactory adhesion and proper bead embedment has been achieved and a post-application  visual cue that the installation procedures have been followed.
	
	
	

	It shall be capable of application on new, dense and open graded asphalt concrete wearing courses during the paving operation in accordance with the manufacturer's instructions
	
	
	

	Marking shall be available conforming to the current edition of the Manual on Uniform Traffic Control Devices.  In addition, markings shall meet state specifications and be approved for use by the appropriate state agency.
	
	
	


INSTALLATION PROCEDURE




The material shall be applied according the manufacturer instructions, which are included in the packaging.


