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NOTICE OF REQUEST FOR PROPOSALS

REQUEST FOR PROPOSALS: 
RFP 09-001

SERVICE: Golf Course Equipment and Services

ISSUE DATE: 12/17/08 

PROPOSAL DUE DATE: 
JANUARY 16, 2009 AT 2:00 PM

LOCATION:

Purchasing Department



13000 High Ridge Drive



Brighton, Michigan 48114



(810) 227-2757

DESCRIPTION: The Metroparks is soliciting proposals for the purchase of golf course and grounds maintenance turf maintenance equipment and services to operate and maintain the equipment at the Metropark Locations. The  contract period will be from January 2009 to December 31, 2011. This agreement will be subject to renewal annually agreed upon by both parties. Proposals will be evaluated based on criteria set forth in this proposal such as equipment quality, pricing, service and support, parts availability and training. It is the intent of this proposal to obtain a supplier who will provide the best value for the Authorities needs.  
Download this solicitation from our website at: www.metroparks.com Copies of the complete Request for Proposals documents may also be obtained from the Purchasing Department, 13000 High Ridge Drive, Brighton, Michigan 48114, (810) 227-2757.  

Proposals must be in the actual possession of the Purchasing Department at the location indicated, on or prior to the exact time and date indicated above. Proposals received by the correct time and date shall be publicly acknowledged.  Late proposals shall not be considered.

PROPOSERS ARE STRONGLY ENCOURAGED TO CAREFULLY READ THE ENTIRE REQUEST FOR PROPOSALS.

_________________________________________

Scott W. Michael, Purchasing Manager

THIS BID IS OFFERED BY: ______________________________________________

1.0 - GENERAL INFORMATION FOR THE RESPONDING FIRM

1.1
ISSUING OFFICE: This RFP is issued for the Huron-Clinton Metropolitan Authority (hereinafter referred to as the "Metroparks") through the Purchasing Office, which shall be referred to as the "Issuing Office."

1.2 
PROPOSALS: All proposals received by the Metroparks in response to this RFP will be retained.

A. 
Contractors must submit a complete, detailed response to this RFP.

B. 
Contractors must submit one (1) original and twelve (12) copies of each proposal directed to the Office of the Purchasing Manager, 13000 High Ridge Drive, Brighton, Michigan 48114.

C. 
Proposals must be signed by an individual authorized to bind the contractor to its provisions.

D. 
All proposals shall be tightly sealed in an opaque envelope and plainly marked with the Request for Proposal number, due date and the proposer's name and address clearly indicated on the envelope.

E.
Proposals must arrive in the Office of the Purchasing Department on or before the date and time indicated, Michigan time to be considered timely. Contractors mailing proposals should allow normal mail delivery time to ensure timely receipt of the proposal. Late proposals will not be accepted and will be returned to the proposer.

F.
All proposals submitted in response to this invitation shall become the property of the Metroparks.  Proposals shall be a matter of public record available for review, unless an exemption is requested and approved, in advance, for protection of trade secrets.  However, proposals shall not be considered fully received for the purpose of Freedom of Information Act requests until the Metroparks has determined that no additional clarifications or revisions of offers shall be accepted.

G.
Proposals are an irrevocable offer and may not be withdrawn within 90 days after the deadline for submission.  Submission of clarifications and revised offers automatically establish a new 90-day period.

H.
The Metroparks is not liable for any costs incurred by contractors prior to issuance of a contract.

I.
Before submitting a proposal, firms shall carefully examine the scope of work and shall fully inform themselves as to all existing conditions and limitations and shall indicate in the proposal all items requested.

1.3
PRE-PROPOSAL ASSISTANCE: Questions relative to the development of a proposal are to be directed to Scott Michael, in the Purchasing Office at (810) 227-2757.  

1.4
AWARD OF CONTRACT 

This project will be awarded to a single contractor who submits the proposal deemed to be in the best interest of the Metroparks, unless otherwise noted in this document. Notwithstanding any other provision of the Request for Proposal, the Metroparks reserves the right to: (1) waive any immaterial defect or informality; or (2) reject any or all proposals or portions thereof; or (3) reissue the Request for Proposal.

A response to any Request for Proposal is an offer to contract with the Metroparks based upon the terms, conditions, and specifications contained in the Metroparks Request for Proposal. Proposals do not become contracts unless and until the Metroparks executes them.  A contract has its inception in the award, eliminating a formal signing of a separate contract. For that reason, all of the terms and conditions of the contract are contained in the Request for Proposal, unless any of the terms and conditions is modified by a Request for Proposal amendment, a contract amendment, a Best and Final Offer, or by mutually agreed terms and conditions.

1.5
SPECIAL INFORMATION
A.
Addenda to the RFP:  In the event it becomes necessary to revise any part of the RFP, addenda will be provided to all contractors who are recorded as having received the RFP.

B.
News Releases:  News releases pertaining to this RFP or the services, study or project to which it relates will not be made without prior approval, and then only in coordination with the Issuing Office.

C.
Contract Compliance Program: The selected firm shall comply with relevant requirements of the Metroparks Contract Compliance/Affirmative Action Program. In addition, the firm selected must comply with all state and federal civil rights and equal employment opportunity laws.

1.6
INDEPENDENT PRICE DETERMINATION
By submission of a proposal, the Offeror certifies that in connection with this proposal:

A.
The fees in the proposal have been arrived at independently, without consultation, communication or agreement, for the purpose of restricting competition, as to any matter relating to such fees with any other Offeror or with any competitor; and,

B. 
Unless otherwise required by law, the fees which have been quoted in the proposal have not been knowingly disclosed by the Offeror directly or indirectly to any other Offeror or to any competitor; and,

C. No attempt has been made or will be made by the Offeror to induce any other person or firm to submit or not to submit a proposal for the purpose of restricting competition. 
2.0 - SCOPE OF WORK

The Metroparks is looking for a supplier of equipment to provide a full service to purchase equipment and support product accordingly. Proposals are to be submitted to the Purchasing Department which will provide sale, service and support of product. 
2.1 History of the Organization’s Fleet Management Operations:


The Metroparks has a diverse number of maintenance needs to maintain the park grounds and operations departments. In addition the park system operates and maintains 7 each 18 hole and 2 par 3 golf courses. Each 18 hole golf course has the average number of maintenance units to perform the day to day operations of each course. The staff manages a diverse range of equipment, ranging from walk behind units to large mowers. Most of the routine maintenance is performed at each site except specialized repairs. The staff includes 2 full time employees and several seasonal workers. The attached list of equipment is typical of the equipment at all the golf course and used in the park maintenance. 

The maintenance departments are set up for light duty to medium repairs. Most of the facilities are set up to do repairs and have at least one bay.  The park operations opens open 365 days of the year for operation with the golf courses opening early spring for regular business and weather permitting could go through the winter months. The complexes have there own fuel facility with both regular gas and diesel fuel. Future plans are to incorporate fuel management and merge with the equipment maintenance software system to track fuel consumption by unit.

It is the desire of the Metroparks to have a suppler to furnish equipment and provide dealer support to make the maintenance operation a well functioning operation. Attention to ease of maintenance, operator friendly design and reducing down time will be of primary importance in the operations and maintenance of equipment at this site. 
2.2
Training 
Operation and maintenance must be available to all staff on site.  Support services should be available by dealer from 8 to 8 Monday thru Friday. Dealer must provide regular onsite visits as requested as part of this service. In service training sessions on a regular basis are required.

2.3 Internet access

Manufacturer must have an easy access web site for maintenance and parts records. 
3.0 - SUBMITTAL REQUIREMENTS

3.1
EVALUATION CRITERIA:

All proposals received will be evaluated by the Metroparks for the purposes of selecting a firm.  The following factors, listed in relative order of importance, will be considered in making the selection:

A.  SERVICES AND SUPPORT
B.  QUALITY OF EQUIPMENT
C.  EXPERIENCE/QUALIFICATIONS
D.  DELIVERY
E.  PRICE 

D. Green Products 
The narrative portion and the materials presented in response to this RFP shall focus on these criteria and shall be submitted in the same order as requested. It must contain, at a minimum, all of the items listed below.

3.2
GENERAL SUBMITTAL REQUIREMENTS

The Offeror shall include a copy of the RFP with all necessary forms completed including:

* Offer and Acceptance Form

* Contract compliance forms contained in Attachment A

3.3 
SUBMITTAL REQUIREMENTS SPECIFIC TO EVALUATION CRITERIA:
A.
SERVICES AND SUPPORT
1. Describe the proposed overall program to accomplish the objectives of this proposal.
2. Supply a statement of what quantity and dollar amounts of parts on the average are stocked.

3. What is the proposed process of ordering parts and the turn around time to point of destination?
4. Describe the technical support services of the following areas:
A) Factory representatives
B) Internet Support for parts and service
C) Local dealer sales support
D) Dealer service department and service manager support

5. Describe the staff levels of the office including number of locations, sales, accounting, parts and service teams.

6. Describe the maintenance programs and what types of materials are included.

7. How are updates and service bulletins handled?

8. Describe the training, where it is conducted, type of training aids used, cost and who conducts the training?
9. Is loaner equipment available while equipment is in your shop for service and provide list of fleet available.
10. What is the ordering process and how is system set up for communicating data to accomplish this process.

B.
QUALITY OF EQUIPMENT
1. 
Provide literature and detailed explanation of equipment offered on this proposal. 
2. 
State in detail what aspects of design and engineering make the product advantageous to service and  
       operator comfort.


3. 
State in detail the warranty period and type offered on the equipment bid.
4. 
State the point of origin of manufacturing facilities and components.


C.  EXPERIENCE/QUALIFICATIONS

1. Provide a history of the Company.  

2. Describe professional staffing available for development, training, implementation, and support services. Include qualifications and experience.

3. Describe any special staffing resources in the areas of overall fleet management, equipment operations, equipment maintenance, and other management tasks.

4. Describe the general characteristics that differentiate your company from others in the industry. Including any special advantages your company and services you can provide.    

5. Describe installed base of customers in the southeaster Michigan area.

6. Provide a list of ten (10) agencies and municipal golf courses that your company is currently supplying product and service. 


D.  DELIVERY DATE
            1.  Provide an average delivery turn around after orders are placed.


E.  PRICE

1. Submit the Price Sheet attached herein.

2. Show how you arrived at the unit prices and total.
3. State discount offered on parts.

4. 
State length of term on pricing.

3.4
GENERAL
A.
The Metroparks anticipates short listing the responses based upon responses to the above items. If necessary, the Metroparks shall conduct interviews/demonstrations. However, the Metroparks may determine that short listing and/or interviews/demonstrations are not necessary. 

B.
The Metroparks reserves the right to make such additional investigations as it deems necessary to establish the competency and financial stability of any firm submitting a proposal.

C.
Experiences with the Metroparks and entities that evaluation committee members represent shall be taken into consideration when evaluating qualifications and experience.

D.
Exceptions to Contract Terms and Specifications

Offeror shall clearly identify any proposed deviations from the Contract Terms or Scope in the Request for Proposal. Each exception must be clearly defined and referenced to the proper paragraph in this RFP. The exception shall include, at a minimum, the Offeror's proposed substitute language and opinion as to why the suggested substitution will provide equivalent or better service and performance. If no exceptions are noted in the Offeror's proposal, the Metroparks will assume complete conformance with this specification and the successful Offeror will be required to perform accordingly. Alternate written proposals submitted may be considered; however, the Metroparks will make final determination as to suitability and compliance with the scope of service. Proposals submitted that do not meet all requirements might be rejected. Oral proposals will not be considered.

4.0 - GENERAL TERMS AND CONDITIONS

4.1
MATERIALS AND WORKMANSHIP: Unless otherwise specified, all materials and workmanship shall be new and of the best grade of their respective kinds for the purpose. Whenever an article, material or equipment is specified by name, a substitute of equal qualifications may be used upon the written approval of the Metroparks.

4.2
NON-DISCRIMINATION CLAUSE: The bidder agrees not to discriminate against any employee or applicant for employment, to be employed in the performance of such contract, with respect to hire, tenure, terms, conditions or privileges, of employment, or any matter directly or indirectly related to employment, because of race, color, religion, national origin, age, sex, height, weight, or marital status. Breach of this covenant may be regarded as material breach of the contract as provided for in Act 220 and Act 453 of the Public Acts of 1976, as amended, entitled "Michigan Handicapper's Civil Rights Act" and the Michigan Elliott Larson Civil Rights Act". The bidder further agrees to require similar provisions from any subcontractors, or suppliers.

4.3
ASSIGNMENT OF CONTRACT: The contractor shall assign no right or interest in this contract in whole or in part and no delegation of any duty of Contractor shall be made without prior written permission of the Metroparks.
4.4
INDEMNIFICATION: The contractor shall protect, defend, and save the Metroparks, its officials, employees, departments and agents harmless from and against any and all claims, demands, suits, actions, or proceedings of any kind or nature, in any way resulting from acts or omissions of the contractor or any of its agents, employees, boards, commissions, divisions, departments, or authorities in performing obligations under this agreement. Each party to this agreement agrees that any bond or insurance protection required by this agreement or otherwise provided shall in no way limit the terms of this indemnification provision. In case of any action or proceeding brought against the Metroparks by reason of any such claim, suit, action or demand, upon prompt notice from the Metroparks, contractor covenants to defend such action or proceeding by counsel that is reasonably satisfactory to the Metroparks.

4.5
CONTRACT: The contract shall contain the entire agreement between the Metroparks and the Contractor relating to this requirement and shall prevail over any and all previous contracts, proposals, negotiations, or master agreements in any form. By signing the Offer to Contract, it is understood and agreed to that the RFP in its entirety and all enclosed forms are fully incorporated herein as a material and necessary part of the contract. In case of conflicts, the following order shall prevail: 1) Addendum, 2) Specifications, 3) Special Terms and Conditions 4) General Terms and Conditions, 5) General Information.

4.6
PROVISIONS REQUIRED BY LAW: Each and every provision of law and any clause required by law to be in the contract shall be read and enforced as though it were included herein, and if through mistake or otherwise any such provision is not inserted, or is not correctly inserted, then upon the application of either party the contract shall forthwith be physically amended to make such insertion or correction.

4.7
RELATIONSHIP OF PARTIES: It is clearly understood that each party shall act in its individual capacity and not as an agent, employee, partner, joint venture, or associate of the other. An employee or agent of one party shall not be deemed or construed to be the employee or agent of the other party for any purpose whatsoever. The Contractor is advised that taxes or social security payments shall not be withheld from a Metroparks payment issued hereunder and that Contractor should make arrangements to directly pay such expenses, if any.

4.8
RIGHTS AND REMEDIES: No provision in this document or in the bidder's offer shall be construed, expressly or by implication as a waiver by either party of any existing or future right and/or remedy available by law in the event of any claim or default or breach of contract. The failure of either party to insist upon the strict performance of any term or condition of the contract or to exercise or delay the exercise of any right or remedy provided in the contract, or by law, or the acceptance of materials or services, obligations imposed by this contract or by law, and shall not be deemed a waiver of any right of either party to insist upon the strict performance of the contract.
4.9
ADVERTISING: Contractor shall not advertise, issue a press release or otherwise publish information concerning this RFP or contract without prior written consent of the Metroparks. The Metroparks shall not unreasonably withhold permission.

4.10
APPLICABLE REGULATIONS/POLICIES: The Revised Code of the State of Michigan, the Charter of the Huron-Clinton Metropolitan Authority, all local ordinances, Rules and Regulations and Policies shall apply. It shall be the responsibility of the Proposer to be familiar and comply with said regulations/policies.

4.11
ROYALTIES, PATENTS, NOTICES AND FEES: Contractor shall give all notices and pay all royalties and fees. S/he shall defend all suits or claims for infringement of any patent rights and shall save the Metroparks harmless from loss on account thereof. He shall comply with all laws, ordinances and codes applicable to any portion of the work.

4.12
SUBCONTRACTORS:  No subcontract shall be made by the contractor with any other party for furnishing any of the services herein contracted for without the advance written approval of the Metroparks.  All subcontractors shall comply with Federal and State laws and regulations which are applicable to the services covered by the subcontractor and shall include all the terms and conditions set forth herein which shall apply with equal force to the subcontract, as if the subcontractor were the Contractor referred to herein. Contractor is responsible for contract performance whether or not subcontractors are used.

4.13
PATENTS, COPYRIGHTS:  All services, information, computer program elements, reports, and other deliverables which may have a potential patent or copy right value and which are created under this contract shall be the property of the Metroparks and shall not be used by the contractor or any other person except with the prior written permission of the Procurement Agent.
5.0 - SPECIAL TERMS AND CONDITIONS

5.1
PRE-PROPOSAL CONFERENCE: Prospective bidders are invited to attend a pre-proposal conference. The date, time and location of this conference are indicated on the front page of this Request for Proposals. The purpose of this conference will be to clarify the contents of this Request for Proposals in order to prevent any misunderstanding of the Metroparks position. Any doubt as to the requirements of this Request for Proposals or any apparent omission or discrepancy should be presented to the Metroparks at this conference. The Metroparks will then determine the appropriate action necessary, if any, and issue a written amendment to the invitation for bid. Oral statements or instructions shall not constitute an amendment to this Request for Proposals.

5.2
KEY PERSONNEL:  It is essential that the contractor provide adequate experienced personnel, capable of and devoted to the successful accomplishment of work to be performed under this contract. The Contractor must agree to assign specific individuals to the key positions.

A.
The Contractor agrees that, once assigned to work under this contract, key personnel shall not be removed or replaced without written notice to the Metroparks.

B. If key personnel are not available for work under this contract for a continuous period exceeding thirty calendar days, or are expected to devote substantially less effort to the work than initially anticipated, the Contractor shall immediately notify the Metroparks, and shall, subject to the concurrence of the Metroparks, replace such personnel with personnel of substantially equal ability and qualifications.

5.3
CANCELLATION: The Metroparks reserves the right to cancel the whole or any part of this contract due to failure by the contractor to carry out any material obligation, term or condition of the contract. The Metroparks shall issue written notice to the contractor for acting or failing to act as in any of the following:

A.
The contractor fails to adequately perform the services set forth in the specifications of the contract:

B.
The contractor fails to make progress in the performance of the contract and/or gives the Metroparks reason to believe that the contractor will not or cannot perform to the requirements of the contract.

Upon receipt of the written notice of concern, the contractor shall have ten (10) days to provide a satisfactory response to the Metroparks. Failure on the part of the contractor to adequately address all issues of concern may result in the Metroparks resorting to any single or combination of the following remedies:

A.
Cancel any contract:

B.
Reserve all rights or claims to damage for breach of any covenant of the Contract:

C.
In case of default, the Metroparks reserves the right to complete the required work. The Metroparks may recover reasonable excess cost from the contractor by any remedies as provided by law.

5.4
INSURANCE: 

a. The Contractor shall at the time of execution of this contract, file with the Metroparks the Certificate of Insurance, which shall cover all of his insurance as required herein, including evidence of payment of premiums thereon, and the policy or policies or insurance covering said Metroparks and their officers, agents and employees. Each such policy and certificate shall be satisfactory to the Metroparks at least thirty (30) days prior notice thereof in writing. Nothing contained in these insurance requirements is to be construed as limiting the extent of the Contractor's responsibility for payment of damages resulting from his operations under this Contract.

b. The contractor shall maintain shall maintain insurances in force at all times during the term of this agreement at the minimum amounts and types as indicated.

Coverage Afforded









Limits of Liability



Workers' Compensation:   








$   100,000 or statutory limit

Commercial General Liability: 

Bodily Injury 


$1,000,000 each occurrence

(Including XCU if appropriate)

Property Damage 

$1,000,000 each occurrence









Or Combined Single Limit
$1,000,000

Automobile Liability: 



Bodily Injury


$   300,000 each person










Liability




$   500,000 each occurrence










Property Damage

$   500,000









Or Combined Single Limit
$   500,000

The Huron-Clinton Metropolitan Authority shall be listed as an additional insured on all liability coverage’s, and shall be provided with a Certificate of Insurance that reflects this additional insured status. A 30-day notice of cancellation or material change shall be provided to the Metroparks and so noted on the Certificate of Insurance. All certificates and notices shall be sent to Huron-Clinton Metropolitan Authority, 13000 High Ridge Drive, Brighton, Michigan 48014.



6.0 - PRICE SHEET

The quantities and items listed below are estimated for a 3 year period. This is a typical list that will be purchased but may vary form year to year. Not all of the items may be used in one year period. All prices are to include per specifications accessories listed and warranty. It is estimated that the annual average dollar value will be $600,000.
	ITEM NUMBER
	ESTIMATED QUANTITY
	DESCRIPTION
	UNIT PRICE (including all items specified and warranty)  

	1
	1 ONLY
	AERATOR FAIRWAY PTO DRIVE
	

	2
	2 ONLY
	AERATOR WALK BEHIND
	

	3
	4 ONLY
	MOWER ROTARY Bank/TRIM, 3 WD, 68” cut
	

	3a
	1 ONLY
	MOWER ROTARY Bank/TRIM, 2 WD, 68” cut
	

	4
	4 ONLY
	BUNKER/SAND TRAP RAKE RIDING 3 WHEEL
	

	5
	1 ONLY
	DEBRIS SWEEPER TRACTOR TOW ENGINE DRIVEN 
	

	6
	7 EACH
	MOWERS FAIRWAY, 5 ea 7-8”cutting units, 100 inch cut
	

	7
	1 SET 
	REELS GREENS REELS, 9-11 blade SET OF THREE 
	

	8
	1 SET 
	REELS THATCHING with rollers and scrapers SET OF THREE
	

	9
	1 SET
	ROLLERS TURF ROLLERS STATIC SET OF THREE
	

	10
	6 EACH
	MOWER GREENS TRIPLEX, 18 hp, power steering, 3 ea 9-11 blade CUTTING UNITS
	

	11
	5 ONLY
	MOWER ROTARY, 4 WD, 3 ea deck cutting units, 132 inch cut (11’)
	

	12
	2 ONLY
	SPRAYER 4 WHEEL 300 GALLON TANK HEAVY DUTY 
	

	13
	1 SET
	REELS TEE, 7- 8 blade 
	

	14
	6 EACH
	MOWER TEES TRIPLEX, 18 hp, power steering, 3 ea 7-8 blade CUTTING UNITS
	

	15
	5 ONLY
	WORK VEHICLE 4 WHEEL HEAVY DUTY  2 WD
	

	16
	1 ONLY
	BLOWER REAR MOUNT PTO DRIVE
	

	17
	1 ONLY
	SWEEPER, CORE COLLECTOR
	

	18
	2 ONLY
	BLOWER, TOW TYPE, ENGINE DRIVEN TURBINE TYPE
	

	19
	4 ONLY
	MOWER ROTARY UPFRONT 72” 2WD
	

	20
	4 ONLY
	MOWER ROTARY UPFRONT 72” 4WD
	

	21
	1 ONLY
	MOWER ROTARY CONTOUR, 109”, 5 CUTTING UNITS 
	

	22
	1 ONLY
	MOWER ROTARY CONTOUR, 150”, 7 CUTTING UNITS
	

	23 
	4 ONLY
	MOWER ROTARY, 4 WD, 3 ea deck cutting units, 192 inch cut (16’)
	

	24
	1 ONLY
	MOWER FAIRWAY, 4 wd, 7 ea 7-8”cutting units, 133 inch cut
	

	25
	1 ONLY
	WORK VEHICLE 4 WHEEL medium DUTY  2 WD
	

	26
	2 EACH
	SWEEPER TURF, RIDING SELF CONTAINED 
	

	27 
	1 ONLY
	CORE PROCESSOR
	


* See requirements section for details 

7.0 - OFFER AND ACCEPTANCE FORM

TO THE HURON-CLINTON METROPOLITAN AUTHORITY:

The Undersigned hereby offers and agrees to furnish the material or service in compliance with all terms, scope of work, conditions, specifications, and amendments in the Request for Proposal.

The undersigned hereby states, under penalty of perjury, that all information provided is true, accurate, and complete and states that he/she has authority to submit this proposal, which will result in a binding contract if accepted by the Huron-Clinton Metropolitan Authority.

We acknowledge receipt of the following addendum(s): _____, _____, _____, _____.

I certify, under penalty of perjury, that I have the legal authorization to bind the firm hereunder:








For clarification of this offer, contact:

Company Name









Name: 






Address









Phone:







City


State

Zip












Fax:






Signature of Person Authorized to Sign 





Printed Name

Title

ACCEPTANCE OF OFFER:

The Offer is hereby accepted. 










The Contractor is now bound to sell the materials or services listed by the attached contract and based upon the Invitation for Bid, including all terms, conditions, specification, amendments, etc. and the Contractor's Offer as accepted by the Metroparks.

This contract shall henceforth be referred to as Contract No. ___________. The Contractor has been cautioned not to commence any billable work or to provide any material or service under this contract until Contractor receives purchase order and/or a notice to proceed from the Huron-Clinton Metroparks Purchasing Manager.

COUNTERSIGNED:

Director







Date



Witness Signature

APPROVED AS TO FORM BY:

Attorney

__________________

Date

Project Name: 

Product Trade Name: ___________________________________ 

1.



Firm Name

2.


Address/City/State/Zip


Telephone



Fax Number 



County


3.



The name and address of the Headquarters/Home Office, if different from above.
4.
What is main function of your business? (Be specific.)

5.   Year established ________________

6.   Company ownership (if any) _________________________________________________________________

7.  Personnel in development and support, full time and total. __________________________________________

8.
Is the firm Minority Owned?


 

9.
Please include a copy of your current business license.

Authorized Signature

Position Title


EQUIPMENT SPECIFICATIONS AND SUPPLIER RESPONSE

Respond to each item listed.  Any bid which does not include a complete response may be deemed unresponsive.  Complete space provided with code and details of specifications.
RESPONSE CODES:

Y - Yes – meets requirements 
M – Modification necessary to meet specification or the application provides this functionality in a different way.  
N – No, system does not, and will not, meet this requirement

	AERATOR FAIRWAY PTO DRIVE
	
	NUMBER 1

	QUANTITY-1 EACH
	
	Bidders Response

	ENGINE
	Tractor 35 minimum 
	

	DRIVE
	540 PTO category 1, 3 point hitch
	

	GROUND SPEED
	0.5-2.3 mph aerating 
	

	SPACING
	Lateral 1.3 to 2.6 inch
	

	
	Forward 1.0 to 4.5 inches
	

	
	
	

	ACCESSORIES
	None
	

	HEADS
	
	

	NUMBER
	8(six)
	

	TYPE
	Capable of several size head kits
	

	
	
	

	AERATION WIDTH
	64 inch approx.
	

	AERATION DEPTH
	Up to 5” maximum
	

	
	
	

	ACCESSORIES
	Heads 3 (three) tine, tines ¾” hollow steel HD side eject
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	ANSI
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


	AERATOR GREENS WALK BEHIND
	
	NUMBER 2

	
	
	Bidders Response

	ENGINE
	2-cylinder 23 hp 4 cycle gas OH valve air cooled
	

	TRANSMISSION-TRACTION DRIVE 
	3 wd Hydrostatic
	

	GROUND SPEED
	0-3.5mph forward & 0-2 mph reverse variable and .075 to 1.5 mph aerating 
	

	SPACING
	1.5 to 3 inch
	

	HYDRAULIC OIL TYPE & CAPACITY
	Biodegradable Mobil EAL  preferred
	

	TIRE SIZE
	
	

	BRAKES 
	Dynamic through hydrostatic w/parking brake
	

	STEERING
	Hand control
	

	GAUGES
	Hour meter
	

	ACCESSORIES
	
	

	HEADS
	
	

	NUMBER
	6(six)
	

	TYPE
	Capable of several size head kits
	

	AERATION WIDTH
	48 inch preferred
	

	ROLLERS  
	Solid for solid core application, lifts for transport
	

	
	
	

	ACCESSORIES
	2(two) head kits, mini(10) and 4 tine, tines ¼” core side eject, ½” hollow
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


	MOWERS BANK -TRIM ROTARY
	
	NUMBER 3 & 3a

	QUANTITY-1 only
	
	Bidders Response

	ENGINE
	35 hp diesel water cooled
	

	TRANSMISSION-TRACTION DRIVE 
	3 or 4 wheel drive hydrostatic, series parallel preferred, 3a – 2 or wheel drive
	

	GROUND SPEED
	0-6 mph maximum mowing
	

	HYDRAULIC OIL TYPE & CAPACITY
	Mobil 15M or equal
	

	TIRE SIZE-FRONT
	
	

	                     REAR
	
	

	BRAKES 
	Dynamic with emergency
	

	STEERING
	Power 
	

	GAUGES
	Hour meter, fuel, engine temp & pressure, emergency warning lights and shut down for high coolant temperature.
	

	ACCESSORIES
	Work light kit
	

	CUTTING UNITS
	
	

	NUMBER
	3(three) each  independent flotation, side shift design, 3a - stationary design
	

	TYPE
	 Rotary, rear discharge preferred,  spindle grease- able
	

	Blades
	Heavy duty std. lift
	

	CUTTING RANGE HEIGHT & WIDTH
	.75 to 4 inch, 68 inch width
	

	ROLLERS 
	Rear, one per deck, for stripping
	

	ACCESSORIES
	
	

	SAFETY FEATURES
	2 post ROPS 
	

	SEAT
	Standard with arm rest and seat belt 
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	Manufacturer and Model
	
	

	
	
	

	ALLIED ITEMS
	Sun Guard Canopy w/beacon light mounted on ROPS
	

	MFG & PART NUMBER
	
	


	BUNKER/SAND TRAP RAKE RIDING 3 WHEEL
	
	NUMBER 4

	
	
	Bidders Response

	ENGINE
	2-cylinder 16 hp 4 cycle gas OH valve air cooled
	

	TRANSMISSION-TRACTION DRIVE 
	2 wd hydrostatic 
	

	ELECTRICAL 
	12 volt electric start
	

	GROUND SPEED
	Variable 0-11mph forward & 0-4 mph reverse   
	

	CONTROLS
	Hydraulic for raising/lowering float & foot pedal traction F&R
	

	HYDRAULIC OIL TYPE & CAPACITY
	Biodegradable Mobil EAL 
	

	TIRE SIZE
	Low pressure
	

	BRAKES 
	Dynamic through hydrostatic w/parking brake
	

	STEERING
	Manual front steering 
	

	SEAT
	Deluxe w/fore/aft adjustment
	

	GAUGES
	Hour meter
	

	DOZER WIDTH
	36 inch minimum
	

	ACCESSORIES (REQUIRED)
	dozer blade, tooth rake and cultivator
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	ANSI
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	Unit price
	
	

	
	
	

	ALLIED ITEMS (Required)
	Work lights
	

	Part number
	
	

	
	
	


	DEBRIS SWEEPER TRACTOR TOW ENGINE DRIVEN 
	SPECIFICATIONS
	NUMBER 5

	
	
	Bidders Response

	ENGINE
	2 cylinder 22 hp air cooled gas engine preferred or PTO
	

	DESIGN
	Tractor Drawn, low center of gravity
	

	HITCH
	Pin type ¾”
	

	DRIVE
	Banded double
	

	FAN IMPELLER
	Centrifugal type, 4 blade minimum
	

	REEL/BRUSH DRIVE
	Belted double 
	

	HOPPER SIZE
	5 ¾ cubic yard
	

	TIRES 
	High flotation
	

	POWER HEAD
	Flex tip Reel kit
	

	
	
	

	
	
	

	
	
	

	SWEEPING WIDTH
	60 inches approx.
	

	
	
	

	
	
	

	
	
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	ANSI
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


	MOWERS FAIRWAY
	
	NUMBER 6

	
	
	Bidders Response

	ENGINE
	35 hp diesel water cooled
	

	TRANSMISSION-TRACTION DRIVE 
	2 wheel drive hydrostatic
	

	GROUND SPEED
	8 mph maximum mowing
	

	HYDRAULIC OIL TYPE & CAPACITY
	Citgo HYD 68 or equal
	

	TIRE SIZE-FRONT
	
	

	                     REAR
	
	

	BRAKES 
	Dynamic with emergency
	

	STEERING
	Power 
	

	GAUGES
	Hour meter, fuel, engine temp & pressure, emergency warning lights and shut down for high coolant temperature.
	

	ACCESSORIES
	Work light kit
	

	CUTTING UNITS
	
	

	NUMBER
	5 each
	

	TYPE
	7-8 blade, 7 inch diameter, grease able bearing 
	

	BEADKNIFE
	Fairway thicker high alloy heavy duty
	

	CUTTING RANGE HEIGHT & WIDTH
	.5 to 1 inch, 100 inch width
	

	ROLLERS  FRONT
	Front-3 inch nylon Wiehle 
	

	ROLLERS REAR
	3 inch solid steel with scraper
	

	ACCESSORIES
	Diagnostic tool
	

	SAFETY FEATURES
	4 post ROPS with canopy and Mesh protective cover enclosure
	

	SEAT
	Deluxe with seat belt 
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	


	SEPARATE EQUIPMENT
	GREENS MOWERS
	NUMBER 7, 8 & 9

	
	
	Bidders Response

	1 SET OF THREE GREENS REELS 
	Same specifications on greens mower s
	

	Manufacturer and model/part number
	
	

	Unit price/set
	
	

	1 SET OF THREE THATCHING REELS with rollers and scrapers
	For greens mower
	

	Manufacturer and model/part number
	
	

	Unit price/set
	
	

	1 SET OF THREE TURF ROLLERS STANDARD
	For greens mower, static type
	

	Manufacturer and model/part number
	
	

	
	
	


	MOWERS GREENS
	
	NUMBER 10

	
	
	Bidders Response

	ENGINE
	18 hp 4 cycle gas OH valve air cooled, low dB(a) level, Quiet muffler 
	

	NOISE LEVEL 
	dB(a) level
	

	TRANSMISSION-TRACTION DRIVE 
	Hydrostatic 
	

	GROUND SPEED
	
	

	HYDRAULIC OIL TYPE & CAPACITY
	Biodegradable Mobil EAL
	

	TIRE SIZE
	
	

	BRAKES 
	
	

	STEERING
	Power 
	

	GAUGES
	
	

	ACCESSORIES
	Work light kit
	

	CUTTING UNITS
	
	

	NUMBER
	3(three)
	

	TYPE
	11 blade, grease able or sealed bearing 
	

	BEADKNIFE
	tournament
	

	CUTTING RANGE HEIGHT & WIDTH
	.062 height of cut range, 59 inch cutting width
	

	ROLLERS  FRONT
	Front-Aluminum Wiehle Narrow spacing
	

	ROLLERS REAR
	Smooth steel with scraper
	

	ACCESSORIES
	Baskets & rear roller brushes
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


	MOWERS ROTARY
	
	NUMBER 11

	
	
	Bidders Response

	ENGINE
	60 hp diesel water cooled
	

	TRANSMISSION-TRACTION DRIVE 
	All wheel drive hydrostatic and 2 wd in transport
	

	GROUND SPEED
	0-8 mph maximum mowing
	

	HYDRAULIC OIL TYPE & CAPACITY
	Citgo HYD 68 or equal
	

	TIRE SIZE-FRONT
	
	

	                     REAR
	
	

	BRAKES 
	Internal wet disc or  equal with emergency
	

	STEERING
	Power 
	

	GAUGES
	Hour meter, fuel, engine temp & pressure, emergency warning lights and shut down for high coolant temperature.
	

	ACCESSORIES
	Work light kit
	

	CUTTING UNITS
	
	

	NUMBER
	3(three) each 
	

	TYPE
	 Rotary, rear discharge,  spindle grease able anti scalping
	

	Blades
	Heavy duty std. lift
	

	CUTTING RANGE HEIGHT & WIDTH
	1 to 5 inch, 132 inch width
	

	CASTER WHEELS 
	Smooth, low puncture
	

	
	
	

	ACCESSORIES
	Leaf mulch kit
	

	SAFETY FEATURES
	2 post ROPS 
	

	SEAT
	Premium suspension w/arm rests
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	Unit price (EACH)
	
	

	TOTAL 
	
	

	
	
	

	ALLIED ITEMS
	Sun Guard Canopy  mounted on ROPS
	

	MFG & PART NUMBER
	
	

	
	
	


	
SPRAYER 4 WHEEL HEAVY DUTY 
	SPECIFICATIONS
	NUMBER 12

	QUANTITY-1 EACH
	
	Bidders Response

	ENGINE
	3 cylinder 35 hp liquid cooled 4 cylinder diesel engine 
	

	TRANSMISSION/DRIVE
	Hydrostatic driving rear wheel motors or approved equal
	

	GROUND SPEED
	0-10 mph forward
	

	RADIATOR
	Mid mount easy access
	

	STEERING
	Power
	

	BRAKES
	4-wheel multi disc wet with parking brake.
	

	CONTROLS
	Foot operated traction pedal, brake, sprayer and speed lock system
	

	GUAGES
	Sprayer pressure, fuel, engine temp, oil pressure and hour meter
	

	LIGHTS
	Front head, Work (2 facing rear), and necessary wire harnesses 
	

	SEATS
	Twin with back rests and hip restraints and seat belts
	

	TIRES 
	Turf tread
	

	TIRE SIZES-FRONT
	
	

	                      REAR
	
	

	TIRE TYPE
	Low ground pressure
	

	TANK
	300 gallon high density poly with 16 inch inlet
	

	PUMP
	Dual diaphragm 30 gpm
	

	AGITATOR
	Jet
	

	OPTIONS EQUIPMENT REQUIRED
	Pro Control Ravin or equal computer control system with foam marker kit. Unit must be capable of ground speed control to maintain uniform application of chemicals and give accurate amounts for record keeping. 
	

	SPRAY BOOM
	Folding 3 section, electric lift with 20 inch nozzle spacing and JD “Turbo Rain Drop” nozzles, triangular truss style
	

	SAFETY FEATURES
	ROPS-2 post with 2 work lights mounted facing sprayer
	

	CERTIFICATION
	ANSI
	

	WARRANTY
	
	

	Manufacturer and Model
	
	

	 
	
	


	REELS TEE
	
	NUMBER 13

	SEPARATE EQUIPMENT
	
	Bidders Response

	
	
	

	1 SET OF THREE TEE REELS 
	Same specifications as  Tee Mowers
	

	Manufacturer and model/part number
	
	

	
	
	


	MOWERS TRIPLEX TEES
	
	NUMBER 14

	
	
	Bidders Response

	ENGINE
	18 hp 4 cycle gas OH valve air cooled, low dB(a) level, Quiet muffler
	

	NOISE LEVER
	dB(a) level rating
	

	TRANSMISSION-TRACTION DRIVE 
	Hydrostatic
	

	GROUND SPEED
	
	

	HYDRAULIC OIL TYPE & CAPACITY
	Biodegradable Mobil EAL
	

	TIRE SIZE
	
	

	BRAKES 
	
	

	STEERING
	Power 
	

	GAUGES
	Hour
	

	ACCESSORIES
	Work light kit
	

	CUTTING UNITS
	
	

	NUMBER
	3(three)
	

	TYPE
	7-8 blade, grease able or sealed bearing 
	

	BEADKNIFE
	High cut
	

	CUTTING RANGE HEIGHT & WIDTH
	.5 cutting height, range .312 to 1.00, 59 inch width of cut
	

	ROLLERS  FRONT
	Front-Aluminum Wiehle Narrow spacing
	

	ROLLERS REAR
	Smooth steel with scraper
	

	ACCESSORIES
	Baskets
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	


	WORK VEHICLE 4 WHEEL HEAVY DUTY 
	SPECIFICATIONS
	NUMBER 15

	QUANTITY-1 EACH
	
	Bidders Response

	ENGINE
	3 cylinder 31-32 hp liquid cooled 4 cycle gas engine, EFI 
	

	TRANSMISSION/DRIVE
	Rear transaxle drive, 3-speed synchromesh with high-low range and lockout for high gear
	

	CLUTCH
	6-7 inch
	

	RADIATOR
	Side mount easy access
	

	STEERING
	Power
	

	BRAKES
	4-wheel hydraulic, self adj.
	

	INSTUMENT PANEL
	Fuel, engine temp, oil pressure horn, hour meter, speedometer and tachometer
	

	LIGHTS
	Front head, Work, brake, turn signal, safety beacon and necessary wire harnesses 
	

	SEATS
	Twin with back and hip restraints, seat belts
	

	TIRES 
	Turf tread
	

	TIRE SIZES-FRONT
	
	

	                      REAR
	
	

	BED
	Full with sides and fold down tail gate, hydraulic lift
	

	HITCH
	Heavy duty draw bar
	

	RATED CAPACITY
	1500 lbs. minimum
	

	ACCESSORIES
	Auxiliary hydraulics, high flow 8 gpm to accommodate core harvester 
	

	
	
	

	SAFETY FEATURES
	ROPS-2 post and horn
	

	
	
	

	CERTIFICATION
	ANSI
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	

	
	
	

	
	
	


	BLOWER 3 point type
	
	NUMBER 16

	Quantity 1 only
	SPECIFICATIONS
	Bidders Response

	
	
	

	ENGINE
	Tractor driven, 25 hp min.
	

	TRANSMISSION-TRACTION DRIVE 
	P.T.O, 3 point hitch category 1 belt drive fan
	

	GROUND SPEED
	
	

	FAN SPEED
	1173 rpm at 540 pto impute
	

	AIR FLOW
	7000 cfm approx.
	

	TIRE SIZE
	
	

	CONTROL 
	Manual directional
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	


	SWEEPER CORE HARVESTER TOW TYPE HYD DRIVE
	SPECIFICATIONS
	NUMBER 17

	QUANTITY 1 ONLY
	
	BIDDERS RESPONSE

	ENGINE OR POWER

SYSTEM
	Auxiliary hydraulics  8 GPM from work vehicle or tractor
	

	COLLECTION SYSTEM DRIVE 
	Hydraulic powered rotary brush
	

	BRUSH SPEED
	0-4 mph forward
	

	ROLLER
	6” full width directly behind brush, adjustable to set brush height or alternative turf applications
	

	HOPPER CAPACITY
	25 cubic feet approx
	

	
	
	

	HITCH
	¾ inch pin
	

	TOW HITCH DESIGN 
	Directly behind or offset 
	

	LIFT
	Hydraulic lift cylinder
	

	HYDRUALIC CONNECTION
	Dual quick couplers w/hose with dash mount control
	

	TIRE SIZE
	
	

	TIRE TYPE
	High flotation type
	

	
	
	

	SWEEPING WIDTH
	52”
	

	
	
	

	
	
	

	WEIGHT
	
	

	
	
	

	
	
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	
	

	
	
	

	MANUFACTURER AND MODEL
	
	

	
	
	

	WARRANTY
	
	

	
	
	


	BLOWER, ENGINE DRIVEN TOW TYPE
	
	NUMBER 18

	
	SPECIFICATIONS
	BIDDERS RESPONSE

	ENGINE/POWER SOURCE
	23-27 hp gas engine 
	

	Control
	remote wireless electric start/stop, chute and throttle
	

	GENERAL 
	Tow type, engine driven designed to be towed by work vehicle or tractor
	

	DRIVE SYSTEM
	Direct drive axial type
	

	DIRECTION CONTROL
	Single piece chute, 360 degree rotation with wireless remote control 
	

	HITCH ADJUSTMENT
	Adjustable with tong extension to clear tow vehicle
	

	GROUND CLEARANCE
	Sufficient for most conditions with adjustment depending on tow vehicle and hitch adjustment
	

	FAN HOUSEING 
	Heavy Duty 
	

	
	
	

	
	
	

	TIRE SIZE
	
	

	TIRE TYPE
	High flotation turf
	

	WHEELS (TWO)
	STEEL
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	


	MOWERS ROTARY UPFRONT 72”
	
	NUMBER 19 & 20

	
	
	Bidders Response

	ENGINE
	25 hp diesel water cooled
	

	TRANSMISSION-TRACTION DRIVE 
	2 or 4 wheel drive hydrostatic, rear mechanical
	

	GROUND SPEED
	0-10 mph maximum mowing
	

	HYDRAULIC OIL TYPE & CAPACITY
	Mobil 424 or equal
	

	TIRE SIZE-FRONT
	
	

	                     REAR
	
	

	BRAKES 
	Dynamic with emergency
	

	STEERING
	Power 
	

	GAUGES
	Hour meter, fuel, engine temp & pressure, emergency warning lights and shut down for high coolant temperature. 
	

	ACCESSORIES
	Work light kit
	

	CUTTING UNITS
	
	

	NUMBER
	One deck with 3(three) each  blades 
	

	TYPE
	 Rotary, rear discharge preferred,  spindle grease- able
	

	Blades
	Heavy duty std. lift
	

	CUTTING RANGE HEIGHT & WIDTH
	1 to 4 inch, 72 inch width
	

	SUSPENSION & CASTER WHEELS
	Two front and rear, foam filled with anti-scalp F & R
	

	ACCESSORIES
	
	

	SAFETY FEATURES
	2 post ROPS 
	

	SEAT
	Standard with arm rest and seat belt 
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	ALLIED ITEMS
	Sun Guard Canopy w/beacon light mounted on ROPS
	

	MFG & PART NUMBER
	
	

	
	
	

	
	
	


	MOWERS ROTARY CONTOUR 
	
	NUMBER 21 & 22

	
	
	Bidders Response

	ENGINE
	60 hp diesel water cooled
	

	TRANSMISSION-TRACTION DRIVE 
	All wheel drive hydrostatic and 2 wd in transport
	

	GROUND SPEED
	0-8 mph maximum mowing
	

	HYDRAULIC OIL TYPE & CAPACITY
	Citgo HYD 68
	

	TIRE SIZE-FRONT
	
	

	                     REAR
	
	

	BRAKES 
	Internal wet disc or  equal with emergency
	

	STEERING
	Power 
	

	GAUGES
	Hour meter, fuel, engine temp & pressure, emergency warning lights and shut down for high coolant temperature.
	

	ACCESSORIES
	Work light kit
	

	CUTTING UNITS
	
	

	NUMBER
	5 (five) each & 7 (seven) 
	

	TYPE
	 Rotary, rear discharge,  spindle grease able anti scalping
	

	Blades
	Heavy duty std. lift
	

	HEIGHT  CUT
	¾ to 4 inch, 
	

	WIDTH OF CUT
	5 unit – 109”, 7 unit – 150”
	

	CASTER WHEELS 
	Smooth, low puncture
	

	
	
	

	ACCESSORIES
	Leaf mulch kit
	

	SAFETY FEATURES
	2 post ROPS 
	

	SEAT
	Premium suspension w/arm rests
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	Unit price (EACH)
	
	

	TOTAL 
	
	

	
	
	

	ALLIED ITEMS
	Sun Guard Canopy  mounted on ROPS
	

	MFG & PART NUMBER
	
	

	
	
	


	MOWERS ROTARY 3 DECK, 192”
	
	NUMBER 23

	
	
	Bidders Response

	ENGINE
	90 hp minimum diesel water cooled
	

	TRANSMISSION-TRACTION DRIVE 
	All wheel drive hydrostatic and 2 wd in transport
	

	GROUND SPEED
	0-8 mph maximum mowing
	

	HYDRAULIC OIL TYPE 
	Citgo HYD 68 or equal
	

	HYD OIL CAPACITY
	
	

	TIRE SIZE-FRONT
	
	

	                     REAR
	
	

	BRAKES 
	Internal wet disc or  equal with emergency
	

	STEERING
	Power 
	

	GAUGES
	Hour meter, fuel, engine temp & pressure, emergency warning lights and shut down for high coolant temperature.
	

	ACCESSORIES
	Work light kit & Road Light Kit
	

	CUTTING UNITS
	
	

	NUMBER
	3(three) each 
	

	TYPE
	 Rotary, rear discharge,  spindle grease able anti scalping
	

	Blades
	Heavy duty std. lift
	

	CUTTING RANGE HEIGHT 
	1 to 6 inch
	

	OVERALL WIDTH CUT
	192”
	

	CASTER WHEELS 
	Smooth, low puncture
	

	
	
	

	ACCESSORIES
	Leaf mulch kit
	

	SAFETY FEATURES
	2 post ROPS 
	

	SEAT
	Premium suspension w/arm rests
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	Manufacturer and Model
	
	

	Unit price (EACH)
	
	

	TOTAL 
	
	

	ALLIED ITEMS
	Sun Guard Canopy  mounted on ROPS
	

	MFG & PART NUMBER
	
	

	
	
	


	MOWERS FAIRWAY
	
	NUMBER 24

	
	
	Bidders Response

	ENGINE
	46 hp diesel water cooled
	

	TRANSMISSION-TRACTION DRIVE 
	2 wheel drive hydrostatic with 4 WD on demand
	

	GROUND SPEED
	10 mph maximum mowing
	

	HYDRAULIC OIL TYPE & CAPACITY
	Mobil 424 or equal 
	

	TIRE SIZE-FRONT
	
	

	                     REAR
	
	

	BRAKES 
	Dynamic with emergency
	

	STEERING
	Power 
	

	GAUGES
	Hour meter, fuel, engine temp & pressure, emergency warning lights and shut down for high coolant temperature.
	

	ACCESSORIES
	Work light kit
	

	CUTTING UNITS
	
	

	NUMBER
	7 each
	

	TYPE
	22” wide, 7-8 blade, 7 inch diameter, grease able bearing 
	

	BEADKNIFE
	Fairway thicker high alloy heavy duty
	

	CUTTING RANGE HEIGHT & WIDTH
	.25 to 1 inch, 133 inch width
	

	ROLLERS  FRONT
	Front-3 inch nylon Wiehle 
	

	ROLLERS REAR
	3 inch solid steel with scraper
	

	ACCESSORIES
	Diagnostic tool
	

	SAFETY FEATURES
	4 post ROPS with canopy and Mesh protective cover enclosure
	

	SEAT
	Deluxe with seat belt 
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	


	WORK VEHICLE MD 
	SPECIFICATIONS
	NUMBER 25

	
	
	Bidders Response

	ENGINE
	Single cylinder 12 hp air cooled 4 cycle gas engine, EFI 
	

	MAXIMUM SPEED
	15-16 MPH
	

	TRANSMISSION/DRIVE
	Continuously variable belt drive
	

	STEERING
	Manual
	

	BRAKES
	4 wheel hydraulic disk
	

	FRAME
	Steel, heavy duty, e-coat or equal
	

	SUSPENSION
	Torsion independent “A” frame front and active frame rear capable of meeting weight requirements
	

	FUEL CAPACITY
	7 gallons
	

	GROUND CLEARANCE
	6” minimum
	

	INSTUMENT PANEL
	Fuel, hour meter 
	

	LIGHTS
	Front head, brake/tail, turn signal, safety beacon and necessary wire harnesses 
	

	SEATS
	Twin, with side braces and seat belts
	

	BODY
	Constructed of dent and corrosion resistant plastic.
	

	TIRES 
	Turf tread
	

	TIRE SIZES-FRONT
	
	

	                      REAR
	
	

	BED
	Full with sides and fold down tail gate, electric lift
	

	BED CAPACITY
	 800 lbs minimum
	

	CARGO BED SIZE
	49” length, 52” width and approximately 10” sides
	

	HITCH
	Standard Hitch
	

	RATED TOTAL CAPACITY
	1200 lbs minimum
	

	TRAILER TOWING CAPACITY
	400 lbs. trailer, and 50 lbs. tongue weight
	

	ACCESSORIES
	ROPS, Canopy, folding windshield, HD bumper & light kits (see above)
	

	SAFETY FEATURES
	ROPS-2 post and horn
	

	
	
	

	CERTIFICATION
	ANSI
	

	WARRANTY
	
	

	Manufacturer and Model
	
	


	TURF SWEEPER RIDING TYPE 
	SPECIFICATIONS
	NUMBER 26

	
	
	Bidders Response

	ENGINE
	2 cylinder 18 hp air cooled gas engine preferred
	

	DESIGN
	Self Contained unit
	

	
	
	

	TRACTION DRIVE
	Sunstrand 15 pump with wheel motors or equal
	

	REEL PICKUP
	Belt Drive, Dual Rubber finger reels
	

	REEL ENGAGEMENT
	2 Position reel height adjustment
	

	HOPPER SIZE
	1 ¼  cubic yard capacity
	

	TIRES 
	High flotation
	

	TIRE SIZES 
	
	

	
	
	

	SWEEPING WIDTH
	48 inches approx.
	

	
	
	

	
	
	

	
	
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	ANSI
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


	CORE PROCESSOR

PULL TYPE ENGINE DRIVEN
	
	NUMBER 

	
	
	Bidders Response

	ENGINE
	2-cylinder 35 hp 4 cycle gas 
	

	FUEL CAPACITY
	10 gallons
	

	PROCESSING WIDTH
	70” preferred for productivity
	

	PROCESSING SYSTEM
	Belt drive nylon brush sweeps 
	

	OPERATING SPEED
	1-5 MPH
	

	ROLLER
	6” diameter full width rear roller
	

	CONSTRUCTION
	Welded steel frame
	

	HITCH SYSTEM
	Piggy back for single pass capable of behind aerator. Offset design for hitching to HD work vehicle.
	

	CONTROLS
	Engine mounted key switch, choke and throttle. Remote kill and offset control.
	

	TIRE SIZE
	
	

	WEIGHT
	2200 lbs. approx
	

	
	
	

	OPTIONS AVAILABLE
	
	

	
	
	

	
	
	

	SAFETY FEATURES
	
	

	
	
	

	CERTIFICATION
	
	

	WARRANTY
	
	

	
	
	

	Manufacturer and Model
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