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Number:  12704


PR Number:	017727	Procurement Officer:	Linda Gronquist
Replaces Contract:	n/a	Telephone: 	785-296-2375
Date Mailed:		E-Mail Address:	linda.gronquist@da.ks.gov  
		Web Address:  	www.da.ks.gov/purch/ 

Closing Date:	February 5, 2010, 2:00 PM

Item:	Leased Space – Topeka

Agency(s):	Department of Administration – Kansas Surplus Properties
Department of Administration – Facilities Management Grounds Dept.

Move-in date:  To Be Negotiated	Sq. Ft. (both Divisions): 115,000 sq. ft.
		Surplus Properties:  60,000 sq. ft.
		Grounds:  55,000 sq. ft.

Pre-proposal Conference:  A pre-proposal conference will be held at 9:30 AM on Tuesday, January 5, 2010, at the following location:

Kansas Division of Printing
201 NW MacVicar Road
Topeka, KS 66606

If the weather is bad and you question whether or not the pre-bid will be held, you may contact Julie at 785-296-3631.

Vendors should bring a copy of the RFP document (including all embedded documents) as this will be used as the agenda.

Attendance is not required at the pre-proposal conference but is encouraged.  Impromptu questions may be permitted and spontaneous unofficial answers provided, however bidders should understand that the only official answer or position of the State of Kansas will be in writing.

Failure to notify the Procurement Officer of any conflicts or ambiguities in the Request for Proposal may result in items being resolved in the best interest of the State.  Any modification to this Request as a result of the pre-proposal conference, as well as written answers to written questions, shall be made in writing by addendum and mailed to all vendors who received the original request from the Division of Purchases.  Only written communications are binding.

Answers to questions will be available on the Division of Purchases’ website, www.da.ks.gov/purch/, bid solicitation link.

It shall be the responsibility of all participating vendors to acquire any and all addenda and additional information as it is made available from the web site cited above.  Vendors are required to check the website periodically for any additional information or instructions.
	
READ THIS REQUEST CAREFULLY
Failure to abide by all of the conditions of this Request may result in the rejection of a bid.
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SIGNATURE SHEET

Item:	Leased Space - Topeka 
	
Agency:	Department of Administration – Kansas Surplus Properties
	Department of Administration – Facilities Management Grounds Dept.

Location:	Topeka, KS

Closing Date:	February 5, 2010

By submission of a bid and the signatures affixed thereto, the bidder certifies all products and services proposed in the bid meet or exceed all requirements of this specification as set forth in the request and that all exceptions are clearly identified.  


Legal Name of Person, Firm or Corporation	

Mailing Address 	  City & State	Zip 	

Toll Free Telephone	Local	  Cell:  		Fax	

Tax Number		
CAUTION:  If your tax number is the same as your Social Security Number (SSN), you must leave this line blank.  DO NOT enter your SSN on this signature sheet.  If your SSN is required to process a contract award, including any tax clearance requirements, you will be contacted by an authorized representative of the Division of Purchases at a later date.    

E-Mail  		

Signature	Date	

Typed Name  	Title	


In the event the contact for the bidding process is different from above, indicate contact information below.

Bidding Process Contact Name	

Mailing Address 	  City & State	Zip 	

Toll Free Telephone	Local	  Cell:  		Fax	

E-Mail	


If awarded a contract and purchase orders are to be directed to an address other than above, indicate mailing address and telephone number below.

Award Contact Name	

Mailing Address 	  City & State	Zip 	

Toll Free Telephone	Local	  Cell:  		Fax	

E-Mail	



State of Kansas
Department of Administration
Division of Purchases

Supplier Diversity Survey Form

Why is the Division of Purchases requesting this information?

Current statutes governing the activities of the Kansas Division of Purchases do not include preferences or set-asides for Small Business Enterprises (SBEs).  The Division of Purchases is interested in determining to what extent purchase orders and contracts are awarded to SBEs under existing work efforts.  Please Note:  You must submit this form with each bid opportunity.

Persons or concerns wishing to receive a Purchase Order or Contract Award resulting from this bid opportunity must provide the information contained in this document before the award is made.  To help expedite this procurement, it is requested that you submit this form with your bid.

COMPANY DATA

Legal Company Name 	
Doing Business As (if applicable)	
Federal Tax ID Number  / FEIN 	
CAUTION:  If your tax number is the same as your Social Security Number (SSN), you must leave this line blank.  DO NOT enter your SSN on this sheet.  If your SSN is required for any reason, you will be contacted by an authorized representative of the Division of Purchases at a later date.    

Diversity Program Contact Name	Title	
Phone Number 	Fax Number 	
E-Mail Address 	Company Web 	
Address 		
City 	State 	Zip Code 	
Legal Structure:	□ Corporation	□ Partnership	□ Non-Profit	□ Sole Proprietorship	□ LLC

Signature 	Date:	

COMPANY DIVERSITY DATA  

 (A)	Business Classification   (See Appendix A for definitions):
Is your business a Small Business Enterprise (SBE) as defined by the SBA?
□ Yes	□ No	□ Don’t Know
Check all that Apply:	□ Disabled (DIS) 	□ SBA-Small Disadvantage Business (SDB)
□ Veteran-Owned (VBE)	□ Women-Owned (WBE)	□ Service-Disabled Veterans-Owned (DVBE)
□ African American	□ Native American	□ Minority-Owned Business Enterprise (MBE)
□ Hispanic American 	□ Asian Pacific American	□ Disadvantaged Business Enterprise (DBE)
□ Asian Subcontinent American 	□ Other: __________________________________________________________

 (B)	Has your Business Classification Status been certified by a state, municipal, federal or other certifying agency?
□ No	□ Yes	Certifying Entity:	



Other State of Kansas Resources for Small Business Enterprises (SBE)

Kansas Department of Commerce
Office of Minority/Women Business Development
http://www.kansas.gov/ksbdc/

State of Kansas
Department of Administration
Division of Purchases
Supplier Diversity Survey Form

Appendix A
Definition of Terms

[bookmark: _Toc104952916]Small Business Enterprise / Concern (SBE)
SBEs are businesses that do not exceed the size standard for the product or service it is providing as measured by its employment and/or business receipts in accordance with the U.S. SBA numerical size standards.  These standards are defined as FAR 52.219-8, 13 CFR Part 121 and 13 CFR 121.410.

Disadvantaged Business Enterprise (DBE) 
DBEs are defined as a business which are (a) owned by socially disadvantaged individuals who have been subjected to racial or ethnic
prejudice or cultural bias because of their identity as a member of a group without regard to their individual qualities; or (b) owned by economically disadvantaged individuals whose ability to compete in the free enterprise system has been impaired due to diminished opportunities to obtain capital and credit as compared to others in the same line of business who are not socially disadvantaged.

Disabled Business Enterprise (DIS)
DIS businesses are at least 51% owned and controlled by one or more U.S. citizens who has a physical or mental impairment which substantially limits one or more of such person’s major life activities.

Small Disadvantage Business Concern (SDB)
SDB businesses are certified by the SBA as meeting the following criteria: (1) they are small business concern and (2) must be at least 51% owned and controlled by one or more U.S. citizens who are socially and economically disadvantaged.  African Americans, Asian Pacific Americans, Asian Subcontinent Americans, Hispanic Americans and Native Americans are presumed to qualify as being socially disadvantaged.  Other individuals can qualify if they show by a preponderance of the evidence that they are socially disadvantaged.  In addition, the personal net worth of each eligible owner applicant must be less than $750,000, excluding the values of the applicant’s ownership interest in the business seeking certification and the owner’s primary residence.  Successful applicants must also meet applicable size standards for small businesses in their industry.  SDB regulations can be found in FAR 52.219-8 and 13 CFR parts 121 & 124.

Veterans-Owned Business Concern (VBE)
VBE businesses are at least 51% owned and controlled by one or more U.S. citizens who are Veterans of the U.S. Armed Forces.  In the case of any publicly owned business, at least 51% of the stock is owned by one or more veterans and one or more veterans must control the management and daily business operation.  The term “Veteran” means a person who served in the active military, naval or air service and who was discharged or released there from under conditions other than dishonorable.  VBE regulations can de found in FAR 52.219-9 & 38 USC 101 (2).

Service-Disabled Veterans-Owned Business Concern (DVBE)
DVBE businesses are at least 51% owned and controlled by one or more U.S. citizens who are service-disabled Veterans of the U.S. Armed Forces.  In the case of any publicly owned business, at least 51% of the stock is owned by one or more service-disabled veterans and one or more veterans must control the management and daily business operation.  The term “Veteran” means a person who served in the active military, naval or air service and who was discharged or released there from under conditions other than dishonorable.  The term “Service-Disabled” means a veteran of the U.S. Military Service has a service-connected disability with a disability rating of 0%-100%.  In the case of permanent or severe disability, the spouse of caregiver of such a service-disabled veteran may control the management and daily operations.  DVBE regulations can be found in FAR 52.219-9 & 38 USC 101 (2) & USC 101 (16).

Women-Owned Business Concern (WBE)
WBE businesses are at least 51% owned and controlled by one or more U.S. citizens who are female gender.  In the case of any publicly owned business, at least 51% of the stock is owned by one or more women and one or more women must control the management and daily business operations.  For Federal contracting regulations see FAR 52-219-8.

Minority-Owned Business Enterprise (MBE)
MBE businesses are at least 51% owned and controlled by one or more U.S. citizens belonging to certain ethnic minority groups.  In the case of any publicly owned business, at least 51 % of the stock is owned by one or more minorities, and one or more minorities must control the management and daily business operations.  “Ethnic Minority Groups” are people of Asian Pacific American, Asian Subcontinent American, African American, Hispanic American and Native American descent.  
· African Americans: People whose origins lay in any of the Black racial groups of Africa.
· Asian Pacific Americans: People whose origins lay in Brunei, Burma, China, Guam, Indonesia, Japan, Kampuchea (Cambodia), Korea, Laos, Malaysia, Northern Mariana Islands, Republic of the Marshall Islands, Federated States of Micronesia, Republic of Palau (U.S. Trust Territory of the Pacific Islands), the Philippines, Samoa, Singapore, Taiwan, Thailand and Vietnam.
· Asian Subcontinent Americans: People whose origins lay in Bangladesh, Bhutan, India, Pakistan, Sri Lanka or Nepal.
· Hispanic Americans: People whose origins are in the South and Central America, Mexico, Puerto Rico, Cuba or the Iberian Peninsula (including Portugal).
· Native Americans: American Indians, Inuit (Eskimos), Aleuts, and native Hawaiians of Polynesian ancestry.

TAX CLEARANCE
PLEASE NOTE:  THIS INFORMATION HAS CHANGED EFFECTIVE 10/27/09

Per KSA 75-3740-(c), the Director of Purchases may reject the bid of any bidder who is in arrears on taxes due the State of Kansas.  The Secretary of the Kansas Department of Revenue is authorized to exchange such information with the Director of Purchases as is necessary to determine a bidder’s tax clearance status, notwithstanding any other provision of law prohibiting disclosure of the contents of taxpayer records or information.

A “Tax Clearance” is a comprehensive tax account review to determine and ensure that the account is compliant with all primary Kansas Tax Laws administered by the Director of Taxation.  Information pertaining to a Tax Clearance is subject to change(s), which may arise as a result of a State Tax Audit, Federal Revenue Agent Report, or other lawful adjustment(s).

Bidders (and their subcontractors) are expected to submit a current Tax Clearance Certificate with every event response.  Bidders can obtain a Kansas Tax Clearance Certificate through the Kansas Department of Revenue’s secure website (http://www.ksrevenue.org/taxclearance.htm).  

Please Note:  For applications entered prior to 5:00 PM Monday through Friday, results typically will be available the following business day.  Individual and business applications are available.  Tax clearance requests may be denied if the request includes incomplete or incorrect information. 

Information about Tax Registration can be found at the following website:
http://www.ksrevenue.org/busregistration.htm

The Division of Purchases reserves the right to confirm tax status of all potential contractors and subcontractors prior to the release of a purchase order or contract award.  

In the event that a current tax certificate is unavailable, the Division of Purchases reserves the right to notify a bidder (one that has submitted a timely event response) that they have to provide a current Tax Clearance Certificate within ten (10) calendar days, or the Division may proceed with an award to the next lowest responsive bidder, whichever is determined by the Director of Purchases to be in the best interest of the State.

Contact Information:  Please provide the attached contact information for use should the State of Kansas need to contact the appropriate officials within your company to discuss your tax clearance / registration status.

CONTRACTOR
Contact Person for Tax Issues:	
Company Name:			
FEIN / Tax Number:			
CAUTION:  If your tax number is the same as your Social Security Number (SSN), you must leave this line blank.  DO NOT enter your SSN on this Tax Clearance Form.  If your SSN is required to process a contract award, including any tax clearance requirements, you will be contacted by an authorized representative of the Division of Purchases at a later date.

Mailing Address	
City & State	Zip Code	
Toll Free Telephone	Local	  Cell:  		Fax	
E-Mail	


SUBCONTRACTOR(S)
Contact Person for Tax Issues:	
Company Name:	Tax Number:	
Mailing Address	
City & State	Zip Code	
Toll Free Telephone	Local	  Cell:  		Fax	
E-Mail	
Additional pages may be added, as required, indicating the same information for multiple subcontractors.

CERTIFICATION REGARDING
IMMIGRATION REFORM & CONTROL


	All Contractors are expected to comply with the Immigration and Reform Control Act of 1986 (IRCA), as may be amended from time to time.  This Act, with certain limitations, requires the verification of the employment status of all individuals who were hired on or after November 6, 1986, by the Contractor as well as any subcontractor or sub-subcontractor.  The usual method of verification is through the Employment Verification (I-9) Form.  With the submission of this bid, the Contractor hereby certifies without exception that Contractor has complied with all federal and state laws relating to immigration and reform.  Any misrepresentation in this regard or any employment of persons not authorized to work in the United States constitutes a material breach and, at the State’s option, may subject the contract to termination and any applicable damages.  

	Contractor certifies that, should it be awarded a contract by the State, Contractor will comply with all applicable federal and state laws, standards, orders and regulations affecting a person’s participation and eligibility in any program or activity undertaken by the Contractor pursuant to this contract.  Contractor further certifies that it will remain in compliance throughout the term of the contract.  

	At the State’s request, Contractor is expected to produce to the State any documentation or other such evidence to verify Contractor’s compliance with any provision, duty, certification, or the like under the contract.  

	Contractor agrees to include this Certification in contracts between itself and any subcontractors in connection with the services performed under this contract.




____________________________________________			______________________
Signature, Title of Contractor						Date

SECTION I
INSTRUCTIONS

1.1	Proposal Reference Number:  The RFP number, indicated in the header of this page, as well as on the first page of this proposal, has been assigned to this Request and MUST be shown on all correspondence or other documents associated with this Request and MUST be referred to in all verbal communications.  All inquiries, written or verbal, shall be directed only to the procurement officer reflected on Page 1 of this proposal.  There shall be no communication with any other State employee regarding this Request except with designated state participants in attendance ONLY DURING:

Negotiations
Contract Signing
as otherwise specified in this Request.

Violations of this provision by vendor or state agency personnel may result in the rejection of the proposal.

1.2	Negotiated Procurement:  This is a negotiated procurement pursuant to K.S.A. 75‑37,102.  Final evaluation and award will be made by The Procurement Negotiation Committee (PNC) consisting of the following entities (or their designees):

Secretary of Department of Administration;
Director of Purchases, Department of Administration; and
Head of Leasing Agency

1.3	Appearance Before Committee:  Any, all or no vendors may be required to appear before the PNC to explain the vendor's understanding and approach to the project and/or respond to questions from the PNC concerning the proposal; or, the PNC may award without conducting negotiations, based on the initial proposal.  The PNC reserves the right to request information from vendors as needed.  If information is requested, the PNC is not required to request the information of all vendors.

Vendors selected to participate in negotiations may be given an opportunity to submit a revised proposal and/or their best and final offer to the PNC.  Prior to a specified cut‑off time for best and final offers, vendors may submit revisions to their technical and cost proposals.  Meetings before the PNC are not subject to the Open Meetings Act.  Vendors are prohibited from electronically recording these meetings.  All information received prior to the cut‑off time will be considered part of the vendor's best and final offer.

No additional revisions shall be made after the specified cut‑off time unless requested by the PNC.

1.4	Real Estate Lease Agreement:  The successful bidder will be required to enter into a formal contract that is acceptable to the tenant agency and the State of Kansas.  The base document required for this contract is the Department of Administration, Real Estate Lease Agreement, 
DA-46. This document can be found at the following website: 
http://da.ks.gov/fm/dfm/forms/DA-46_RealEstateLeaseAgreement.pdf 

Vendors will be allowed 30 days to review and sign the Lease Agreement once it is received.  Receipt of the Lease Agreement shall be presumed to have occurred within three (3) days of the date of the notice.  If parties are unable to agree on the terms of the Lease document, the State reserves the option to open negotiations with the next lowest bidder.

The bid document, bidder’s response to this RFP, bidder’s counter offer and best and final offer shall be included as a legal part of the real estate lease agreement.  In the absence of any language to the contrary, this RFP will be the determining document in questions of compliance with the specifications for this project.

1.5	Cost of Preparing Proposal:  The cost of developing and submitting the proposal is entirely the responsibility of the vendor.  This includes costs to determine the nature of the engagement, preparation of the proposal, submitting the proposal, negotiating for the contract and other costs associated with this Request.  

1.6	Preparation of Proposal:  Prices are to be entered in spaces provided in Exhibit A&B provided herein.  Computations and totals shall be indicated where required.  In case of error in computations or totals, the unit price shall govern.  The Committee has the right to rely on any price quotes provided by vendors.  The vendor shall be responsible for any mathematical error in price quotes.  The Committee reserves the right to reject proposals which contain errors.  

A proposal shall not be considered for award if the price in the proposal was not arrived at independently and without collusion, consultation, communication or agreement as to any matter related to price with any other vendor, competitor or public officer/employee.

Technical proposals shall contain a concise description of vendor's capabilities to satisfy the requirements of this Request for Proposal with emphasis on completeness and clarity of content.  Repetition of terms and conditions of the Request for Proposal without additional clarification shall not be considered responsive.

1.7	Signature of Proposals:  Each proposal shall give the complete mailing address of the vendor and be signed by an authorized representative by original signature with his or her name and legal title typed below the signature line.  If communication regarding the RFP process will be a different entity, indicate that individual’s contact information.  Each proposal shall include the vendor's tax number.

1.8	Acknowledgment of Addenda:  All vendors shall acknowledge receipt of any addenda to this Request by returning a signed hard copy with the bid.  Failure to acknowledge receipt of any addenda may render the proposal to be non-responsive.  Changes to this Request shall be issued only by the Division of Purchases in writing.

1.9	Modification of Proposals:  A vendor may modify a proposal by letter or by FAX transmission at any time prior to the closing date and time for receipt of proposals. 

1.10	Withdrawal of Proposals:   A proposal may be withdrawn on written request from the vendor to the Procurement Officer at the Division of Purchases prior to the closing date.

1.11	Competition:  The purpose of this Request is to seek competition.  The vendor shall advise the Division of Purchases if any specification, language or other requirement inadvertently restricts or limits bidding to a single source.  Notification shall be in writing and must be received by the Division of Purchases no later than five (5) business days prior to the bid closing date.  The Director of Purchases reserves the right to waive minor deviations in the specifications which do not hinder the intent of this Request.

1.12	Evaluation of Proposals:  Award shall be made in the best interest of the State as determined by the Procurement Negotiating Committee or their designees.  

The bidder should develop the building and space design through a process that considers the mission and involvement of the prospective Kansas tenant agency.  Existing buildings or new construction will be considered.  The location and surrounding neighborhood, the building form, the building’s site orientation with regards to energy conservation concerns, the efficiency of space in the layout plan, and the selection and assembly of materials should reflect performance, energy conservation, economy of design, and appearance.  A bidder is not limited in the materials chosen for the exterior construction of the building.  

All proposals submitted in response to the RFP will be evaluated by the Procurement Negotiating Committee, or their designees, using the following criteria and factors (listed in no particular order of importance):

1.12.1	Quality and Suitability of Space.   
The extent to which the proposed building and space meets the overall housing need of the tenant agency, as described in the specifications and general criteria set forth in this RFP.

1.12.2	General Space Efficiencies, including energy.  
A further consideration is total efficiency of the proposal in regards to space and resources.

1.12.3	Price of Proposal.  
The extent to which bidder’s total cost proposal is in keeping with prevailing market prices with respect to lease rates, the cost of building services, and the cost of constructing and furnishing the space, as specified herein.  In addition, proposals will be evaluated within the context of the limitations imposed by the tenant agency’s budget and capital resources.  

1.12.4	Cost of Associated Services.  
The cost of building services, including utility services and the cost of high-speed Internet connections, will be considered.  The proposed property will not be considered in the event a location cannot support the overall telecommunications requirements of the tenant agency.

1.12.5	Timing of Delivery of Space. 
The extent to which the bidder’s proposed schedule for the build-out and delivery of the finished space, ready for occupancy, conforms to the needs of the tenant agency.

1.12.6	Technical Response.  
The extent to which the bidder effectively demonstrates an understanding of the space needs of the tenant agency, as described in this RFP, and offers appropriate housing solutions to meet that need.  The quality of the technical response is measured by the extent to which the space specifications are adequately addressed within the bidder’s proposal, and the extent to which the bidder may suggest recommendations for improvements and anticipate potential problems that may arise in the performance of the work and delivery of the space.

1.12.7	Response Format and Completeness.   
Adequacy and completeness of the proposal is required and carries an important weighting in the evaluation of all proposals.  The proposal is to be complete, clear, and understandable.  Pages are to be numbered.

1.12.8	Financial Ability.  
The bidder’s demonstrated financial ability to implement, manage and maintain the proposed offering.

1.12.9	Experience and Qualifications.  
The bidder’s general experience and qualifications, and the PNC’s assessment of bidder’s ability to perform the work in a timely and professional manner.

1.13	Acceptance or Rejection:  The Committee reserves the right to accept or reject any or all proposals or part of a proposal; to waive any informalities or technicalities; clarify any ambiguities in proposals; modify any criteria in this Request; and unless otherwise specified, to accept any item in a proposal.

1.14	Special Provisions:  Special Provisions within the lease agreement allow for the addition of attachments, amendments, and special conditions that may be negotiated by the successful bidder and the Procurement Negotiating Committee.  Bidder MUST submit, with their initial response documents, any and all items they wish to be considered as “Special Provisions” with this lease in a separate section to be entitled “Special Provisions”.  The State reserves the right to add special provisions as finalized in the RFP process.

1.15	Proposal Disclosures:  At the time of closing, only the names of those who submitted proposals shall be made public information.  No price information will be released.  Interested vendors or their representatives may be present at the announcement at the following location:

State of Kansas Division of Purchases
900 Jackson Street, Room 102N
Topeka, KS  66612‑1286


Bid results will not be given to individuals over the telephone. Results may be obtained after contract finalization by obtaining a bid tabulation from the Division of Purchases by sending (do not include with bid):

· A check for $3.00, payable to the State of Kansas
· A self -addressed, stamped envelope
· Contract Proposal Number

Send to:

Kansas Division of Purchases
Attention: Bid Results/Copies
900 SW Jackson, Room 102N
Topeka, KS   66612‑1286

Copies of individual proposals may be obtained under the Kansas Open Records Act by sending an email to janet.miller@da.state.ks.us or calling 785-296-0002 to request an estimate of the cost to reproduce the documents and remitting that amount with a written request to the above address or a vendor may make an appointment by calling the above number to view the proposal file.  Upon receipt of the funds, the documents will be mailed.  Information in proposal files shall not be released until a contract has been executed or all proposals have been rejected.

1.16	Disclosure of Proposal Content and Proprietary Information:  All proposals become the property of the State of Kansas.  The Open Records Act (K.S.A. 45-205 et seq) of the State of Kansas requires public information be placed in the public domain at the conclusion of the selection process, and be available for examination by all interested parties.  (http://da.state.ks.us/purch/KSOpenRecAct.doc)  No proposals shall be disclosed until after a contract award has been issued.  The State reserves the right to destroy all proposals if the RFP is withdrawn, a contract award is withdrawn, or in accordance with Kansas law.  Late Technical and/or Cost proposals will be retained unopened in the file and not receive consideration or returned to the bidder.

Trade secrets or proprietary information legally recognized as such and protected by law may be requested to be withheld if clearly labeled “Proprietary” on each individual page and provided as separate from the main proposal.  Pricing information is not considered proprietary and the vendor’s entire proposal response package will not be considered proprietary.  

All information requested to be handled as “Proprietary” shall be submitted separately from the main proposal and clearly labeled, in a separate envelope or clipped apart from all other documentation. The vendor shall provide detailed written documentation justifying why this material should be considered “Proprietary”.   The Division of Purchases reserves the right to accept, amend or deny such requests for maintaining information as proprietary in accordance with Kansas law.

The State of Kansas does not guarantee protection of any information which is not submitted as required.

1.17	Exceptions:  By submission of a response, the vendor acknowledges and accepts all terms and conditions of the RFP and DA-46 Lease Agreement unless clearly avowed and wholly documented in a separate section to be entitled:  “Exceptions”.  

1.18	Notice of Award:  An award is made on execution of the written contract by all parties.  

1.19	News Releases:  Only the State is authorized to issue news releases relating to this Request, its evaluation, award and/or performance of the contract.


SECTION II
[bookmark: _Toc104952914]PROPOSAL RESPONSE

2.1	Submission of Proposals:  Vendor’s proposal shall consist of four (4) copies of the Proposal, including signature sheet, applicable literature and other supporting documents.

Vendor's proposal, sealed securely in an envelope or other container, shall be received no later than 2:00 p.m., Central Time, on the closing date indicated on Page 1, addressed as follows:

Kansas Division of Purchases
Proposal # (Indicated on Page 1)
Closing Date:  (Indicated on Page 1)
900 SW Jackson Street, Room 102N
Topeka, KS  66612‑1286

Faxed, e-mailed or telephoned proposals are not acceptable.

Proposals received prior to the closing date shall be kept secured and sealed until closing.  The State shall not be responsible for the premature opening of a proposal or for the rejection of a proposal that was not received prior to the closing date because it was not properly identified on the outside of the envelope or container.  Late Technical and/or Cost proposals will be retained unopened in the file and not receive consideration.  

It is the vendor’s responsibility to ensure bids are received by the closing date and time.  Delays in mail delivery or any other means of transmittal, including couriers or agents of the issuing entity shall not excuse late bid submissions.

PLEASE NOTE:  If you expect to deliver your bid in person, watch for a major construction project which  result in the closure of streets around the Landon State Office Building at various times throughout 2009.  This construction activity will affect ease of access to the building.  Please plan accordingly.

2.2 	Proposal Format: No paperwork or form is provided by the State for the narrative section of the proposal.  Instead, bidders are asked to prepare their proposals in a format that they believe best conveys the details of their property and offering.  It is generally recommended that bidders organize their proposals following the same sequence of property characteristics provided in the overall space requirements located in the Statement of Work, Section 4  (i.e., location, building, space, HVAC systems, etc), and address each line item that has a specified requirement indicated.

As a general guideline in preparing the narrative, bidders should also be careful to thoroughly identify themselves, both individually and/or corporately, as well as the property in question.  At minimum, all bidders shall provide the following identifying information in the narrative portion of their proposals:

· Bidder Identification - Name, address, phone number, and authorized signature of bidder.  
· Corporate identification - If applicable, bidder’s corporate or other business information, date established, structure (trust, partnership, corporation, non-profit, etc.), and federal tax identification number.  See agency specifications for additional information required.
· Building Identification - Building name, address, and other identifiers
· Property Ownership - Name of ownership entity; if partnership or corporation, include names of principals and those with controlling interest in the asset.
· Current zoning and platting - Please indicate if non-conforming use, or if it must be rezoned to accommodate proposed use.
· Use restrictions & easements - Please list all restrictions to land use, right-of-ways, or easements for this property.
· Historic register - List if structure has been nominated or date listed on the National Register of Historic Places, or the Register of Historic Kansas Places, and any conditions or restrictions imposed due to such designation.
· 
Environmental conditions - Adverse environmental conditions and status of abatement of all known or suspected hazardous or contaminated conditions in the facility or on site.
· Occupancy work site history - Indicate current and prior uses, including current tenancy within the building, as well as vacant square feet and location of vacant space, if any.
· Property management - Identify property manager of the proposed property, including credentials and experience.
· Elements of non-compliance - Identify space and other requirements described in this RFP that are not being met in bidder’s proposal.

2.3	Additional Proposals:  Bidders may submit more than one proposal; however, the proposals for each site shall be in accordance with the provisions of this RFP.  Bidders should submit complete specifications, descriptive materials and indicate any deviation from the specifications of this proposal.

A clear, well-organized and complete proposal will facilitate the review process by the Procurement Negotiating Committee.  Please follow the proposal format described, as failure to do so may result in disqualification.  

A completed bid submission package from respondents consists of the following elements:
-Preparation of a narrative section for the proposal, as described below.
-Completion of worksheet Exhibits A through C found at the end of this RFP.

Bidders shall, at a minimum, complete Exhibits A through C as part of their bid submission for additional proposals.

2.4	Qualifications:  A description of the vendor's qualifications and experience providing the requested or similar service shall be submitted with the bid.  The vendor must be an established firm recognized for its capacity to perform.  The vendor must have sufficient personnel to meet the deadlines specified in the Request.

2.5	Timeline:  A timeline for implementing services must be submitted with the bid via Exhibit C.

2.6	Subcontractors:  The Contractor shall be the sole source of contact for the contract.  The State will not subcontract any work under the contract to any other firm and will not deal with any subcontractors.  The Contractor is totally responsible for all actions and work performed by its subcontractors.  All terms, conditions and requirements of the contract shall apply without qualification to any services performed or goods provided by any subcontractor.

The State of Kansas requires tax information regarding all subcontractors be disclosed on the Signature Sheet, indicating company name, contact information and tax number.  Additional pages may be added, as required.  (See Tax Clearances, Page 3)

2.7	Proof of Insurance:  Upon request, the vendor shall present an affidavit of Worker's Compensation, Public Liability, and Property Damage Insurance to the Division of Purchases.

2.8	References:  Provide three (3) references who have purchased similar items or services from the vendor in the last five (5) years.  References shall show firm name, contact person, address, e-mail address and phone number.  Vendor employees and the buying agency shall not be shown as references.

2.9	Other bid completion instructions:  All bidders shall include the following with their bid submissions:

· Show the Bid Contract Number (noted on the cover of this RFP) on all bid documents and other correspondence with the State of Kansas. 
· Table of Contents with page numbers.
· Include photos of the property as well as plan drawings, including location map, site plans, building plans, space plans, and any other relevant plans.  


Beyond these general guidelines, bidders are invited to submit additional information in the narrative section that they may consider important in fully explaining their proposal and the advantages for its selection. 

SECTION III
TERMS AND CONDITIONS

3.1	Contract Documents:  This Request and any amendments and the response and any amendments of the Contractor shall be incorporated along with the DA‑146a into the written Lease Agreement (DA-46) which shall compose the complete understanding of the parties.

In the event of a conflict in terms of language among the documents, the following order of precedence shall govern:

· Real Estate Lease Agreement, DA-46;
· written modifications to the executed contract;
· this Request including any and all addenda; and
· Contractor's written proposal submitted in response to this Request as finalized.

3.2	Contract:  The successful vendor will be required to enter into a written contract with the State.  The vendor agrees to accept the provisions of form DA‑146a (Contractual Provisions Attachment) attached to this Request and Real Estate Lease Agreement, DA-46.

3.3	Contract Formation:   No contract shall be considered to have been entered into by the State until all statutorily required signatures and certifications have been rendered and a written Lease Agreement has been signed by the successful vendor.

3.4	Notices:  All notices, demands, requests, approvals, reports, instructions, consents or other communications (collectively "notices") which may be required or desired to be given by either party to the other shall be IN WRITING and addressed as follows:

Kansas Division of Purchases
900 SW Jackson St, Room 102N
Topeka, Kansas  66612-1286
RE:  Bid Number 10541

or to any other persons or addresses as may be designated by notice from one party to the other.

3.5	Termination for Cause:  The Director of Purchases may terminate this contract, or any part of this contract, for cause under any one of the following circumstances:

· the Contractor fails to make delivery of goods or services as specified in this contract; or

· the Contractor provides substandard quality and/or workmanship;

· the Contractor fails to perform any of the provisions of this contract, or so fails to make progress as to endanger performance of this contract in accordance with its terms.

The Director of Purchases shall provide Contractor with written notice of the conditions endangering performance.  If the Contractor fails to remedy the conditions within ten (10) days from the receipt of the notice (or such longer period as State may authorize in writing), the Director of Purchases shall issue the Contractor an order to stop work immediately.  Receipt of the notice shall be presumed to have occurred within three (3) days of the date of the notice.

3.6	Debarment of State Contractors:  Any vendor who defaults on delivery or does not perform in a satisfactory manner as defined in this Request may be barred for a period up to three (3) years, pursuant to KSA 75-37,103, or have their work evaluated for pre-qualification purposes.

3.7	Rights and Remedies:   If this contract is terminated, the State, in addition to any other rights provided for in this contract, may require the Contractor to transfer title and deliver to the State in the manner and to the extent directed, any completed materials.  The State shall be obligated only for those services and materials rendered and accepted prior to the date of termination.

In the event of termination, the Contractor shall receive payment prorated for that portion of the contract period services were provided to and/or goods were accepted by State subject to any offset by State for actual damages including loss of federal matching funds. 

The rights and remedies of the State provided for in this contract shall not be exclusive and are in addition to any other rights and remedies provided by law.  

3.8	Force Majeure:  The Contractor shall not be held liable if the failure to perform under this contract arises out of causes beyond the control of the Contractor.  Causes may include, but are not limited to, acts of nature, fires, tornadoes, quarantine, strikes other than by Contractor's employees, and freight embargoes, etc.

3.9	Waiver:  Waiver of any breach of any provision in this contract shall not be a waiver of any prior or subsequent breach.  Any waiver shall be in writing and any forbearance or indulgence in any other form or manner by State shall not constitute a waiver.

3.10	Independent Contractor:  Both parties, in the performance of this contract, shall be acting in their individual capacity and not as agents, employees, partners, joint ventures or associates of one another.  The employees or agents of one party shall not be construed to be the employees or agents of the other party for any purpose whatsoever.

The Contractor accepts full responsibility for payment of unemployment insurance, workers compensation and social security as well as all income tax deductions and any other taxes or payroll deductions required by law for its employees engaged in work authorized by this contract.

3.11	Staff Qualifications:  The Contractor shall warrant that all persons assigned by it to the performance of this contract shall be employees of the Contractor (or specified Subcontractor) and shall be fully qualified to perform the work required.  The Contractor shall include a similar provision in any contract with any Subcontractor selected to perform work under this contract.

Failure of the Contractor to provide qualified staffing at the level required by the proposal specifications may result in termination of this contract and/or damages.

3.12	Conflict of Interest:  The Contractor shall not knowingly employ, during the period of this contract or any extensions to it, any professional personnel who are also in the employ of the State and who are providing services involving this contract or services similar in nature to the scope of this contract to the State.  Furthermore, the Contractor shall not knowingly employ, during the period of this contract or any extensions to it, any state employee who has participated in the making of this contract until at least two years after his/her termination of employment with the State.

3.13	Confidentiality:  The Contractor may have access to private or confidential data maintained by State to the extent necessary to carry out its responsibilities under this contract.  Contractor must comply with all the requirements of the Kansas Open Records Act in providing services under this contract.  Contractor shall accept full responsibility for providing adequate supervision and training to its agents and employees to ensure compliance with the Act.  No private or confidential data collected, maintained or used in the course of performance of this contract shall be disseminated by either party except as authorized by statute, either during the period of the contract or thereafter.  Contractor must agree to return any or all data furnished by the State promptly at the request of State in whatever form it is maintained by Contractor.  On the termination of expiration of this contract, Contractor will not use any of such data or any material derived from the data for any purpose and, where so instructed by State, will destroy or render it unreadable.

3.14	Nondiscrimination and Workplace Safety:  The Contractor agrees to abide by all federal, state and local laws, rules and regulations prohibiting discrimination in employment and controlling workplace safety.  Any violations of applicable laws, rules and regulations may result in termination of this contract.

3.15	Environmental Protection:  The Contractor shall abide by all federal, state and local laws, rules and regulations regarding the protection of the environment.  The Contractor shall report any violations to the applicable governmental agency.  A violation of applicable laws, rule or regulations may result in termination of this contract.


3.16	Hold Harmless:  The Contractor shall indemnify the State against any and all loss or damage to the extent arising out of the Contractor’s negligence in the performance of services under this contract and for infringement of any copyright or patent occurring in connection with or in any way incidental to or arising out of the occupancy, use, service, operations or performance of work under this contract.

The State shall not be precluded from receiving the benefits of any insurance the Contractor may carry which provides for indemnification for any loss or damage to property in the Contractor's custody and control, where such loss or destruction is to state property.  The Contractor shall do nothing to prejudice the State's right to recover against third parties for any loss, destruction or damage to State property.

3.17	Care of State Property:  The Contractor shall be responsible for the proper care and custody of any state‑owned personal tangible property and real property furnished for Contractor's use in connection with the performance of this contract, and Contractor will reimburse State for such property's loss or damage caused by Contractor, normal wear and tear excepted.

3.18	Prohibition of Gratuities:  Neither the Contractor nor any person, firm or corporation employed by the Contractor in the performance of this contract shall offer or give any gift, money or anything of value or any promise for future reward or compensation to any State employee at any time.

3.19	Retention of Records:  Unless the State specifies in writing a different period of time, the Contractor agrees to preserve and make available all of its books, documents, papers, records and other evidence involving transactions related to this contract for a period of five (5) years from the date of the expiration or termination of this contract.

Matters involving litigation shall be kept for one (1) year following the termination of litigation, including all appeals, if the litigation exceeds five (5) years.

The Contractor agrees that authorized federal and state representatives, including but not limited to, personnel of the using agency; independent auditors acting on behalf of state and/or federal agencies shall have access to and the right to examine records during the contract period and during the five (5) year post‑contract period.  Delivery of and access to the records shall be at no cost to the state.

3.20	Antitrust:  If the Contractor elects not to proceed, the Contractor assigns to the State all rights to and interests in any cause of action it has or may acquire under the anti-trust laws of the United States and the State of Kansas relating to the particular products or services purchased or acquired by the State pursuant to this contract.

3.21	Modification:  This contract shall be modified only by the written agreement of the parties with the approval of the PNC.  No alteration or variation of the terms and conditions of the contract shall be valid unless made in writing and signed by the parties.  Every amendment shall specify the date on which its provisions shall be effective.

3.22	Assignment:  The Contractor shall not assign, convey, encumber, or otherwise transfer its rights or duties under this contract without the prior written consent of the State. 

This contract may terminate in the event of its assignment, conveyance, encumbrance or other transfer by the Contractor without the prior written consent of the State.

3.23	Third Party Beneficiaries:  This contract shall not be construed as providing an enforceable right to any third party.

3.24	Captions:  The captions or headings in this contract are for reference only and do not define, describe, extend, or limit the scope or intent of this contract.  

3.25	Severability:  If any provision of this contract is determined by a court of competent jurisdiction to be invalid or unenforceable to any extent, the remainder of this contract shall not be affected and each provision of this contract shall be enforced to the fullest extent permitted by law.

3.26	Governing Law:  This contract shall be governed by the laws of the State of Kansas and shall be deemed executed at Topeka, Shawnee County, Kansas, unless otherwise specified and agreed upon by the State of Kansas.

3.27	Jurisdiction:  The parties shall bring any and all legal proceedings arising hereunder in the State of Kansas, District Court of Shawnee County, unless otherwise specified and agreed upon by the State of Kansas.  The United States District Court for the State of Kansas sitting in Topeka, Shawnee County, Kansas, shall be the venue for any federal action or proceeding arising hereunder in which the State is a party.

3.28	Mandatory Provisions:  The provisions found in Contractual Provisions Attachment (DA‑146a) which is attached are incorporated by reference and made a part of this contract.

3.29	Integration:  This contract, in its final composite form, shall represent the entire agreement between the parties and shall supersede all prior negotiations, representations or agreements, either written or oral, between the parties relating to the subject matter hereof.  This contract between the parties shall be independent of and have no effect on any other contracts of either party.

3.30	Criminal or Civil Offense:   Any conviction for a criminal or civil offense of an individual or entity that controls a company or organization or will perform work under this contract that indicates a lack of business integrity or business honesty must be disclosed. This includes (1) conviction of a criminal offense as an incident to obtaining or attempting to obtain a public or private contract or subcontract or in the performance of such contract or subcontract; (2) conviction under state or federal statutes of embezzlement, theft, forgery, bribery, falsification or destruction of records, receiving stolen property; (3) conviction under state or federal antitrust statutes; and (4) any other offense to be so serious and compelling as to affect responsibility as a state contractor.  For the purpose of this section, an individual or entity shall be presumed to have control of a company or organization if the individual or entity directly or indirectly, or acting in concert with one or more individuals or entities, owns or controls 25 percent or more of its equity, or otherwise controls its management or policies.  Failure to disclose an offense may result in disqualification of the bid or termination of the contract.

3.31	Injunctions:  Should Kansas be prevented or enjoined from proceeding with the acquisition before or after contract execution by reason of any litigation or other reason beyond the control of the State, vendor shall not be entitled to make or assert claim for damage by reason of said delay.

3.32	Statutes:  Each and every provision of law and clause required by law to be inserted in the contract shall be deemed to be inserted herein and the contract shall be read and enforced as though it were included herein.  If through mistake or otherwise any such provision is not inserted, or is not correctly inserted, then on the application of either party the contract shall be amended to make such insertion or correction.

3.33	Materials and Workmanship:  The Contractor shall perform all work and furnish all supplies and materials, machinery, equipment, facilities, and means, necessary to complete all the work required by this solicitation, within the time specified, in accordance with the provisions as specified.

The contractor shall be responsible for all work put in under these specifications and shall make good, repair and/or replace, at the contractor's own expense, as may be necessary, any defective work, material, etc., if in the opinion of agency and/or Division of Purchases said issue is due to imperfection in material, design, workmanship or contractor fault.

3.34	Industry Standards:  If not otherwise provided, materials or work called for in this contract shall be furnished and performed in accordance with best established practice and standards recognized by the contracted industry and comply with all codes and regulations which shall apply.
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3.35	Federal, State and Local Taxes:  Unless otherwise specified, the proposal price shall include all applicable federal, state and local taxes.  The successful vendor shall pay all taxes lawfully imposed on it with respect to any product or service delivered in accordance with this Request.  The State of Kansas is exempt from state sales or use taxes and federal excise taxes for direct purchases.  These taxes shall not be included in the vendor's price quotation.

The State makes no representation as to the exemption from liability of any tax imposed by any governmental entity on the Contractor.

3.36	Accounts Receivable Set-Off Program:  During the course of this contract if the vendor is found to owe a debt to the State of Kansas, agency payments to the vendor may be intercepted / setoff by the State of Kansas.  Notice of the setoff action will be provided to the vendor.  The vendor shall credit the account of the agency making the payment in an amount equal to the funds intercepted.

K.S.A. 75-6201 et seq. allows the Director of Accounts & Reports to setoff funds the State of Kansas owes vendors against debts owed by the vendors to the State of Kansas.  Payments setoff in this manner constitute lawful payment for services or goods received. The vendor benefits fully from the payment because its obligation to the State is reduced by the amount subject to setoff.

3.37	Definite Quantity Contract:  This Request is for a close-ended contract between the vendor and the State to furnish a predetermined quantity of a good or service in a given period of time.

3.38	On-Site Inspection:  Failure to adequately inspect the premises shall not relieve the successful vendor from furnishing without additional cost to the State any materials, equipment, supplies or labor that may be required to carry out the intent of this Request.  Submission of a bid shall be construed as evidence that the vendor has made necessary examination, inspection and investigation. Failure to properly inspect the site may result in rejection of the vendor's bid. 

3.39	Experience:  All bidders are preferred to have a minimum of three (3) years continuous active participation in the applicable industry, providing equipment/services comparable in size and complexity to those specified herein.

Bidders may be required to furnish information supporting the capability to comply with conditions for bidding and fulfill the contract if receiving an award of contract.  Such information may include, but not be limited to, a list of similar size and type projects the Bidder has completed.

3.40	Prices:  Prices shall remain firm for the entire contract period and subsequent renewals. Prices quoted shall be 	net delivered, including all trade, quantity and cash discounts.  Any price reductions available during the contract period shall be offered to the State of Kansas.  Failure to provide available price reductions may result in termination of the contract.

[bookmark: _Toc104952907]3.41	Payment:  Payment Terms are Net 30 days.  Payment date and receipt of order date shall be based upon K.S.A. 75-6403(b).  This Statute requires state agencies to pay the full amount due for goods or services on or before the 30th calendar day after the date the agency receives such goods or services or the bill for the goods and services, whichever is later, unless other provisions for payment are agreed to in writing by the vendor and the state agency.  

NOTE:  If the 30th calendar day noted above falls on a Saturday, Sunday, or legal holiday, the following workday will become the required payment date.

Payments shall not be made for costs or items not listed in the vendor's response.

Payment schedule shall be on a frequency mutually agreed upon by both the agency and the Contractor.

3.42	Implied Requirements:  All products and services not specifically mentioned in this solicitation, but which are necessary to provide the functional capabilities described by the specifications, shall be included. Other products required to make the described software functional shall be identified in the vendor's response.

3.42	Acceptance:  No contract provision or use of items by the State shall constitute acceptance or relieve the vendor of liability in respect to any expressed or implied warranties.

3.43	Submission of the Bid:  Submission of the bid will be considered presumptive evidence that the vendor is conversant with local facilities and difficulties, the requirements of the documents and of pertinent State and/or local codes, state of labor and material markets, and has made due allowances in the proposal for all contingencies.  Later claims for labor, work, materials, equipment, and tax liability required for any difficulties encountered which could have foreseen will not be recognized and all such difficulties shall be properly taken care of by Contractor at no additional cost to the State of Kansas.

3.45	Certification of Materials Submitted:  The response to this request, together with the specifications set forth 	herein and all data submitted by the vendor to support the response including brochures, manuals, and descriptions covering the operating characteristics of the item(s) proposed, shall become a part of any contract between the successful vendor and the State of Kansas. Any written representation covering such matters as reliability of the item(s), the experience of other users, or warranties of performance shall be incorporated by reference into the contract.

3.46	Award:  Awards will be made by the PNC based upon the best interest of the State.  The successful bidder will be notified in writing by the Procurement Negotiating Committee. Neither the bidder nor the State of Kansas is obligated in any way until the Real Estate Lease Agreement has been approved and signed by all parties.  

3.47	Property Maintenance & Capital Repairs:  The successful bidder will maintain the building and the space, including maintenance and replacement of select finish materials (e.g., paint, carpets, lighting, etc.,) as part of the base rent for the term of the lease.  The Lessor is also responsible for landscaping.

3.48	Bidder Qualifications & Evidence of Financial Capacity:  The successful bidder will demonstrate to the Procurement Negotiating Committee that they possess the qualifications and experience needed to perform the work, including the experience and qualifications of their contractors and subcontractors.  In addition, the successful bidder will demonstrate financial capacity to fund and/or finance the construction build-out and tenant fit-up of the space.  

3.49	Performance Guarantees & Liability Protections:  The lease agreement will contain a liquidated damages provision in favor of State of Kansas in the event that the successful bidder fails to deliver space to agreed standards, and/or fails to meet the established date for agency occupancy of space.  

In addition, the successful bidder will agree to hold the State of Kansas harmless for any liability claims related to the work, or workplace accidents during the construction phases of the project. Such language will be added to the real estate lease agreement as a special provision. 

3.50	Timeline:

So that the State may objectively evaluate proposed construction and occupancy schedules, bidders must complete and include the Project Schedule Worksheet (Exhibit C), providing specifics on estimated schedule and completion of milestone tasks.  The Project Schedule Worksheet, and any signed amendments thereto, will be incorporated into the lease agreement.  Time is of the essence in completing the project.


Schedule of Events:	(Note:  The State of Kansas reserves the right to change these dates as required; all registered bidders will receive written notice of any changes to this schedule).

	
	Phase 1:  Proposal request and submittal


	By December 17, 2009
	Request For Proposals (RFP) mailed to prospective parties

	December 24, 2009
	Notice appears in the Kansas Register

	1/5/10

	Pre-proposal Conference - A pre-proposal conference will be held at 9:30 AM, on January 5, 2010, at the following location:

Kansas Division of Printing
201 NW MacVicar Road
Topeka, Ks 66606


	By 1/8/10
	Written response to issues raised at the pre-proposal conference will be posted on Division of Purchases’ website.

	2/5/10
	Deadline for Bid submissions.

	
	Phase 2:  Proposal review and bidder selection


	2/8/10
	Begin review of proposals by the Procurement Negotiating Committee.

	
	Begin site reviews and building inspections by Procurement Negotiating Committee of all proposed sites and facilities.

	
	Procurement Negotiating Committee will meet with selected bidders to interview and discuss bids.  Additional information or meetings may be requested to determine the best proposal.  

	To Be Determined
	Initial lease negotiations will occur during bidder interviews in an effort to establish a clear understanding of the prospective price and terms of the respective bids, thereby helping the decision processes of the Procurement Negotiating Committee.  

	To Be Determined
	Bidder selected and a formal real estate lease agreement is approved and executed between parties.  (Note: No party to transaction is legally obligated in any way until the Agreement has been approved by the State of Kansas and signed by all parties).



	            Phase 3:  Space build-out, occupancy & project completion


	To Be Determined
	The successful bidder works with the tenant agency(ies) to finalize floor plans and other build-out specifications provided in the lease agreement and/or other contracts between the parties. Meetings with the bidder’s design professional(s) are typically required.  

	To Be Determined
	Pre-occupancy inspection(s) made.   

	To Be Determined
	Property and space ready for occupancy.  

	To Be Determined
	State tenant takes occupancy of the space.  The designated occupancy date will be mutually agreed to by Lessee and Lessor at time of execution of the lease agreement.



3.52	Architectural Drawings and Construction Documents:  The successful bidder, following execution of the lease agreement and before completion of the build-out of the space, shall be required to submit the architectural design development and construction documents to the State of Kansas.  These documents shall conform to the guidelines promulgated by all applicable local and state code publications, as listed in this RFP.

3.53	Occupancy Provisions:  A predetermined occupancy date must be established prior to execution of the real estate lease agreement, which shall include a specific schedule of milestone events, 	known as the Project Completion and Occupancy Schedule.  In the event that the successful bidder fails to adhere to the agreed performance schedule, the State of Kansas shall have the right, to be exercised in its sole discretion, to take one of the following two courses of action:


(a)	Terminate Lease agreement:   If the successful bidder (Lessor) falls behind the project schedule by more than sixty (60) days, the State of Kansas (Lessee) has the option of canceling and terminating this lease.  No rents, damages or other monetary costs will be owed.  No legal liability will exist as a result of this cancellation.  Each party will release and discharge each other and will waive all rights to pursue claims against each other in the event of lease cancellation.

(b)	Seek Claim for Liquidated and Stipulated Damages:  The Lessor agrees to begin work upon this project upon lease approval.  The Lessor will fully perform, complete and finish all work on the property, ensure the facility is ready for occupancy and will obtain an occupancy permit issued by local authorities (if applicable) by the lease commencement date of xxxxxx.  In the event that the property is not complete and available by this date, liquidated and stipulated damages in the amount of $ xxxx.xx per calendar day will be assessed.  This assessment will be calculated for every day that this project is uncompleted and unfinished from the lease commencement date, unless the Lessor is delayed in the prosecution and completion of this work by fire or tornado.  The liquidated and stipulated damages assessed will be deducted from monthly rental payments from the start of the actual occupancy date.  If Lessee changes the project specifications or submits a project change order, both parties will mutually agree upon a revised commencement date in writing.

3.54	Defects in Workmanship & Lessee Rights to Remedy Defects:  Occupancy and lease commencement will not 	occur until substantial completion and compliance with building codes, ordinances, standards and regulations takes place; and the local governmental organization(s) having authority has issued a building occupancy permit 	or has inspected the property and given approval for occupancy.  

For remedies of initial defects, see paragraph 7, Repair of Premises, in the DA-46 Lease Agreement.

3.55	Project Review Process and Change Orders:  Within 60 calendar days from lease execution (or four months prior to lease start date, whichever is less), the Lessor shall submit to Project Manager and/or the tenant agency(ies), the architectural and engineering drawings which shall include, but may not be limited to, the following plans and specifications:
· Site Plan
· Plans/Elevations
· Building Section Plans
· Plumbing Plan
· HVAC Plan
· Electrical Plan

The review and approval of these plans by the Project Manager and/or the tenant agency(ies) is required before construction shall commence.  These plans must be sealed by an architect and/or engineer registered with the State of Kansas.  Plans and specifications are to be approved by the Project Manager and the tenant agency within three weeks from their receipt.

The design process sometimes requires that revisions be made to the initially proposed plans and specifications as a result of on-site conditions or changes requested by tenant agency.  The plans and specifications changes shall require the written consent of both parties. This change order process shall utilize a Facility Change Request form provided by the State.  Changes requested by the State will be billed at a pre-approved rate of time and material.  

3.56	Site and space access rights prior to occupancy of space:  The Lessor agrees to allow Lessee, and any of Lessee’s vendors or contractors, access to the demised space prior to the established occupancy date.  Such access, however, does not constitute lease occupancy for purposes of establishing rental payments.  Such site visits and vendor access shall be scheduled in advance whenever possible or practical.

In addition, representatives of the State shall have the right to inspect the premises to determine whether the space is in full compliance with the terms of the lease agreement and build-out specifications.


3.57	Maintenance:  The Lessor will be responsible for maintenance, repairs, and improvements as a result of typical wear and tear of the leased premises, including preventive and corrective maintenance.  The Lessor will maintain or replace the finish materials as part of the base rent for the term of this lease, according to the reasonable life expectancy of such materials and finishes.  Notwithstanding the provisions of this clause, the Lessor shall have no obligation to make repairs or replacements to the extent such repairs or replacements are caused by the negligence of Lessee.  The Lessor is responsible for trash removal. 

3.58	Annual Disclosure of Property Operating Expenses:  The Lessor agrees to provide the tenant agency with a detailed list of operational expenses attributable to the demised space within sixty (60) days following the end of each lease year, calendar year, or other mutually agreed time period for annual reporting.  Such expense detail may include, but is not limited to:  roof repair/inspection, heating/cooling, maintenance, repair, snow removal, landscaping, insurance, taxes and other applicable operating expenses.

SECTION IV
GENERAL SPECIFICATIONS

This Request for Proposal includes two (2) levels of leased space need for different Department of Administration divisions. 

1.	The Division of Surplus Property, and 
2.	The Division of Facilities Management Grounds Department  

Bidders may propose leased space for either, or, or both Divisions.    Pricing shall be submitted separately, if bidding for both divisions.  Cost Worksheet, Exhibit A&B, shall be submitted for each for comparison and evaluation purposes.

This Section IV reflects the general specifications that apply to both divisions and shall be taken into consideration for any bid that is prepared.   

4.1	Deliverable:

The State of Kansas is seeking leased warehouse/storage and office space to house the operations of the Department of Administration’s Division of Surplus Property. The goods and services being sought from prospective bidders include provisions for the following elements, in accordance to the criteria and specifications prescribed in this RFP.

· The leased space itself, also known as the “raw” space, before being customized to meet the particular needs of the tenant agency, together with the building, site and parking areas that support the space.
· Construction of the leased space, also known as the “build-out” of the space, including mechanical, electrical, and plumbing systems, in accordance with the standards and specifications described herein;
· Provision of the furniture, fixtures and equipment (FF&E), including security and paging systems, as may be applicable; 
· Provision of select telephone and computer data systems (“tel-data”), including the computer network cabling system, also known as the Telecommunication PremiseDistribution System;
· On-going maintenance and management of the property after the State tenant agency takes occupancy of the space.

The successful bidder shall be responsible for managing the build-out of the space, including the procurement and installation of all construction materials; the purchase and installation of the prescribed FF&E, if applicable; and the hiring, coordination and oversight of all contractors and subcontractors used to complete the work.  

It is appropriate here to again emphasize the collaborative nature of the interface and meetings that are anticipated and expected between the successful bidder, the bidder’s design professionals and contractors, and the agency tenant in finalizing the design plans and specifications for the space, the building, and the site.  

Prospective bidders should develop preliminary space designs consistent with the requirements described in this RFP, however, major details are not required in these preliminary plans.  Initial plans need to reflect only a level of detail to show all agencies included and the initial footprint proposed.  The selected bidder will finalize the space design and plan specifications through close collaboration with the tenant agencies. 

Any revisions to the construction budget and schedule for performance will be reflected through signed amendments, change orders, and other special provisions in the real estate lease agreement.  Initial plans are not required to be stamped by an architect.  Final plans shall be stamped approved by an architect.


4.2	Terms of Reference:

This RFP may refer to State governmental agencies under alternative names, including “offeree”, “tenant agency”, “State”, “State tenant”, “occupant”, and “Lessee”.  In all instances, these are understood to be synonymous and interchangeable names.  Similarly, prospective respondents may be referred to by different names, including: “bidder”, “proposer”, “developer”, “owner”, “landlord”, and “Lessor”, which are also understood to be synonymous references.

4.5	Lease Type:  

Preference is for a Full Service lease, to include utilities, janitorial services and security.

The State will not agree to assume responsibility for payment of any of the following categories of operating expense or service item:

· Real estate taxes
· Property insurance
· Maintenance and capital repairs
· Parking (both on-site or off-site)

4.6	Purchase Option:  The State of Kansas will consider offers of an option to purchase the leased property.   This would apply only to buildings in which the State is the sole tenant.  The specifics of the purchase option agreement, including the optioned purchase price, will be negotiated between parties prior to the execution of the lease agreement and incorporated therein.

4.7	Energy

Vendors are invited to include in their proposal any “green” environmental efficiencies they may view appropriate, any Energy Management System, etc. The building must meet Kansas Department of Administration energy standards.

In addition, a remodeled, renovated, or new facility is expected to be in compliance with the enclosed criteria.

Energy Audit:  In order to address increasing energy cost the State of Kansas will require the completion of an energy audit when submitting a lease proposal. The State of Kansas has determined the EPA administrated Energy Star auditing program is an acceptable tool in determining the energy usage of the proposed property. The program is free to use after registering at the EPA website. The program will require the entering of the most recent 12 months of utility data, number of employees located in the building, and number of computers. Please submit the audit finding with your proposal.

The EPA Energy Star website can be found at
http://www.energystar.gov/index.cfm?c=evaluate_performance.bus_portfoliomanager

· Other Location and Site Requirements

· The specifications for the office contained in this document should be followed for remodeled, renovated, or new space proposed.  Deviations from these criteria must be so noted in the proposal.

· The agency prefers the size of the various spaces listed; however, minor adjustments are understandable in order to enhance the design, functional relationships, and the available space.  The agency will approve design alterations as the final space plan evolves.  Multiple buildings, same site to meet the total space requirements of the RFP are acceptable.  Multiple buildings, separate sites to meet the total space requirements of the RFP are acceptable.

· Departmental areas list workstations, offices, and supporting area by department.  Common area is space used in general among the departments of the agency.  Common areas are designated as public access or staff areas.  Estimated total useable area is the total of both Departmental and Common area square footage times an interior circulation

multiplier.  It is desirable that rentable area should match or nearly match the calculated useable area.  The proposer needs to realize that sizes listed in the enclosed division tables do not include the additional allowances for the interior circulation multiplier.

· Other factors not specified in these space requirements will affect the building area and need to be considered.  If the facility is a multi-story property, additional space will be needed for duplicate functions on each floor.  Areas for mechanical and equipment rooms have not been included, as they will vary based on the design proposed.  The restroom space has not been determined for this summary, but needs to be considered.  When creating a floor plan, the proposer needs to account for interior wall thicknesses and systems furniture panel thicknesses.  If an efficient design is proposed, these factors often can be accounted for from the area added by the circulation multiplier.

4.9	Building Requirements:

· Building Type – Efficient space utilization, facility design, energy usage, and operation are desired.   If a multi-story building is proposed, the following features must be considered:

· Janitor closets must be located on each floor.
· Water fountains must be installed on each floor.
· Elevator and stairways must be installed in the building.

· Flagpole:  An appropriate height, lighted flagpole shall be provided at a prominent location around the front of the facility, with appropriately sized American flag and State of Kansas flag provided by the Contractor.  Contractor shall be responsible for maintenance of the flags, light and flagpole to ensure proper display and professional appearance.

· Loading Docks/Warehouse and Storage Areas – A standard dock is required.  If a multi-story facility is proposed, each level is preferred to have a standard dock.  

· Entryway – An energy efficient double door public entry vestibule is preferred.  

· Storm Shelter - Access to a storm shelter must be provided.  Providing access to a basement storm shelter may satisfy this requirement.  If a one-floor or multi-story facility above ground is proposed, an appropriate storm shelter area must be provided that is designed for all employees.  Access to adjacent buildings with storm shelter facilities may also satisfy this requirement, if that building agrees to allow use by agency staff, when required.  Bidders are instructed to provide details regarding their proposed storm shelter with the bid response.

· Furniture, Fixtures & Equipment (FF&E) – Summary of Requirements:

· Office Systems Furniture – Not required
· Fixtures & Equipment - Not required
· Other FF&E Requirements – Not required

· Hazardous Materials – Bidders must identify known or suspected areas of asbestos, mold / mildew or presence of other hazardous materials, in the building or on the site, both past and present.  If the property has been abated for hazardous materials, then bidder must present suitable evidence of such.

(Note:  The Selection Committee reserves the right to require the bidder to provide appropriate environmental audits, hazardous material studies, and abatement certifications, as appropriate.  The Selection Committee will determine the need for such verifications prior to selection of the successful bidder).

4.11	General Construction Standards and Design Requirements:

Building codes - The successful bidder is responsible for meeting all applicable local and State building codes, ordinances, standards and regulations as per Section 4.21.  In the event that this RFP has requirements that do not comply with building codes, then the building code requirement will prevail.

American with Disabilities Act of 1990 (ADA) - The remodeling, renovation, or new construction proposed shall comply with the Americans with Disabilities Act Accessibility Guidelines (ADAAG).  The following items are minimal requirements:
· An accessible route from accessible parking through an accessible entrance to primary function areas;
· Accessible toilets; and
· Accessible signage

Space measurement standards - Calculation of rentable and usable area should be based on ANSI/BOMA standards (Z65.1 – 1996, Standard Method for Measuring Floor Area in Office Buildings).

CAD drawings – Initial submissions do not require Cad drawings, specifically; the original submission requires only a level of detail to show all agencies included and the initial footprint proposed.

It is desired that plans be submitted on computer disk, using the most current AutoCAD Version 14 or above, DXF format.  Final plans must be sealed by an architect or engineer registered with the State of Kansas.  A final set of as-built drawings shall be provided to the Project Manager and the tenant agency occupying the space.

4.12	Construction and Finish Specifications:

· General – The proposer shall be responsible for maintenance and improvements required as a result of typical wear and tear.  The proposer shall maintain or replace the selected finish materials as part of the base rent for the term of the lease, according to the reasonable life expectancy of such materials and finishes, except for damages or unusual circumstances caused by normal use.  All finishes and materials in the proposed space should receive appropriate maintenance or replacement provided by the proposer.  

· Paint – All walls, steel door frames, and steel doors should be painted.  Two (2) coats of semi-gloss finish over primer as required.  Paint material shall be acrylic latex or type appropriate to the material.  More durable finishes shall be used in restrooms, break rooms, and public entry.  Any wood doors shall be stained and clear finished.  

· Flooring    - 	Warehouse and shop areas shall have flooring concrete flooring. 

· Grounds facility shall have vinyl composition tile

· Surplus office and common area shall be carpet. 

Only carpet designed for heavy wear (density of not less than 28-ounce weight) for the term of the lease will be accepted.  If proposer intends to install new carpet, the agency prefers to choose the carpet to ensure durability and compatible colors.  Carpet adhesive shall be solvent free, and carpet shall be approved by the Carpet and Rug Institutes Indoor Air Quality Testing Program.  Appearance loss and maintenance needs shall be considered in carpet selection.  Entrances, lobby, break rooms and break room kitchen should have resilient tile or ceramic tile flooring.  Resilient flooring to be 12-inch by 12-inch vinyl composition tile or equivalent.   

· Restrooms and Accessories – An appropriate number of restrooms (separate male and female) shall be provided, based on the number of employees supported.  Restrooms shall have the following accessories as selected by tenant agency:  mirrors, soap dispensers, trash containers, tissue dispensers, and paper towel dispensers or hand dryers. Sanitary napkin disposal units shall be provided in the women’s restrooms. Toilet partitions shall be provided for restrooms with more than one water closet and/or urinal.  Each restroom is to be equipped with an exhaust fan and wall switch to operate this fan.  All restrooms shall comply with ADA design requirements.  Restrooms shall have vinyl composition tile or ceramic tile flooring.  All walls to be trimmed with 4-inch vinyl or rubber cove base molding. 
· 
Doors – All doors shall have a minimum width of 36” as selected by tenant agency.  Doors must be equipped with handicap-accessible hardware and have a doorstop.  All security access doors are required to have a door closer.  

· Tel-Data/Computer Room Floor – Floor covering shall be vinyl composition tile as described above. 

· Sound insulation – Control of noise in the HVAC system and adequate insulation of ductwork is required.

4.13	Plumbing Systems:

· Hot & cold-water distribution – Hot and cold water will be provided at all restroom sinks, custodial closets, break room(s), and training room kitchenette.  

· Floor drains - Provide floor drains in each restroom and in shop area, even if not required by building code.  Warehouse area shall have a floor drain.

· Custodial closet - Provide one floor mounted mop sink with back splash for filling of buckets and disposal of wastewater for each custodial closet.

· Water fountains/coolers – Water fountains are to be provided. These shall comply with ADA design requirements, and be fully accessible to disabled individuals. 

· Sink system – Stainless-steel sink shall be installed in break room area.  

· Water conservation - Bidders are encouraged to develop designs, which conserve natural resources; with respect to water consumption, the control features may include:

· Sensor-operated electronic faucets and toilet flush valves in restrooms.  
· Water flow limited to a maximum of 0.5 gallons of water per minute for restroom lavatories.

· Fire hydrants - Provide outside water hydrants as dictated by the local fire department.

4.14	Mechanical & HVAC Systems:

· HVAC conditioning specifications – general office spaces & common areas - General office and common areas shall be heated in the winter to maintain the space environment at 68-74 degrees F. with a relative humidity of 20-30% and cooled in the summer at 74-78 degrees F. with a relative humidity of 40-60%.  As a guide, an adequately size air distribution system shall provide 4-10 air changes per hour.

· Air conditioning specifications – computer & electronics room(s) - Telecommunication, Computer, UPS and server room(s) require air conditioning systems designed to ensure proper environmental requirements are met.  These shall be sized to cool the tenant agency’s computer systems per manufacturer’s recommendation.   

· Other HVAC design criteria - HVAC design considerations shall include reasonable consideration of sound transmission.  Noise criterion level shall be NC30-45 as defined by ASHRAE Handbook of Fundamentals 2001.  Return air sound transmission should be considered to ensure privacy.  

· Exhaust systems - All toilets, custodial closets, and break rooms shall have mechanical exhaust systems in accordance with International Mechanical Code and/or existing state and local code requirements.


4.15	Electrical Systems:

· General - The overall electrical design must take into account office density and computer usage, telecommunication needs, special-use rooms, and other types of power demands.  The general electrical system specifications are as follows, with greater design detail to be developed once the leased space has been selected

· Power requirement - Provide code-compliant service with adequate amperage to satisfy building and space needs.  Ground-to-neutral voltage not to exceed 1-volt p/p and 3-volts RMS within a range of 58Hz to 60Hz.  House circuits must be within 5% power range of 120 volts AC.  The building’s power factor shall be maintained at or above .85.

· Distribution panels - The dedicated circuits for computers, copiers and specified office equipment are to have a separate ground and dedicated neutral.   All electric panels will be properly labeled according to destination.

4.16	Lighting Systems

· General design standards - The total interior/exterior lighting system shall meet the requirements of the ASHRAE 90.1, latest edition (i.e. the interior lighting power density shall not exceed 1.3 watts per square foot of building area, where the lighting load includes ballast power.

· Brightness of work / desktop areas (foot candles) – An average brightness of 50-60 foot candles is required.    

· Brightness of general and circulation areas –   A brightness of at least 10 foot candles is required.

· Lighting controls - Lighting controls shall meet the requirements of ASHRAE 90.1, section 9.2.1 or latest addition of code. All building exterior and site lighting will be automatically controlled by photo sensors, time clocks, or a combination of both where required for energy conservation or security conditions per ASHRAE 90.1 section 9.2.1 or latest addition of code.

· Exterior lighting - Exterior building illumination, lighting for safety and security, parking lots and driveways shall be illuminated as jointly determined.  Exterior lighting must be designed to avoid glare for drivers and neighbors.

· Other lighting requirements - Bidders are encouraged to develop designs which conserve natural resources by employing energy saving devices, such as lighting occupancy sensors.  

4.17	Telephone & Data Systems (Tel-Data):

· Tel-data distribution system - The successful bidder shall provide the design and installation of the tel-data wiring distribution system.  The number of cable drops shall correspond with the total number of workstations, with expansion capability and layout flexibility to allow for tenant agency growth and/or reconfiguration of workspace areas.

· Tel-data Design Standards - The tele-data wiring design shall conform at minimum to the standards described in the State of Kansas Publication entitled, “Wiring Infrastructure Standards for New and Remodeled Offices, Version 2.71”, October 21, 2009 (click on link, below).  These guidelines are based on EIA/TIA 568 Commercial Building Telecommunications Wiring Standard, and on the BICSI Telecommunications Distribution Methods Manual.    




· 
Telephone device - The successful bidder shall provide individual phone lines to each space using the telcom information listed in the 4.22 space description below. 

4.19	Health & Life Safety Systems:

· Fire detection systems - The space will provide for fire alarm and smoke detection systems that are in compliance with all code standards, including ADA.

· Fire Extinguishers - Fire extinguishers shall be provided and maintained as required by code.

· Emergency lighting - Emergency lights will be provided and positioned, with rechargeable batteries with no less than 90 minutes of back up power per 2000 IBC.

· Emergency exit signs - Illuminated emergency exits signs shall be provided in accordance with 2006 IBC code requirements.  

· Other life safety requirements – The proposer shall identify all known or suspected hazardous or contaminated conditions on-site including, but not limited to, subsurface, surface, and the building and its building envelope.  Identify status of asbestos abatement, if any, for the facility.  Identify known or suspected areas of asbestos contamination.  Identify known surveys and abatement projects or investigations and the author.  The agency reserves the right to require the proposer to provide appropriate environmental audits, hazardous material studies, and abatement.  Agency will determine the need for this during negotiations.

4.20	Energy Design Criteria

· General - The State of Kansas seeks a facility that takes full advantage of proven technology through careful design and a reasonable balance between the cost of energy conservation improvements and their long-term economic value.  Accordingly, the items below list some of the basic energy-conservation features required of the selected building and space.  

· HVAC controls and set-back devices - HVAC equipment shall be properly sized and balanced to meet design conditions.  Each zone provided shall be equipped with programmable thermostatic controls, capable of a 55ο F night/weekend setback in the heating mode and 85ο F night/weekend set-up in the cooling mode.  Controls shall prevent reheating, re-cooling, and simultaneous heating and cooling in the same zone (where multiple system controls exist).  Conference rooms, training rooms, waiting and break rooms shall be zoned separately from normal office space to meet temperature, humidity and IAQ (indoor air quality) requirements of the conditioned space(s).

Minimum HVAC energy and efficiency standards - The State of Kansas requires that the following efficiency standards be achieved on HVAC systems in the proposed facility:

Winter:  	68-74 degF drybulb, 20-30% relative humidity
Summer:  	74-78 degF drybulb, 40-60% relative humidity 

The heating system will use either natural gas, electrical heat pump(s) in conjunction with natural gas back up, or heat recovery chiller.  The heating system energy source will be based on an economic analysis of the specific HVAC system design options considered.

Heating system efficiency will not be less than 80% steady state at full load for natural gas boilers or furnaces.

Air conditioning equipment will meet or exceed the performance ratings required under Federal and State guidelines.  

All ventilation systems will be controlled by a seven-day programmable time device.  Minimum ventilation rates will be capable of 15 cubic feet per minute per person during occupied hours and automatically reduced during off-work hours.

Buildings are to be in full compliance with the ANSI/ASHRAE/ESNA Standard 90.1, latest addition, Energy Design of New/Existing Commercial Buildings.

4.21	Applicable Codes for State Buildings:  (As of September, 2008)

	The Contractor shall ensure compliance with all applicable local and State building codes, ordinances, standards and regulations (see list below).  In the event that this RFP has requirements that do not comply with building codes, then the building code requirement will prevail.  In the event that the city/county does not have required building codes, the following shall apply (this list is not all-inclusive). 

1. 	International Building Code (IBC), 2006 Edition. 

a. 	Chapter 11, Accessibility, is deleted. See Item No. 11 below. 

b. 	Additionally, The Life Safety Code (NFPA 101, 2000 edition) will also be applicable on projects where its use is required to meet Federal requirements (i.e. if the facility receives Center for Medicaid/Medicare Services - CMS funding and inspections). 

2. 	International Building Fire Code (IFC), 2006 Edition. 

3. 	International Residential Code (IRC), 2006 Edition. 

4. 	International Mechanical Code (IMC), 2006 Edition. 

5. 	International Plumbing Code (IPC), 2006 Edition. 

6. 	International Fuel Gas Code (IFGC), 2006 Edition. 

7. 	International Energy Conservation Code (IECC), 2006 Edition. 

8. 	The codes and standards referenced in the Referenced Standards Chapter in the IBC, IFC, IRC, IMC, IPC, IFGC and IECC shall be applicable. 

9. 	National Fire Protection Association (NFPA), National Fire Codes and Standards, as referenced in the codes listed in item 1 through 7 or as required by Division of Facilities Management for special conditions. (NFPA 13 & 13R, 2002 edition – Installation of Sprinkler Systems Code and NFPA 72, 2002 edition – The National Fire Alarm Code are two such codes referenced in the IBC/IFC.) 

a. 	NFPA 101, 2000 edition - The Life Safety Code shall only be applicable on projects where its use is required to meet Federal requirements (i.e. if the facility receives CMS funding and inspections). 

b. 	NFPA 70 - National Electric Code (NEC), 2005 Edition is applicable. 

10.	Kansas Fire Prevention Code (This code combines many different documents including Kansas state statutes (K.S.A.), Kansas state regulations (K.A.R.), and Kansas State Fire Marshal (KSFM) interpretations and rules.) A list of pertinent statutes and regulations can be found at the KSFM website at http://www.accesskansas.org/firemarshal.) 

11. Americans with Disabilities Act Accessibility Guidelines for Buildings and Facilities (ADAAG), published in the Federal Register 7-26-91 (K.S.A. 58-1301 et seq.) and/or the Uniform Federal Accessibility Standards (UFAS), which also apply to agencies covered by Section 504 of the Rehabilitation Act of 1973. 

12. Kansas State Boiler Code (K.S.A 44-913 available though Kansas Department of Labor (http://www.dol.ks.gov found under workplace safety-labor safety programs-boiler safety) and the ASME Boiler Pressure Vessel Code, as referenced in Kansas State Boiler Code. 


SECTION V
SPECIFICATIONS
KANSAS SURPLUS PROPERTIES

4.3	Surplus Property Background and Scope:

The Surplus Property Program’s intent is to facilitate the disposition and reallocation of excess and surplus state property.  Kansas Surplus Property is currently is located at 2830 SW Kanza in Topeka.  This space consists of approximately 19,000 square feet.  Additionally, 5,000 square feet of storage space is currently provided by ten (10) 500 sq. ft. storage Conex trailers.  Warehouse spacing is provided by two separate buildings on the same grounds with approximately 10,000 sq. ft.  Space for up to 150 surplus vehicles is provided off-site.

The current lease expires in approximately 21-25 months; move-in date is to be negotiated.  30 off-street parking spaces are provided in the current leases.

4.4	Requested Lease Terms and Conditions for Surplus Property

The following provides an overview of the lease terms and conditions being sought by State of Kansas.  Additional lease terms and conditions will be provided for in the written Lease Agreement, which, together with the successful bidder’s responses to this RFP, constitutes the contractual agreement between the parties.

· Initial lease term desired:  5 years  
· Estimated space requirement:  Approximately 60,000 square feet of useable space (30,000 sq. ft. for warehousing, 28,000 sq. ft. for sales floor space and 2,000 sq. ft. for office space  
· Number of staff to accommodate in leased space:  10
· Number of off-street parking stalls required:  30
· Area for parking up to 150 surplus vehicles is desired, but not required.

4.8	Surplus Property Overall Space Requirements:

· Location – The office location is to be within 2 miles of the City limits; proximity to downtown is not required.  Easy customer accessibility is required. Compliance with the proper zoning requirements is the responsibility of the bidder.

· Office Space– If a multi-story facility is proposed, office space shall be on one (1) floor for the Federal Surplus – approximately 1500 sq. ft. and a second office will be necessary on the second floor for the State Surplus – approximately 1000 sq. ft.  

· Warehouse Space – Federal Surplus and State Surplus warehouse and retail space shall be separated, whether they be located on different floors, separated with chain link fencing (to allow visibility, but separation), etc.  Two (2) separate, high-ceiling warehouse areas are required.  A freight elevator, with a weight limit of not less than 6,000 lbs is required if two (2) docks are not available.  

· Parking - 30 off-street stalls.  An appropriate number of handicapped parking stalls, based on total parking requirements, shall be provided and located near the building entrance.  Visitor parking shall be available adjacent to or within reasonable walking distance from the building entrance.  The cost for staff off-street parking stalls is to be included in the cost of the lease.

· Tel-Data Infrastructure Access – The proposer is responsible for furnishing and installing the telecommunications wiring, outlets, or jacks to meet voice and data per agency requirements.  An estimated 12 voice/data jacks, 35 general electrical duplex outlets, and 14 computer duplex outlets are required.  Each location is to have the defined number of jacks or electrical outlets as specified.  Electrical circuits for computers and dedicated office equipment are to be separated from general office circuits.


4.9	Surplus Property Building Requirements:

· Interior sign placard for tenant agency – If agency office space is to be in a building shared with other tenants, proposer shall install a directory sign in building lobby listing floor and location of agency offices.   

· Break Room - Furnish and maintain as part of the lease one (1) break room/kitchen.  The break room should be located in the building so that it is convenient for staff usage.  The break room will be used both as a coffee area and for lunchtime activities.  Durable, easily cleaned finishes and flooring must be installed in these areas.  Approximately 6 linear feet (LF) of counter top and 6 LF of base cabinets for use as storage.  The break room also should have an installed exhaust fan and electrical hookups for a refrigerator and two (2) microwave ovens.  

· Exterior Signs - If the agency is the sole occupant of the building, furnish and install an aluminum exterior sign with 6” high letters stating:  “Kansas Surplus Properties”.  Final sign design to be approved by agency.  

· Common Area:  If both Divisions are located in the same facility, common areas such as breakrooms, storm shelters, restrooms, etc., would/could be shared, with bidders keeping in mind the total number of staff involved.

4.10	Surplus Property Interior Space Requirements:

· Space Type – Finished office space and warehouse.  See below.

· HVAC:  HVAC accommodations as described in the general specifications are preferred in the warehouse area, however, not required.  Bidders are instructed to provide information regarding HVAC accommodation in the warehouse if it varies from that described.

· Other electric design requirements – Panel board for tel-data should be located in for easy access.  

Surplus Property Space Requirements Breakdown

	LINE #
	DEPARTMENT – State Surplus Office
	TYPE
	WORK AREAS
	NET USABLE SQ FT
	TOTAL
NET USABLE
SQ FT

	1
	Manager
	E
	1
	175
	175

	2
	Administrative Assistant
	O
	1
	80
	80

	3
	Property Agent
	O
	2
	80
	160

	4
	Public Service Administrator
	O
	1
	80
	80

	5
	Warehouse Staff
	O
	3
	50
	150

	
	Subtotal
	
	8
	465
	645




	LINE #
	DEPARTMENT – Federal Surplus Office
	TYPE
	WORK AREAS
	NET USABLE SQ FT
	TOTAL
NET USABLE
SQ FT

	1
	Administrative Assistant
	O
	2
	80
	160

	2
	Property Agent
	O
	1
	80
	80

	3
	Program Consultant
	O
	1
	80
	80

	
	Subtotal
	
	4
	240
	320



	LINE #
	DEPARTMENT – Warehouse/Retail
	TYPE
	WORK AREAS
	NET USABLE SQ FT
	TOTAL
NET USABLE
SQ FT

	1
	State Surplus
	O
	1
	30,000
	30,000

	2
	Federal Surplus
	O
	1
	30,000
	30,000

	
	Subtotal
	
	2
	60,000
	60,000



	LINE #
	DEPARTMENT – Common & Support Areas
	TYPE
	WORK AREAS
	NET USABLE SQ FT
	TOTAL
NET USABLE
SQ FT

	6
	Tel-Data/Computer Room
	E
	1
	50
	50

	9
	Printer, Fax, Misc.
	O
	2
	50
	100

	   11
	Break Room
	O
	1
	150
	150

	12
	Custodial and Storage
	E
	1
	50
	50

	13
	Restrooms
	E
	1
	100
	100

	14
	Waiting Area
	O
	1
	50
	50

	
	Subtotal
	
	6
	450
	500



Area Type Definitions:

A	Area partly enclosed or open depending on space plan or building configuration
E	Enclosed room or workstation with hard wall construction with a door
O	Open office area – may use miscellaneous open office systems furniture and components (typically Herman Miller).


Summary of Space Requirements - Surplus Property
	
	
	
# OF
WORK STATIONS
	
# OF AREA UNITS
	
NET 
SQUARE FEET

	1
	Office Area*
	12
	2
	1,545

	2
	Warehouse/Retail
	2
	2
	60,000

	
	Total Departmental & Common Area*
	11
	4
	61,545




Total Dept. and Common Area Sq Ft times an Interior Circulation multiplier of 30%.

	
	
Subtotal
	
Percent
	Total Useable Office Area

	Total Useable Area*
	1545
	30%
	2,000



Note:  The Total Useable square footage is expected to be in close proximity to total rentable area.


*The preceding is the approximate square footage need.  Each building is unique, and development of the building floor plan will determine the actual square footage need.

4.18	Surplus Property Security Requirements

· General - The proposed plan must take into account building and site security, which shall be developed in detail with the tenant agency as part of the design process.  The following security features shall be understood as a baseline requirement, possibly supplemented with other security systems as may be requested by the tenant agency on a to-be-negotiated basis.

· Access management – Not Required

· Intrusion detection & control - Intrusion detection and alarm devices shall be required for the space.  

· Video surveillance – Not required.

· Security lighting - Photo sensors, time clocks, motion detection shall automatically control building exterior and site lighting, or a combination of both where required for security conditions.  

4.21	Telecommunication Jacks, Electrical Outlets, Special Lighting - Surplus Property

	Line
#
	Area
	Type A,E,O
	Work
Areas
	Telecom
Jacks
	General
Outlets
	Computer
Outlets
	Room
Fans
	Notes

	1
	Manager Office
	E
	1
	1
	1
	1
	1
	

	2
	Front Office / Fed
	O/A
	2
	2/1 FAX
	6
	2
	1
	FED

	3
	Staff Office / Fed
	E/O/A
	4
	4
	4
	4
	1
	FED

	4
	Front Office / State 
	E
	1
	1
	3
	1
	1
	STATE

	5
	Staff Office / State
	O/A
	2
	2
	6
	2
	1
	STATE

	6
	Retail Space / Fed
	O
	-
	-
	4
	-
	4
	FED

	7
	Retail Space / State 
	O
	-
	-
	4
	-
	4
	STATE

	8
	Inventory warehouse / State
	O
	1
	-
	2
	-
	1
	STATE

	9
	Inventory Warehouse / Fed
	O
	1
	-
	2
	-
	1
	FED




Notes:	The above number of electrical outlets is for a duplex outlet.  However, when applicable a four-plex design is desired containing a duplex outlet for general usage and another color keyed duplex outlet for computer usage whenever possible.  If separate outlets are used a general outlet is required to be located in proximity to each computer outlet and these jacks must separated by at least one (1) foot to avoid electrical interference.  The tel-data room has specific design requirements to be met not withstanding this schedule.

AREA TYPE DEFINITIONS:

A	Area partly enclosed or open depending on space plan or building configuration
E	Enclosed room or workstation with hard wall construction with a door
O	Open office area - may use miscellaneous open office systems furniture and components (typically Herman Miller).  

EXHIBIT A – VENDOR'S ESTIMATED COST WORKSHEET (1ST TAB)
&
EXHIBIT B - VENDOR'S PROPOSED LEASE COST SUBMISSION FORM (2ND TAB)

Bidders should use the MS Excel worksheets available by clicking on the icons below.  Populate the necessary pricing fields, print and submit with bid documents.  There are two (2) tabs on this worksheet (exhibit a & exhibit b).  Include both with your proposal.

The State of Kansas will not pay any up-front payments or payments in addition to that which bidders indicate on the attached worksheets.



· VARIANCE(S) REQUESTED:  Check this box if this proposal is contingent upon any variances to provisions of the Specifications and/or Attachment(s).  All variances to the Specifications and Attachment(s) must be fully explained on a separate document attached to the completed Proposal Forms.  Failure to comply with this requirement may result in disqualification of the proposal or, at the discretion of the State, insistence on full compliance with Specifications.

VENDORS ARE INSTRUCTED TO COMPLETE THE FOLLOWING:

Vendors are instructed to complete the following:

1)	Site the source and provide applicable documentation for the pricing on the following items:

Insurance:   	

Taxes:		

Utilities:  		

2)	Provide comparable rates for leases within the same geographical area:
	
	

3)  The proposed facility is:	7)  The proposed premises are:
____ (a) an existing structure with renovations	____ (a) all in one continuous space
____ (b) an existing structure with no renovations	____ (b) located on more than one level
____ (c) an existing structure with an addition	____ (c) located on one level but different areas, not ____ (d) new construction		connected

4)  The proposed premises are currently:	8)  The exterior of the proposed facility is:
____ (a) owned by the bidder	____ (a) brick	____ (b) block	____ (c) wood
____ (b) Bidder has a signed option to purchase contract	____ (d) metal	____ (e) drivit	____ (f) other
____ (c ) Bidder is acquiring an option to purchase contract
____ (d) Bidder has a verbal agreement with the owner	9)  The proposed facility’s roof is:
____ (e) Bidder has no ownership rights or obligations	____ (a) Shingle____ (b) metal____ (c) membrane
____ (f) Broker representing an individual

5)  In order to comply with local zoning 	10)  The proposed facility’s HVAC system is:
     requirements, the proposed premises:	Heat:  ____ (a) gas____ (b) electric  (c) other ____
____ (a) are zoned correctly____ (b) must be re-zoned	Air:     ____ (a) gas____ (b) electric  (c) other ____
		(if other, please clarify)

6)  The proposed facility would be designed for and 	11)  The proposed facility’s parking lot is:
     occupied by:	____ (a) asphalt	____ (b) concrete
____ (a) only the agency(s) specified in this RFP
____ (b) the agency(s) specified in this RFP and other 	12)  The proposed facility is:  
	state agencies	____ (a) single level ____ (b) a multi-level 
____ (c) the agency(s) specified in this RFP and other 
	non-state organization(s)


	
EXHIBIT C—BIDDER’S PROPOSED PROJECT SCHEDULE
(Schedule shall include ALL agencies)

BID CONTRACT NUMBER:  __________________________________
BIDDER NAME:________________________________________________________


	 #
	MILESTONE
	DURATION
	START
	COMPLETION

	 1
	Lease agreement approved
	
	
	

	 2
	Final space plan due from Owner
	
	
	

	 3
	50% Construction Document Review
	
	
	

	 4
	Final Construction Document Review
	
	
	

	 5
	Building permit acquisition
	
	
	

	 6
	Construction contract bid/award
	
	
	

	 7
	Demolition of existing structure
	
	
	

	 8
	Start of construction or remodeling
	
	
	

	 9
	Foundation work
	
	
	

	10
	Rough framing
	
	
	

	11
	Building enclosed
	
	
	

	12
	Interior framing
	
	
	

	13
	Mechanical rough-in
	
	
	

	14
	Electrical rough-in
	
	
	

	15
	Telecom conduit installed
	
	
	

	16
	Construction complete
	
	
	

	17
	Occupancy permit awarded
	
	
	

	18
	ADAAG checklist completed
	
	
	

	19
	Inspection and occupancy by State tenant
	
	
	





Shaded milestone numbers are the responsibility of State of Kansas personnel and/or their contractors.


Bidder  ______________________________  Bidder’s Signature:______________________________________


SECTION VI
SPECIFICATIONS
FACILITIES MANAGEMENT GROUNDS DEPARTMENT

5.2	Grounds Department Background and Scope:

The Grounds Department is responsible for the maintenance of all state owned property within the Capital Complex and Cedar Crest. The Department is currently located at 400 Van Buren in Topeka. 

5.3	Requested Lease Terms and Conditions

The following provides an overview of the lease terms and conditions being sought by State of Kansas.  Additional lease terms and conditions will be provided for in the written Lease Agreement, which, together with the successful bidder’s responses to this RFP, constitutes the contractual agreement between the parties.

· Initial lease term desired:  5 years
· Estimated space requirement:  Approximately 25,000 square feet of garage and 30,000 square feet of outdoor storage. 
· Number of staff to accommodate in leased space:  10
· Number of off-street parking stalls required:  10.

5.8	Overall Space Requirements:

· Location – The office location is to be as close proximity to the Capital Complex while meeting all zoning requirements. Compliance with the proper zoning requirements is the responsibility of the bidder. 

· Office Space– Office space shall be on one (1) floor. 

· Shop Space – The shop area shall be approximately 25,000 sq. ft. The area should be on the ground level, have a garage door for entry of, and exit of equipment. In addition the area should have a for employee entrance. The shop area shall have the following items: 

· Wash bay for the washing of equipment with floor drainage within the bay. The area should have water connections and shall conform to all requirements and approvals for dumping into the city sewer.

· Outdoor Storage – The outdoor storage area will house sand/salt for usage in addition to fuel storage. The proposal shall meet all zoning requirements for the storage of the above mentioned items. 

· Parking - 10 off-street stalls.  An appropriate number of handicapped parking stalls, based on total parking requirements, shall be provided and located near the building entrance.  Visitor parking shall be available adjacent to or within reasonable walking distance from the building entrance.  The cost for staff off-street parking stalls is to be included in the cost of the lease.

· Tel-Data Infrastructure Access – The proposer is responsible for furnishing and installing the telecommunications wiring, outlets, or jacks to meet voice and data per agency requirements.  An estimated 4 voice/data jacks, 4 general electrical duplex outlets, and 4 computer duplex outlets are required. Each location is to have the defined number of jacks or electrical outlets as specified. Electrical circuits for computers and dedicated office equipment are to be separated from general office circuits.

· Break Room –The requirement is for 10 employees. If located on the same premises, this area can be provided in conjunction with Federal and State Surplus break room. If so please adjust the State Surplus break room size accordingly. 

5.10	Interior Space Requirements:

· Space Type – Finished office space and warehouse. 

· HVAC:  HVAC requirement in the shop area is for heating as described above. The installation of cooling in the shop area is not required.

Grounds Department Space Requirements Breakdown

	LINE #
	DEPARTMENT – Office
	NOTES
	TYPE
	WORK AREAS
	NET USABLE SQ FT
	TOTAL
NET USABLE
SQ FT

	1
	Manager
	
	O
	1
	80
	80

	2
	Administrative Assistant
	
	O
	1
	80
	80

	3
	Fax/Copier Area
	
	O
	1
	80
	80

	
	
	
	
	
	
	

	
	
	
	
	3
	240
	240



	LINE #
	DEPARTMENT – Shop  Area
	NOTES
	TYPE
	WORK AREAS
	NET USABLE SQ FT
	TOTAL
NET USABLE
SQ FT

	1
	Shop
	
	O
	1
	25,000
	25,000

	
	
	
	
	
	
	

	
	Subtotal
	
	
	1
	25,000
	25,000




	LINE #
	DEPARTMENT – Outdoor Storage
	NOTES
	TYPE
	WORK AREAS
	NET USABLE SQ FT
	TOTAL
NET USABLE
SQ FT

	1
	Outdoor Storage
	
	O
	1
	30,000
	30,000

	
	
	
	
	
	
	

	
	Subtotal
	
	
	1
	30,000
	30,000



Area Type Definitions:

A	Area partly enclosed or open depending on space plan or building configuration
E	Enclosed room or workstation with hard wall construction with a door
O	Open office area – may use miscellaneous open office systems furniture and components (typically Herman Miller).

Summary of Space Requirements - Grounds
	
	
	# OF
WORK STATIONS
	# OF AREA UNITS
	NET 
SQUARE FEET

	1
	Office Area*
	2
	
	240

	2
	Shop Area
	
	
	25,000

	
	Outdoor Area
	
	
	30,000

	
	Total Departmental & Common Area*
	2
	
	55,240



Total Grounds Dept. and Common Area Sq Ft times an Interior Circulation multiplier of 30%.

	
	Subtotal
	Percent
	Total Useable Office Area

	Total Useable Area*
	240
	30%
	312



Note:  The Total Useable square footage is expected to be in close proximity to total rentable area.


*The preceding is the approximate square footage need.  Each building is unique, and development of the building floor plan will determine the actual square footage need.

5.18	Security Requirements – Grounds Department

General - The proposed plan must take into account building and site security, which shall be developed in detail with the tenant agency as part of the design process.  The following security features shall be understood as a baseline requirement, possibly supplemented with other security systems as may be requested by the tenant agency on a to-be-negotiated basis.

Access management – Not Required

Intrusion detection & control - Intrusion detection and alarm devices shall be required for the space.  

Video surveillance – Not required.

Security lighting - Photo sensors, time clocks, motion detection shall automatically control building exterior and site lighting, or a combination of both where required for security conditions.  

5.21	Grounds Department Telecommunication Jacks, Electrical Outlets, Special Lighting 

	Line
#
	Area
	Type A,E,O
	Work
Areas
	Telecom
Jacks
	General
Outlets
	Computer
Outlets
	Room
Fans
	Notes

	1
	Manager Office
	O
	1
	1
	1
	1
	
	

	2
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	



Notes:	The above number of electrical outlets is for a duplex outlet.  However, when applicable a four-plex design is desired containing a duplex outlet for general usage and another color keyed duplex outlet for computer usage whenever possible.  If separate outlets are used a general outlet is required to be located in proximity to each computer outlet and these jacks must separated by at least one (1) foot to avoid electrical interference.  The tel-data room has specific design requirements to be met not withstanding this schedule.

AREA TYPE DEFINITIONS:

A	Area partly enclosed or open depending on space plan or building configuration
E	Enclosed room or workstation with hard wall construction with a door
O	Open office area - may use miscellaneous open office systems furniture and components (typically Herman Miller).  


EXHIBIT A – VENDOR'S ESTIMATED COST WORKSHEET (1ST TAB)
&
EXHIBIT B - VENDOR'S PROPOSED LEASE COST SUBMISSION FORM (2ND TAB)

Bidders should use the MS Excel worksheets available by clicking on the icons below.  Populate the necessary pricing fields, print and submit with bid documents.  There are two (2) tabs on this worksheet (exhibit a & exhibit b).  Include both with your proposal.

The State of Kansas will not pay any up-front payments or payments in addition to that which bidders indicate on the attached worksheets.



· VARIANCE(S) REQUESTED:  Check this box if this proposal is contingent upon any variances to provisions of the Specifications and/or Attachment(s).  All variances to the Specifications and Attachment(s) must be fully explained on a separate document attached to the completed Proposal Forms.  Failure to comply with this requirement may result in disqualification of the proposal or, at the discretion of the State, insistence on full compliance with Specifications.

VENDORS ARE INSTRUCTED TO COMPLETE THE FOLLOWING:

Vendors are instructed to complete the following:

1)	Site the source and provide applicable documentation for the pricing on the following items:

Insurance:   	

Taxes:		

Utilities:  		

2)	Provide comparable rates for leases within the same geographical area:
	
	

3)  The proposed facility is:	7)  The proposed premises are:
____ (a) an existing structure with renovations	____ (a) all in one continuous space
____ (b) an existing structure with no renovations	____ (b) located on more than one level
____ (c) an existing structure with an addition	____ (c) located on one level but different areas, not ____ (d) new construction		connected

4)  The proposed premises are currently:	8)  The exterior of the proposed facility is:
____ (a) owned by the bidder	____ (a) brick	____ (b) block	____ (c) wood
____ (b) Bidder has a signed option to purchase contract	____ (d) metal	____ (e) drivit	____ (f) other
____ (c ) Bidder is acquiring an option to purchase contract
____ (d) Bidder has a verbal agreement with the owner	9)  The proposed facility’s roof is:
____ (e) Bidder has no ownership rights or obligations	____ (a) Shingle____ (b) metal____ (c) membrane
____ (f) Broker representing an individual

5)  In order to comply with local zoning 	10)  The proposed facility’s HVAC system is:
     requirements, the proposed premises:	Heat:  ____ (a) gas____ (b) electric  (c) other ____
____ (a) are zoned correctly____ (b) must be re-zoned	Air:     ____ (a) gas____ (b) electric  (c) other ____
		(if other, please clarify)

6)  The proposed facility would be designed for and 	11)  The proposed facility’s parking lot is:
     occupied by:	____ (a) asphalt	____ (b) concrete
____ (a) only the agency(s) specified in this RFP
____ (b) the agency(s) specified in this RFP and other 	12)  The proposed facility is:  
	state agencies	____ (a) single level ____ (b) a multi-level 
____ (c) the agency(s) specified in this RFP and other 
	non-state organization(s)


	
EXHIBIT C—BIDDER’S PROPOSED PROJECT SCHEDULE
(Schedule shall include ALL agencies)

BID CONTRACT NUMBER:  __________________________________
BIDDER NAME:________________________________________________________


	 #
	MILESTONE
	DURATION
	START
	COMPLETION

	 1
	Lease agreement approved
	
	
	

	 2
	Final space plan due from Owner
	
	
	

	 3
	50% Construction Document Review
	
	
	

	 4
	Final Construction Document Review
	
	
	

	 5
	Building permit acquisition
	
	
	

	 6
	Construction contract bid/award
	
	
	

	 7
	Demolition of existing structure
	
	
	

	 8
	Start of construction or remodeling
	
	
	

	 9
	Foundation work
	
	
	

	10
	Rough framing
	
	
	

	11
	Building enclosed
	
	
	

	12
	Interior framing
	
	
	

	13
	Mechanical rough-in
	
	
	

	14
	Electrical rough-in
	
	
	

	15
	Telecom conduit installed
	
	
	

	16
	Construction complete
	
	
	

	17
	Occupancy permit awarded
	
	
	

	18
	ADAAG checklist completed
	
	
	

	19
	Inspection and occupancy by State tenant
	
	
	





Shaded milestone numbers are the responsibility of State of Kansas personnel and/or their contractors.


Bidder  ______________________________  Bidder’s Signature:______________________________________


State of Kansas
Department of Administration
DA-146a    (Rev. 1-01)

CONTRACTUAL PROVISIONS ATTACHMENT

Important:	This form contains mandatory contract provisions and must be attached to or incorporated in all copies of any contractual agreement.  If it is attached to the vendor/contractor's standard contract form, then that form must be altered to contain the following provision:

	"The Provisions found in Contractual Provisions Attachment (Form DA-146a, Rev. 1-01), which is attached hereto, are hereby incorporated in this contract and made a part thereof."

	The parties agree that the following provisions are hereby incorporated into the contract to which it is attached and made a part thereof, said contract being the _____ day of ____________________, 20_____.

 1.	Terms Herein Controlling Provisions:  It is expressly agreed that the terms of each and every provision in this attachment shall prevail and control over the terms of any other conflicting provision in any other document relating to and a part of the contract in which this attachment is incorporated.

 2.	Agreement With Kansas Law:  All contractual agreements shall be subject to, governed by, and construed according to the laws of the State of Kansas.

 3.	Termination Due To Lack Of Funding Appropriation:  If, in the judgment of the Director of Accounts and Reports, Department of Administration, sufficient funds are not appropriated to continue the function performed in this agreement and for the payment of the charges hereunder, State may terminate this agreement at the end of its current fiscal year.  State agrees to give written notice of termination to contractor at least 30 days prior to the end of its current fiscal year, and shall give such notice for a greater period prior to the end of such fiscal year as may be provided in this contract, except that such notice shall not be required prior to 90 days before the end of such fiscal year.  Contractor shall have the right, at the end of such fiscal year, to take possession of any equipment provided State under the contract.  State will pay to the contractor all regular contractual payments incurred through the end of such fiscal year, plus contractual charges incidental to the return of any such equipment.  Upon termination of the agreement by State, title to any such equipment shall revert to contractor at the end of State's current fiscal year.  The termination of the contract pursuant to this paragraph shall not cause any penalty to be charged to the agency or the contractor.

 4.	Disclaimer Of Liability:  Neither the State of Kansas nor any agency thereof shall hold harmless or indemnify any contractor beyond that liability incurred under the Kansas Tort Claims Act (K.S.A. 75-6101 et seq.).

 5.	Anti-Discrimination Clause:  The contractor agrees: (a) to comply with the Kansas Act Against Discrimination (K.S.A. 44-1001 et seq.) and the Kansas Age Discrimination in Employment Act (K.S.A. 44-1111 et seq.) and the applicable provisions of the Americans With Disabilities Act (42 U.S.C. 12101 et seq.) (ADA) and to not discriminate against any person because of race, religion, color, sex, disability, national origin or ancestry, or age in the admission or access to, or treatment or employment in, its programs or activities; (b) to include in all solicitations or advertisements for employees, the phrase "equal opportunity employer"; (c) to comply with the reporting requirements set out at K.S.A. 44-1031 and K.S.A. 44-1116; (d) to include those provisions in every subcontract or purchase order so that they are binding upon such subcontractor or vendor; (e) that a failure to comply with the reporting requirements of (c) above or if the contractor is found guilty of any violation of such acts by the Kansas Human Rights Commission, such violation shall constitute a breach of contract and the contract may be cancelled, terminated or suspended, in whole or in part, by the contracting state agency or the Kansas Department of Administration; (f) if it is determined that the contractor has violated applicable provisions of ADA, such violation shall constitute a breach of contract and the contract may be cancelled, terminated or suspended, in whole or in part, by the contracting state agency or the Kansas Department of Administration.

	Parties to this contract understand that the provisions of this paragraph number 5 (with the exception of those provisions relating to the ADA) are not applicable to a contractor who employs fewer than four employees during the term of such contract or whose contracts with the contracting state agency cumulatively total $5,000 or less during the fiscal year of such agency.

 6.	Acceptance Of Contract:  This contract shall not be considered accepted, approved or otherwise effective until the statutorily required approvals and certifications have been given.

 7.	Arbitration, Damages, Warranties:  Notwithstanding any language to the contrary, no interpretation shall be allowed to find the State or any agency thereof has agreed to binding arbitration, or the payment of damages or penalties upon the occurrence of a contingency. Further, the State of Kansas shall not agree to pay attorney fees and late payment charges beyond those available under the Kansas Prompt Payment Act (K.S.A. 75-6403), and no provision will be given effect which attempts to exclude, modify, disclaim or otherwise attempt to limit implied warranties of merchantability and fitness for a particular purpose.

 8.	Representative's Authority To Contract:  By signing this contract, the representative of the contractor thereby represents that such person is duly authorized by the contractor to execute this contract on behalf of the contractor and that the contractor agrees to be bound by the provisions thereof.

 9.	Responsibility For Taxes:  The State of Kansas shall not be responsible for, nor indemnify a contractor for, any federal, state or local taxes which may be imposed or levied upon the subject matter of this contract.

10.	Insurance:  The State of Kansas shall not be required to purchase, any insurance against loss or damage to any personal property to which this contract relates, nor shall this contract require the State to establish a "self-insurance" fund to protect against any such loss or damage.  Subject to the provisions of the Kansas Tort Claims Act (K.S.A. 75-6101 et seq.), the vendor or lessor shall bear the risk of any loss or damage to any personal property in which vendor or lessor holds title.

11.	Information:  No provision of this contract shall be construed as limiting the Legislative Division of Post Audit from having access to information pursuant to K.S.A. 46-1101 et seq.

12.	The Eleventh Amendment:  "The Eleventh Amendment is an inherent and incumbent protection with the State of Kansas and need not be reserved, but prudence requires the State to reiterate that nothing related to this contract shall be deemed a waiver of the Eleventh Amendment."
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1.0
INTRODUCTION 


1.1  
Subject:  Telecommunications wiring guidelines apply to all Department of Social and Rehabilitation(SRS) agency buildings within the State of Kansas.


1.2
Intent: SRS ITS wants to have a uniform wiring plan for voice, data, image, and video to allow flexibility for personnel changes, office renovations and equipment migration and updates, as well as current technology. This concept is based on a structured cabling system that is not vendor proprietary and conforms to most accepted Commercial Wiring Standards.


1.3
Authority: The Information Technology Services(ITS) section, Infrastructure Management section, of SRS will be the authority, responsible for compliance with State policy.


1.4
Scope: These guidelines are intended to provide advisory guidelines for state agencies for all new state buildings, major renovations or multi-tenant occupancy. Specifically these guidelines are for wiring in: 

· 

Newly constructed buildings 


· 

Buildings undergoing major renovations


· 

New long-term leased occupancy 


· 

New multi-building networks with state owned fiber or wire cable


· 

New or remodeled buildings containing multiple tenants


For retrofitting and telecommunications recabling, these guidelines should be used unless there is valid justification for not doing so.  Unless specifically exempted, all telecom rooms, equipment closets, etc., in multiple tenant buildings will comply with all requirements included in this document.


1.5
Exclusions


A. Video is considered a special case and is not covered within these guidelines. 


B. Any building containing tenants other than SRS staff is considered a special case, and will have to be reviewed extensively before an infrastructure plan can be prepared.


These guidelines are based on EIA/TIA 568 Commercial Building Telecommunications Wiring Standard and on the BICSI© Telecommunications Distribution Methods Manual. The BICSI© manual is a good source for detailed planning of telecommunications distribution systems.  These guidelines do not recommend a particular method of horizontal distribution (under floor, ceiling, under carpet, etc.) because of the wide disparity of buildings and designers used in the state. The BICSI© manual cited above and EIA/TIA 569 are excellent references and should be reviewed for more detail on horizontal pathways.  The National Electrical Code and other national, state and local building codes are recognized as having jurisdiction over related parts of these guidelines.


1.6  Purpose: This guideline is intended to give recommended minimum requirements for telecommunications service for general and administrative office space. The guidelines address the physical pathways, media, and cable administration practices 


The purpose is threefold:


· To provide direction. 


· To enable the planning of telecommunications facilities with little knowledge of the specific products that will be installed. 


· To define a generic telecommunications wiring system that will support most agency wiring needs in a multi- vendor and/or multi-product environment.

2.0
APPROACH 


This guideline follows the generally accepted best practice standard of using a "premise distribution system" (PDS). A PDS attempts to wire a building for information needs without knowing specifically what equipment will be utilized. A PDS is geared for long term stability and flexibility and is based on the idea of wiring the building once. 

The premise distribution cabling system approach allows the wire and outlets to remain unchanged while the connections and services vary. The main components of a PDS are:


· Common Media - Unshielded twisted pair (UTP) and/or fiber optic cables capable of supporting voice, image and data communications. Services can change without affecting the media used to connect the services. 


· Star Topology - Media is distributed only from designated frames within the system. The signal quality improves because the number of connections is limited. 


· Cross connects - Cross connects and patch panels provide the system with the flexibility to make changes to the service quickly and easily using jumper wires or modular jacks and patch cords. Agency personnel with little training can make changes to the service in the work area, thereby reducing the amount of time, effort, and cost in making changes. 


· Universal outlet - Common universal outlets provide a standard interface that permits devices to connect to any service by changing the connection to the outlet and not the outlet itself. Connection to the outlet can be done directly or by using adapters when necessary. 


· Administration - An administrative system is used to record installations and is maintained on a continuing basis. 


3.0
WIRING SYSTEM ELEMENTS

3.1 Horizontal wiring


The horizontal wiring is the wiring from the telecommunications outlet to the connecting frame in the telecommunications closet and is UTP Level 6a (or current highest standard) for LAN or UTP Level 3 for Voice with pathway planning for fiber.


3.2 Telecommunications closets 


Telecommunications closets are spaces dedicated to the use of interconnecting wiring and equipment. It is here that the logical topology wiring is accomplished. The physical star workstations may be connected in ring or bus topologies in addition to star. 


3.3 Backbone Wiring


Backbone wiring is the riser wiring in multi-story buildings or the main distribution system in a campus environment. Single-mode fiber optic cable is the required minimum backbone topology for Local Area Network(LAN) wiring, unless valid justification can be made for UTP.  UTP multi-pair cabling is acceptable for voice riser installations, upon approval from SRS ITS Telecom.


3.4 Entrance facility 


This is not the point where the local telephone company enters the building(also called the Point Of Minimum Penetration(POMP)), but is considered the demarcation point between the local telephone company and the user.  Any telephone company demarcation points are required to be located in a secured room, generally called the “equipment” or “telecommunications” room.  This is also called the Demarc.  This Demarc must be located in the same SRS-controlled telecommunications closet as the equipment and systems that connect to the Demarc, in order to comply with SRS security requirements and HIPAA requirements.

3.5 Tuned Category 6augmented Wiring Plant


A “tuned” system is defined as containing one patch panel port, wiring, and one jack outlet of Category 6augmented specifications, provided by the property owner, from the same manufacturer, and installed by certified installation personnel.  This wiring plant will be tested and certified by the wiring installer to meet Category 6augmented standards.  This “tuned” system only relates to the data side of these wiring specifications.  Voice wiring is not included, unless specifically directed by SRS Telecom.  See section 4 for more information.


3.6 Campus distribution 


The interbuilding connections and campus backbone in a complex or multi-building environment.


4.0
HORIZONTAL WIRING

4.1
Structure: The horizontal wiring structure extends from the telecommunications closet to the telecommunications outlet, and includes the outlet, the horizontal distribution system cables, the wiring supporting rack, patch panels(if determined by SRS Telecom) and the cross-connect in the closet.  The word “wire” may reflect UTP, Fiber, or other media.


4.2
Major items: The major points of the horizontal system are:


 Star topology  -  each outlet is directly connected to a closet.  This does not preclude physical bus and ring topology;  this is done in the telecommunications closet.  Advanced planning considers the use of fiber optic cabling to all training rooms, conference rooms and computer rooms.  On a business case basis, pathways of inner duct, raceways and conduit are provided to support the use of fiber optic cabling.  Cable length maximums are determined by the media itself.


4.3
Outlets and Jacks.



4.3.1 Cable and Jack Specifications



This suggested configuration will serve most needs:


Four pairs (8 wires) of unshielded twisted pair (UTP) for voice (CAT 3 minimum) and another four pairs for data(CAT 6a or current highest standard) applications.  The performance for these cables is defined by recently adopted EIA/TIA Category 6augmented standard.  All voice(CAT3) pairs are terminated in a RJ11-size 4 pin jack, and data pairs are terminated in a RJ45-size 8 pin jack.  The latter jack must be "Category 6a (or current highest standard)" compliant. These jacks must be wired with the EIA/TIA 568B pin-out. A faceplate should be provided that will allow expansion.  Each jack should be mounted in an industry-standard double-gang outlet box, mounted 18 inches above the floor, equipped with a reducer ring for single-faceplate mounting where needed.  For offices of 5,000 square feet or less, ¾” conduit should be used for each faceplate location unless otherwise identified by SRS ITS Telecom.  For buildings exceeding 5,000 square feet, 1” conduit should be used for each faceplate location as the minimum acceptable size, unless there is a valid business case to use a smaller size.  Regardless of the size of building, industry-accepted fill rates for the appropriate wires being used shall not be exceeded.


Each outlet box should be connected to one (1) inch conduit, with insulated bushing, stubbed out above the finished ceiling or top plates, unless otherwise directed by SRS ITS Telecom.


The LAN jacks, patch panels, wiring and all other related items should be from a manufacturer’s certified installer.  A manufacturer should be selected that will certify and warranty a “tuned” wiring plant installation, guaranteed to pass the Category 6a Alien Cross-talk test.   This “tuned” system contains one patch panel port, wiring, and one jack outlet, provided by the property owner, from the same manufacturer, and installed by certified installation personnel.  All workstation location outlets should consist of the following parts: one faceplate(allowing for a minimum of 6 jack outlets); each faceplate assembly must contain a required minimum of one (1) four-pin Category 3 Voice Outlet Module, and one (1) Category 6a 8-pin LAN outlet module;  each workstation data/LAN location will include the associated patch panel port for that location.

4.3.2
Location and Spacing


Outlets should be located to give every work space location an outlet. If locations have not been determined, then a quantity estimate of one location per 100 square feet should be made. Each conference room should be provided with at least one voice and data outlet, plus one wall-mount outlet(voice only). Consideration should be given to spaces that may be eventually used as work spaces.  Additional outlets may be identified during floor space planning and will be ordered during installation where possible.


4.3.3
Acceptable cables


Unshielded Twisted Pair – Category 3 for voice applications and Category 6a (or current highest standard) for LAN applications, conforming to industry standard specifications and requirements.  All wiring must be plenum-rated wiring. All Category 6a wiring must be installed in accordance with the installation standards and guidelines contained in the recently adopted EIA/TIA Category 6augmented standard.

4.3.4
Electrical Service


A minimum of two(2) duplex 110 Volt 20 ampere AC power outlets shall be provided for each work space location or private office.  There shall be one duplex 110 Volt  20 ampere AC power outlet, on a dedicated, isolated ground circuit, provided for computer use at each work space location or private office, unless there is valid justification not to do so.  All specialty or dedicated outlets shall be color-coded for ease of identification.


4.4
Wiring support racks


Wire support racks must be provided from the main telecommunications room, across and above the finished ceiling, to central points located amongst the workstation areas.  This rack must be of commercially-manufactured origin, sized to fit the particular cable running path and must be sized to no more than a 40% fill rate This wiring rack/path should be constructed in such a way that conforms with the recently adopted EIA/TIA Category 6a standard.  This rack must be securely fastened as appropriate to solid building points.  A pull wire or string should be placed in the wiring rack to facilitate additions after rack installation.  All wiring racks must be grounded to each other to provide a contiguous ground from bus bar ground to the end of the wiring rack.  The path for this rack installation shall be determined by SRS Telecom personnel in conjunction with building architectural staff.


4.5
Building Wide One-way Paging System

SRS will provide equipment for this system but not the building wiring for a multiple zone one-way paging system.  The proposers wiring vendor will be required to install this wiring as required by SRS.  SRS will provide the speakers as well as identify the speaker locations, and number of zones after the building design is completed and a detailed floor plan has been developed.  The cost for this work is to be incorporated into the cost of the lease agreement.  System design, as it relates to the wire size and number of speakers per wire run will conform to established technical specifications for the paging system selected by SRS and will be the responsibility of the wiring vendor.

4.6
Fiber Optic cable specifications


Singlemode Fiber Specification 


The singlemode cable shall meet the EIA/TIS-492CAAA, "Detail Specification for Class IVa Dispersion Unshifted Single Mode Optical Fiber Cable. and ITU-T G.652 "Characteristics of Singlemode Optical Fiber Cable


Fiber type: Singlemode


Coating Diameter: 250 Microns Core Eccentricity: 7.5% maximum (1.5% typical) Numerical aperture: 275 plus or minus .0 15 


Attenuation: 1.0 dB/KM @ 1310 NM & 0.75 dB/KM @ 1550 NM 


Bandwidth:  N/A


Distance:  Serial Gigabit Ethernet=5000M @1310 NM, Serial 10 Gigabit 


Ethernet =10,000M @1300 NM for 10GBase-LX4, 10,000M@ 1310NM for 10GBase-L 


& 40,000M@1550 NM for the 10Gbase-E


Maximum Dispersion :  Less than 3.2 PS/NM*KM @ 1310 NM and less than 18 


PS/(NM*KM )@ 1550NM


Fiber connectors: SC (straight through) tyW - .4 dB plus or minus .2 dB 


loss maximum Single Mode Fiber Specifications 


Fiber type 8 Micron Cladding diameter 125 Micron 


Attenuation.5 dB/KM @ 850 NM.5 dB/KM @ 1350 NM 


Zero dispersion wavelength 1300-1320 NM 


UL rating of OFNR for riser usage OFNP for Plenum usage 


Cable bend radius 20 times the cable diameter during installation


5.0
TELECOMMUNICATIONS CLOSET 


5.1
Riser Closets: In multi-story buildings, closets shall be stacked, when practical. Closets should be directly vertically above/below each other with riser provisions between them, and must have two(2) conduits or sleeves of at least 3 inch diameter connecting the rooms.  If rooms are not stacked then riser and conduit provisions as outlined here will still apply.


5.2
Size:  Equipment rooms and telecommunications closets should be large enough to house all telecommunications &  networking systems and devices,  equipment racks, wiring facilities, and public networking equipment as needed.  Closets should have a minimum ceiling height of 8 feet.  This ceiling may be suspended acoustical tile or a finished ceiling.  Fire protection for telecom rooms must be in compliance with local building and fire codes.  There shall be no wet pipes traversing, entering or residing in the telecom room unless specifically required in local building or fire codes.  No sinks, furnaces, air conditioners or other moisture-producing devices will be allowed in telecommunications closets or equipment rooms unless these devices are required by the equipment installed in such rooms.  All telecommunications rooms are to have a sealed floor, such as sealed concrete or vinyl composition tile.  All walls shall be trimmed out at the bottom with 4 inch vinyl or rubber cove base. No carpeting of any type is allowed in equipment rooms.


Based on square footage served, telecommunications closets shall be minimally sized according to the table below: 




Serving Area Closet Size



Square Feet 




10,000
10 X 15


 8,000    9 x 10


 5,000    7 x 10


For each 10,000 square feet per floor there shall be one telecommunications closet, or where one closet is desirable, the size must be increased accordingly.  Floors with multiple telecom closets should have these closets evenly distributed.


Multi-tenant buildings will require additional telecom closets and possibly additional equipment rooms.  Appendix B addresses additional shared-tenant considerations and is attached.


5.3
Security and access: Equipment rooms and telecommunications closets should be located in such a manner that access and entry can be controlled by office personnel.  All entry doors to equipment or telecom rooms must be of solid-core type construction.  Any hollow or non-solid door is unacceptable.  Electronic card reader access should be installed on equipment and telecommunications access doors and is acceptable as long as restricted access is observed, and only authorized personnel are granted access.  In offices where electronic card readers are not installed, a manual push-button-type locking mechanism can be substituted.  Physical access to the primary telecom room by non-SRS authorized staff is not acceptable.  In the situation where multiple tenants occupy a building, separate rooms for the non-SRS tenants’ equipment(Servers, hubs, phone equipment, etc.) must be provided.


 5.4
AC Power Outlets: 


Utility Outlets:  A minimum of one fourplex 120 VAC 20 Ampere power outlets shall be located every 6 linear feet along each wall, unless there is a good business case not to.  These outlets will be utility outlets and do not need separate 20 ampere circuits, with no more than two (2) fourplex outlets per circuit.



Dedicated Outlets: A minimum of one fourplex 120VAC 20 Ampere power outlets shall be located on each backboard or every 6 linear feet along wall if there is no backboard.  These outlets will be isolated ground, dedicated outlets, with separate circuits, and no more than one fourplex outlet per circuit.


5.5
Wall Space and Layout:  Wall space should be provided that is adequate for termination of cables and equipment with access to the complete riser cable.  Room layout will be designed by SRS Telecom staff and provided to wiring vendor as soon as practical.


5.6
Cross Connect Field:  Termination blocks shall be mounted on 4X8' sheets of 3/4" AC grade plywood.  This plywood should be mounted a minimum of 18 inches above the finished flooring and covering a space up to 8 feet above the finished floor.  A minimum of three walls shall be covered in plywood.  The plywood should be installed with the “A” side out, and sealed by an accepted method, such as painting.  The intermediate distribution frames located in the telecommunications closets consist of plywood-mounted 110 type cross connect blocks that terminate the interframe backbone and the horizontal distribution system.

Intermediate distribution frame blocks should be divided into two sections, with one  section for voice and the other section for LAN.  Interframe backbone blocks will always appear closest to the backbone cable.  Station blocks which terminate the horizontal distribution system wires should appear farthest from the backbone. All in-use blocks should be clearly labeled.  Regardless of the block type used, the number of twists must be maintained all the way to the punch down where mandated.  All station-wire pairs should be connected at the wiring block, so spare or additional pairs can be utilized with minimum effort.  The 66-type connecting block should be installed unless there is valid justification to not to do so, or at direction of SRS Telecom.


Patch cables may be used at some locations and punch down type at other locations depending on need and expertise of personnel that can use patch cables, and frequency of change.  Access clearance for front and sides of backboard shall be a minimum of 3 feet.


5.7
Electrical Breaker Panels:  Electrical breaker panels serving the telecommunications room may be mounted in the telecom room.  Any panel not serving the telecom room must not be located within the controlled space of the telecom room.

5.8
Heating and cooling: All telecommunications closets and equipment rooms must be provided adequate heating and cooling to maintain a constant temperature and humidity level year round.  Temperature should be regulated to maintain 65°-72°.  Humidity should be regulated to maintain 40-60% relative without condensation.  Loading will be determined specific to each office.


6.0
BACKBONE WIRING 


6.1
Riser Design: The riser connects telecommunications closets with the common equipment providing a high capacity riser cable. Single-mode fiber must be used for data(LAN), unless there is valid justification for not doing so. Fiber risers consist of a minimum of 12 strand single-mode fiber optic cable in high rise buildings and in any other buildings where the distance is greater than 300 feet.


Voice riser cabling may consist of multiple-pair cables in one binder as needed for size and capacity.


For locations that could not ever use fiber, UTP riser cable should be sized to accommodate 50 per cent growth over the number of initially installed 8 pair workstations. Even if no fiber is installed initially, the pathways of conduit and duct should allow room for the later addition of fiber.


6.2
Minimum Acceptable cables



   Unshielded Twisted Pair - Category 6a(or current highest standard) Data Grade



   Unshielded Twisted Pair - Category 3 Data Grade


7.0
ENTRANCE FACILITY 


7.1
National Electrical Code Adherence: All telephone communications circuits are to be installed in accordance with Article 800 of the National Electrical Code. Exception: The "Protective Devices" requirements of paragraph 800- 2 are to apply to all outside circuits of any length whether aerial or underground. All arrestors must be solid state type, tested and listed per ANSI/UL 497. They shall be installed on each telephone circuit entering a building as close as practical to the point of entry.


7.2
Protectors:  All protectors shall be grounded using AWG 12 (minimum) copper wire for single line or double line, AWG 10 for three through six lines, and AWG 6 for seven or more lines. This conductor shall be connected to the buildings Grounding Electrode System described by NEC 250- 81 in accordance with NEC 800- 3 1 (b)5. The protector shall equal current existing standards.


7.3
Grounding: The increasing need for the reliable transfer of massive amounts of information creates an environment where electrical protection takes highest priority, The main consideration in developing requirements for grounding, bonding, and electrical protection is safeguarding of personnel, property and equipment from the potential harm from foreign electrical voltages and currents.  A solid bus-bar grounding facility/connection must be installed, and grounding shall be provided by the electrical contractor.  Grounding will be verified by the telecommunications vendor and SRS ITS Telecom staff.


The protection of telecommunications facilities is an essential part of any distribution system.  The National Electrical Code defines grounding and bonding parameters for telecommunications from the aspect of human safety. NEC Articles 250 and 800 cover the general requirements for grounding, bonding, and protecting electrical and telecommunications circuits. NEC requirements are considered the minimum for safeguarding personnel and equipment.


It is the SRS standard that telecommunications systems be isolated to the building ground. Neutral ground current problems are so severe in some modern buildings that telecommunications systems fail to work. Equipment manufacturers grounding and bonding instructions must be closely adhered to. 


Multi-line cable with separate shield is to be grounded per section 7.2 above, where it enters any building, but by separate conductor. The cable shield is to be removed for a length of at least 12 inches on the equipment side of this ground connection, or non- shielded cable used from this point to the equipment.


The telecommunications equipment is to be Single Point Grounded(SPG).   This single point ground consists of bonding together, at one point, the station equipment grounding connection, the green power wire, the inside cable shield (if any), and the station protector grounding conductors (if the protectors are co- located with the equipment). Where the protectors are not co- located with the equipment, a "couple bond conductor" of #10 AWG copper is to be run from the SPG along the incoming cable to the station protector grounding terminal.


7.4
Surge Protectors: The AC power circuit feeding the electronic station must be provided with a surge protector. No other equipment should be connected to this circuit. 


7.5
Sneak Current Fuses: Certain station equipment (usually with circuits of 100 OHM or less impedance to ground) may require "Sneak Current Fuses" to prevent equipment failure, line hazard, and danger to personnel.


7.6
Entrance Conduit 


Sizes: Entrance conduit size will vary with number of lines entering building, but the absolute minimum is two 2 inch conduits. Buildings larger than 10,000 square feet shall have at least three 4 inch conduits. Riser sleeves or conduit will be at least three inches. (Provisions may be made for non-continuous sleeves for riser rather than conduit). Conduit for horizontal service from floor equipment rooms to jack locations shall be 1 inch or greater. Planned capacity should be for 100% redundancy. 


Entrance conduit must extend from backboard beyond any paved areas.



Excluded Locations


Elevator shafts shall be excluded for possible locations of all such conduit.


7.7
Innerduct


A sleeved physical channel shall be provided for fiber optic cable. This is to be within the conduit system, unless the "inner duct" is plenum rated. The innerduct shall contain a pull string, in addition to whatever fiber is pulled at the time of the installation of the duct. 

8.0
CAMPUS DESIGN 


This section is intended as a typical campus distribution structure. This method of distribution occurs usually on hospital or college campuses, but should be used as a guide when  interconnecting multiple buildings wherever a number of buildings are functionally collocated with property right of ways. 


Multi-building campus example: The local telephone company enters Building I and terminates connections on plywood-mounted 110-type cross connect blocks in the Entrance Facility. This is the demarcation point and the owner/agency is responsible for wiring beyond this.  The Main Cross connect  is the focal point for interbuilding communications. There is one Main Cross connect where telephone company and outside facility cabling is terminated. Cables are then distributed to other floors and/or to other buildings. The Main Cross connect should be centrally located.  A campus distribution system can be viewed as a common communications network, but each building should be treated individually for basic wiring considerations of:


Bonding 


Grounding 


Electrical Protection 


Building codes and regulations


Fire stopping as required by local, state or federal codes


Interbuilding cables should consist of single 25 pair Level 3 UTP cables, or multiple-binder Level 3 UTP cables, and not less than 12-strand optical single-mode fibers. Fiber cables should be in inner duct inside conduit.


9.0
HANDICAP AND OTHER SPECIAL REQUIREMENTS


The Americans With Disabilities Act (ADA) (36CFR Part II 9 1) shall be complied with. This act outlines specific requirements for text control telephones and volume control telephones be provided along with signage wherever banks of pay phones are installed. It also details mounting heights and clearances for telephones.


9.1
Handicap Requirements 


All "banks" of public telephones should have at least one telephone which can be used by physically disabled, including those in wheel- chairs and those with hearing and sight disabilities, The following are minimum requirements: 


· The dial and headset shall be placed no more than 4 feet above the floor. 


· The telephone should be equipped for those with hearing disabilities with an adjustable volume control for the headset with instructions for use. 


· The telephone shall be equipped for those with sight disabilities with visual and tactile instructions for use. Large tactile letters shall be used for instructions. 


· On every floor where telephones are installed, at least one should be placed so that the dial and headset are no more than 4 feet above the floor, and equipped for those with hearing and sight disabilities and so identified with visual and tactile instructions for use. 


Controls and operating mechanisms shall be operable by a force of five pounds or less; operation shall not require the use of a firm grip, tight pinching motion, or a turning- twisting motion for activation.


9.2
Elevator Requirements

9.2.1
Elevator Telephone: A single line wall telephone set shall be installed in each elevator in a telephone box supplied by the elevator company.  This phone shall be provided by the elevator vendor and installed accordingly.


9.2.2
Elevator Wiring: The telephone for each elevator shall be wired so it is independent of the telephone system in the rest of the building. Connection of this telephone will be dependant upon local, state or federal standards.  In the absence of these standards, SRS will determine this connection. 


9.2.3
Dial Tone: The telephone system in each elevator will have dial tone or function as outlined in section 9.2.2  in order to pass inspection. 


9.2.4
Elevator Conduit: A one- half inch conduit should be placed between the elevator control room and the nearest telephone closet.


9.3
Code Compliance 


All wiring will comply with Article 800 of the National Electrical Code and the American National Standards Institute NESC (National Electric Safety Code) and will be subject to acceptance tests as described in FCC Rules and Regulations, Title 47, Section 28.215, Chapter 1, Part 68. The primary application of these guidelines for communications is directed to (a)protective devices and methods for "exposed" cable and wiring, (b)separation of power circuits, and (c)fire stopping and special fire resistant and low-smoke producing cable in specified environments. As such all new cable and wire installed in air plenums and ducts shall be flame resistant and have low smoke properties in accordance with Article 800-3(d) of the 1990 National Electrical Code and shall be so classified by Underwriters Laboratories, Inc. All cable installed in steam tunnels must be able to withstand temperatures of 125 degrees centigrade and be jelly-filled(or acceptable substance) for moisture-repellence.


10.0
ADMINISTRATION

10.1
General Rules


ANSI/EIA/TIA 606 Administration Standard for the Telecommunications Infrastructure of Commercial Buildings is incorporated by reference and is to be compiled with.


Each pathway (conduit, tray, raceway, etc.) that conveys telecommunications media from space to space must be given a unique identifier and labeled at each end-point.


Each telecommunications space (equipment room, telecommunications closet, work area, entrance facility, manhole and handhole) must be uniquely identified and labeled.


Each cable must be uniquely identified and labeled at each end.


Each cable record must indicate the cable type by manufacturer and manufacturer's designation, and document every pair/conductor in the cable. Cable identifier must be linked to all pathways in which it runs.


Each piece of termination hardware such as a patch panel or wiring block must be uniquely named and labeled.  Termination position on cross-connect must be identified by type, the pair/conductor terminated and a user code.


In multi-tenant buildings, all guidelines must be observed as noted.  Additional labeling or designations may be required.


10.2
Labeling


Each work area is labeled with a unique identifying number. A consistent labeling and numbering scheme shall be used. The labeling shall be clearly legible on the outlet face and the termination end, The numbering plan should identify the source and destination of the cable for horizontal runs. A sample numbering plan is:



1-1B-110-KF132


Where “1" is the floor, 1B is the telecommunications closet room, 110 is the specific room on the floor, KF132 is  the work space of the user in room 110.  In offices where there is only one telecommunications closet per floor, the “1B” portion can be deleted.  Where a building is a single story, the first “1" could be eliminated.

Horizontal cable shall be labeled at the workstation end and the cross-connect end. Backbone cables (whether riser or horizontal) shall have an identifying number that is labeled at each end. Labels shall be the same color on each end. Performance documentation must use the same labeling scheme. 


10.3
Cable Tracking


To support future expansion, reconfiguration and maintenance, complete records of all system characteristics should be developed and maintained. On each element in the route, identification labels should be completed and attached. Labels should meet the requirements of SRS standard for marking and labeling Systems. A Final Report should record system configuration, unique identifier, fiber labels, pathways and "as built" details. Loss measurements and OTDR traces should also be included with the records. Testing records can be furnished on diskette, but a paper copy should also be created and left on the jobsite.  As a part of any cable installation, records of the connections are required. Changes to wiring should be maintained and accurate records available at all times. A physical inventory should be performed on a periodic basis.


Tracking can be done manually, with a computer based system or both. It is recommended that any installation having 350 or more devices (telephones, PCs, terminals, printers, LAN devices, plotters, etc.) pursue a computer based system. There are reasonably priced systems available that can be implemented compliant to the standard this document requires.


For major renovations or extensive additions, records are required. Existing buildings can be added to as  moves, adds and changes are done to the building. Work orders for wiring changes should be retained with other records for backup and research reasons.


10.4
Color Coding


Color coding should follow established industry standards.


10.5
Records


Records of the installation shall be provided in an as-built format by the wiring vendor.  One copy should be left on-site, one copy provided to the local area office contact, and the third provided to SRS Telecom staff for future reference.  These documents will also be used to verify that wiring was installed as requested.


11.0
TESTING 


11.1
Required Wiring Plant Testing 


All cable pairs must be tested, including voice, LAN(data) and/or fiber.  All wire/fiber must be tested for the following conditions, where the conditions/testing applies to the specific type of installed product:


1. Polarity


2. Reversal of pairs


3. Wire transpositions 


4. Continuity


5. Opens


6. Shorts 


7. AC & DC foreign voltages


8. NEXT End To End(From Faceplate Through 110 connecting block and/or patch panel and jumper)


9. EIA/TIA 568B wiring discrepancies 

10. Attenuation


11.Return Loss


12. ELFEXT


13. Delay and Delay Skew


14. Must Pass TIA/EIA TSB-155 limits

All test data will be documented and provided to the using agency at the time of acceptance, and can be furnished in diskette form and paper form.


11.2
Fiber Optic Testing


System Testing 


Upon completion of the passive optical cable system, the system must be tested to ensure compliance with the design and link loss specifications. The tests must be done end-to-end, LIU to LIU, with all connectors in place, and include: 


Power meter tests - For building risers, power meter tests are required. Disregard OTDR testing for runs less than 2 km. 


End-to-End Attenuation Testing - completed on each fiber span at operational wavelengths.  Testing in one direction is required. Test results should be retained for inclusion into the documentation package. 


Connector loss readings of each completed connector should be recorded using an OTDR at operational wavelengths in one direction. 


Optical Time Domain Reflectometer (OTDR) Signature Traces of each terminated fiber should be recorded at operational wavelengths  for fiber continuity purposes. OTDR testing is mandatory for runs longer than 2 KM. 


A Final Report should be compiled which records system configuration, fiber labels, cable routes and "as built" details. Loss measurements and OTDR traces should also be included.

GLOSSARY 


ADMINISTRATION - The process of documenting the initial wiring and managing the wiring system after the initial installation. It includes two major components: a standard labeling system and a records system. 


AMERICAN WIRE GAGE (AWG) - An American industrial standard; AWG#22 is a 0.64 millimeter (0.0253 inches) diameter solid conductor and AWG#24 is 0.5 (0.0201 inches). 


BUILDING MAIN DISTRIBUTION FRAME (MDF) - The interface between the public network and/or the interbuilding backbone, and the interframe backbone. 


ENTRANCE FACILITY (EF) - Facility where outside circuits/wiring enter a building through weatherproof sleeves and are terminated on blocks providing electronic protection to guard against damage from electrical disturbances such as lightning. In a single building, this is the point of demarcation between the serving telephone utility and the user.


EQUIPMENT ROOM - An area within a building where major components of large telecommunications systems (PBXs data switches, communications processors) are housed. Equipment rooms are often distinct from telecommunications closets due to the size and quantity of the equipment they contain. 


HORIZONTAL DISTRIBUTION SYSTEM (HDS) - The wiring that connects the intermediate distribution frame in the telecommunications closet to the telecommunications outlet. Horizontal distribution cabling is commonly run through the space provided by drop- tile ceilings or routed through ducts in floors and walls. 


INTERBUILDING BACKBONE - The transmission facilities that connect the campus/complex main distribution frame to the building main distribution frames of each building in the complex. Includes multiagency metropolitan areas with state right of way. 


INTERFRAME BACKBONE - The transmission facilities that originate from the building main distribution frame and are vertically or horizontally distributed to each intermediate distribution frame in the building. 


INTERMEDIATE CROSS CONNECT - Typically the equipment or method used to link the backbone and horizontal wiring systems. The intermediate cross connect is usually located in a telecommunications closet.


INTERMEDIATE DISTRIBUTION FRAME (IDF) - The cross connect between the interframe backbone (IFB) and the horizontal distribution system (HDS). The IDF may also serve as a connection point for per floor Local Area Networking equipment. The IDF is normally in the telecommunications closet.


MAIN CROSS CONNECT - Typically the equipment used to link the interbuilding and intrabuilding wiring systems. The main cross connect is usually located in the building entrance facility.


MEGAHERTZ (MHz) - Unit of frequency equal to one million cycles per second. 


NETWORK INTERFACE (NI) - Contains the demarcation point between outside networks and the campus/complex or building main distribution frame. Includes carrier test, loop back, and disconnect capability.


NEXT - Near End Cross Talk - Signal distortion caused by the coupling of an outgoing signal at the originating end of a circuit with the incoming signal being received from the other end of the circuit 


PATCH CORD - A length of wire, or fiber cable, with appropriate connectors on each end. A patch cord is used to join telecommunications circuits at a cross-connect point. 


PATHWAY - A raceway, sleeve, or exposed location for the placing of telecommunications cable that links telecommunications spaces together. 


STAR - A network topology in which each telecommunications outlet is connected only to a distribution frame by a point- to- point link and connections between distributions frames are by point- to- point links.


TELECOMMUNICATIONS CLOSET - The space in a building designed to provide a secure, suitable environment for the installation of cable, telecommunications equipment, and termination and administration systems. Telecommunications closets are the point where the backbone and horizontal distribution facilities intersect. They are floor- serving rooms whose function is to terminate and connect the backbone cable system to the horizontal cable system and to house electronics that assist in the distribution of information to that floor. 


TELECOMMUNICATIONS INFRASTRUCTURE - The components (telecommunications spaces, cable pathways, grounding, wiring and termination hardware) that together provide the basic support for the distribution of all telecommunications information. 


TELECOMMUNICATIONS MAIN GROUNDING BAR (TMGB) - Primary grounding for the entire telecommunications in a building or structure. 


TELECOMMUNICATIONS GROUNDING BAR (TGB) - Auxiliary grounding for the telecommunications in a satellite telecommunications closet and tying into the telecommunications main grounding bar. 


UNSHIELDED TWISTED PAIR - (UTP) wiring consisting of two insulated wire twisted around each other to reduce induction, this interference, from one wire to the other. Twisted pair wire comes in bundles with varying numbers of pairs of wires, from two pair (four wires) to many thousands of pairs. UTP wiring is used to wire telephone networks within buildings because it is inexpensive and relatively easy to install.


TELECOMMUNICATIONS OUTLET (TO) - The interface between the building network (horizontal distribution system) and the work area connection to the user's equipment (phone and/or terminal device). 


WORK AREA CONNECTION - The interface between the outlet and the user/terminal equipment. Includes media adapters, such as baluns. 


EIA/TIA 568B Pin Wiring Standard


4-Pair Wiring Color Codes 


Pair I
Tip

 White/Blue

Ring
 Blue/White 


Pair 2
Tip

 White/Orange

Ring 
Orange/White 


Pair 3
Tip

 White/Green

Ring 
Green/White 


Pair 4
Tip

 White/Brown

Ring 
Brown/White

APPENDIX A: 


Recommended Cable Specifications 


This guideline recognizes the following type cables: 


Fiber optic Single-mode Riser, Inter-building applications, and horizontal pathways planned Fiber optic single mode - Inter-building applications 


Unshielded Twisted Pair (UTP) - Level 3 & 6a (EIA/TIA TSB36)-Horizontal Distribution Copper Data Cable Levels 


The standards recognizing the data handling characteristics of all twisted pair cable and connectors are the EIA/TIA TSB36 and TSB40. Although other levels are specified in these two standards, this guideline standardizes on Category 6a for all data and Category 3 for all voice telecommunications UTP wiring. Level 6a cable is intended for high speed LANS. 


Singlemode Fiber Specification 

The singlemode cable shall meet the EIA/TIS-492CAAA, "Detail Specification for Class IVa Dispersion Unshifted Single Mode Optical Fiber Cable. and ITU-T G.652 "Characteristics of Singlemode Optical Fiber Cable 
  
Fiber type: Singlemode 
  
Coating Diameter: 250 Microns Core Eccentricity: 7.5% maximum (1.5% typical) Numerical aperture: 275 plus or minus .0 15 
  
Attenuation: 1.0 dB/KM @ 1310 NM & 0.75 dB/KM @ 1550 NM 

Bandwidth:  N/A 

Distance:  Serial Gigabit Ethernet=5000M @1310 NM, Serial 10 Gigabit Ethernet =10,000M @1300 NM for 10GBase-LX4, 10,000M@ 1310NM for 10GBase-L & 40,000M@1550 NM for the 10Gbase-E 

Maximum Dispersion :  Less than 3.2 PS/NM*KM @ 1310 NM and less than 18 PS/(NM*KM )@ 1550NM 
  
Fiber connectors: ST (straight through) tyW - .4 dB plus or minus .2 dB loss maximum Single Mode Fiber Specifications 
  
Fiber type 8 Micron Cladding diameter 125 Micron 
  
Attenuation.5 dB/KM @ 850 NM.5 dB/KM @ 1350 NM 
  
Zero dispersion wavelength 1300-1320 NM 
  
UL rating of OFNR for riser usage OFNP for Plenum usage 
  
Cable bend radius 20 X the cable diameter during installation 


APPENDIX B: 


Additional Shared Space Considerations


Physical access to the Telecom room is limited to SRS employees only unless individually secured areas within the common room are provided.


Patch panels, telephone equipment, connections, etc., for each tenant should be in a secure area for each group, not in a single room or rack where access to other tenant’s equipment would be possible.
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Americans with Disabilities Act (ADA) Accessibility Guidelines for Buildings and Facilities; Final Guidelines (July 1991) 36 CFR Part 1191 


Commercial Building Telecommunications Wiring Standard (July 1991) ANSI/EIA/TIA-568 


Commercial Building Standard for Telecommunications Pathways and Spaces (October 1990) ANSI/EIA/TIA-569 


Administration Standard for the Telecommunications Infrastructure of Commercial Buildings(February 1993) ANSI/EIA/TIA-606 


Technical Systems Bulletin Additional Cable Specifications for Unshielded Twisted Pair Cables (November 1991) ANSI/EIA/TIA/TSB-36 


Technical Systems Bulletin Additional Transmission Specifications for Unshielded Twisted Pair Connecting Hardware (August 1992) ANSI/EIA/TIA/ TSB-40 


Detail Specification for 62.5-m Core Diameter/125-m Class la Multimode Graded Index Optical Waveguide Fibers (July 1991) ANSI/EIA/TIA492AAAA 


Generic Requirements for Optical Fiber and Optical Fiber Cable (February 1989) Bellcore TR-TSY-000020 National Electrical Code Article 700, 725, 800 


Telecommunications Architectural Standards (July 1990) Department of Information Sciences, State of Washington Telecommunications Wiring For General Office and Administrative Space (March 1991) Council on Information 


Management and Department of Information Technology, Commonwealth of Virginia 


Telecommunications Distribution Methods Manual (1991) BICSI


Information Technology Systems, State of North Carolina
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Surplus Property Exhibit A & B.xls
Surplus Property Exh. A

		Exhibit A - Vendor's Estimated Cost Worksheet

		Kansas Department of Administration - Surplus Property

														Column A		Column B		Column C

		VENDOR:								Useable SQ. FT.				Total Cost w/ Add Alts		Total Cost per Useable Sq. Ft.		Total Cost w/o       Add Alts

		Proposed Address:

		Estimated Construction or Renovation Costs:

		Initial Upfront Costs												$   - 0		$   - 0		$   - 0

		1                                      NOT APPLICABLE														$   - 0

		2                       NO COSTS WILL BE PAID UP FRONT												$   - 0		$   - 0

		Foundations														$   - 0		$   - 0

		(Footings & Foundations, Excavation & Backfill)

		Substructure														$   - 0		$   - 0

		(Slab on Grade, Special Substructures)

		Superstructures														$   - 0		$   - 0

		(Columns; Beams; Joists; Roof Deck; Structural Walls;

		Elevated Floors; Stairs, etc.)

		Exterior Closure														$   - 0		$   - 0

		(Walls, Exterior, Brick, Doors, Windows & Glazed Walls)

		Roofing														$   - 0		$   - 0

		(Roof Coverings, Roof Deck Insulation, Openings, etc.)

		Interior Construction														$   - 0		$   - 0

		(Partitions, Interior Doors, Wall, Floor & Ceiling Finishes, Interior

		Surface of Exterior)

		Conveying Systems														$   - 0		$   - 0

		(Elevators, Other)

		Mechanical														$   - 0		$   - 0

		(Plumbing, Fire Protection, Heating, Cooling)

		Electrical														$   - 0		$   - 0

		(Service & Distribution, Lighting & Power, etc.)

		Site Work														$   - 0		$   - 0

		(Earthwork, Utilities, Roads & Parking, Site Improvements,

		Landscaping, Demolition)

		Specialty items or features unique to this RFP                                            (Agency reserves the right to choose to include or exclude during the negotiation and award process).                                                                 The Costs for these items should not appear in Column C.												$   - 0		$   - 0		N/A

		1  Access Management System												$   - 0		$   - 0

		2												$   - 0		$   - 0

		3												$   - 0		$   - 0

		4												$   - 0		$   - 0

		5												$   - 0		$   - 0

		6												$   - 0		$   - 0

		7												$   - 0		$   - 0

		Architectural/Engineering Services														$   - 0

		General Conditions (Overhead & Profit)														$   - 0

		TOTAL BUILDING COST:												$   - 0		$   - 0		$   - 0

		Land and Building Shell Costs:														$   - 0

		Financing Costs:														$   - 0

		TOTAL PROJECT COST:												$   - 0		$   - 0		$   - 0

																		$   - 0





Surplus Property Exh. B

		Exhibit B - Vendor's Proposed Lease Cost Submission Form

		Kansas Department of Administration - Surplus Property

		PROPOSAL SUBMITTED BY:

		GENERAL INFORMATION

		Agency		DofA, Surplus Property

		Proposed Address		='Exhibit B'!C5

		City Location (market)		Topeka, KS

		Lease Space (sq. ft.)		0

		Lease Term (in years, months)

				COST PROPOSAL

				PROPOSED LEASE RATES

				With Add Alternates										Without Add Alternates

				Cost/SF/Year		Cost/Year		1.3 M						Cost/SF/Year		Cost/Year

		LEASE COSTS - provided by 1st Party Landlord within the lease										$0.00

		Base Lease Cost				$0		$10.17		-$4,423,950.00		$0.00				$0

		Storage				$0		$0.00								$0

		Real Estate Taxes				$0		$1.78				$0.00				$0

		Insurance				$0		$0.24				$0.00				$0

		Major Maintenance				$0		$0.30				$0.00				$0

		Utilities - total				$0		not inc.								$0

		Electricity				$0		not inc.								$0

		Gas				$0		not inc.								$0

		Water/Sewer/etc.				$0		not inc.								$0

		Custodial/Janitorial				$0		$0.61				$0.00				$0

		Trash Pickup/Removal				$0		$0.13				$0.00				$0

		Pest Control				$0		$0.00								$0

		Snow Removal				$0										$0

		Grounds Maintenance				$0		$0.27				$0.00				$0

		Common Area				$0		$0.00								$0

		Additional Services (Please list below)

		1				$0		$0.45				$0.00				$0

		2				$0		$0.45				$0.00				$0

		SUBTOTAL - Lease Costs		$0.00		$0		$13.95				$0.00		$0.00		$0

												$43,500.00

		OTHER BUILDING OCCUPANCY COSTS - funded separate from the lease

		Building Operating Cost (not included in base rent)

		Utilities - total (estimated)

		Electricity				$0										$0

		Gas				$0										$0

		Water/Sewer/etc.				$0										$0

		Custodial/Janitorial				$0										$0

		Trash Pickup/Removal				$0										$0

		Pest Control				$0										$0

		Snow Removal				$0										$0

		Grounds Maintenance				$0										$0

		Security				$0										$0

		Total Other Bldg Optg Costs (not included in lease)		$0.00		$0		$2.85						$0.00		$0

		IMPROVEMENTS

		Improvements		$0.00		$0								$0.00		$0

		Subtotal - Improvements		$0.00		$0								$0.00		$0

										10000

		Total Annual Cost of Occupancy (per sq. ft.)(est.)		$0.00		$0				$20,000.00				$0.00		$0

		Total Cost of Lease (estimated)		-		$0				$30,000				-		$0

		Comments



&L&8&Z&F




image5.emf
DFM Grounds  A&B.xls


DFM Grounds A&B.xls
Exhibit A DFM - Grounds

		Exhibit A - Vendor's Estimated Cost Worksheet

										Division of Facilities Management - Grounds Department

														Column A		Column B		Column C

		VENDOR:								Useable SQ. FT.				Total Cost w/ Add Alts		Total Cost per Useable Sq. Ft.		Total Cost w/o       Add Alts

		Proposed Address:

		Estimated Construction or Renovation Costs:

		Initial Upfront Costs (Project costs to be paid upfront by the Lessee and not financed through the proposed lease)												$   - 0		$   - 0		$   - 0

		1														$   - 0

		2												$   - 0		$   - 0

		3												$   - 0		$   - 0

		4												$   - 0		$   - 0

		5												$   - 0		$   - 0

		6												$   - 0		$   - 0

		7												$   - 0		$   - 0

		8												$   - 0		$   - 0

		Foundations														$   - 0		$   - 0

		(Footings & Foundations, Excavation & Backfill)

		Substructure														$   - 0		$   - 0

		(Slab on Grade, Special Substructures)

		Superstructures														$   - 0		$   - 0

		(Columns; Beams; Joists; Roof Deck; Structural Walls;

		Elevated Floors; Stairs, etc.)

		Exterior Closure														$   - 0		$   - 0

		(Walls, Exterior, Brick, Doors, Windows & Glazed Walls)

		Roofing														$   - 0		$   - 0

		(Roof Coverings, Roof Deck Insulation, Openings, etc.)

		Interior Construction														$   - 0		$   - 0

		(Partitions, Interior Doors, Wall, Floor & Ceiling Finishes, Interior

		Surface of Exterior)

		Conveying Systems														$   - 0		$   - 0

		(Elevators, Other)

		Mechanical														$   - 0		$   - 0

		(Plumbing, Fire Protection, Heating, Cooling)

		Electrical														$   - 0		$   - 0

		(Service & Distribution, Lighting & Power, etc.)

		Site Work														$   - 0		$   - 0

		(Earthwork, Utilities, Roads & Parking, Site Improvements,

		Landscaping, Demolition)

		Specialty Items or Features Unique to this RFP (These are Agency Requested Add Alternates and may be removed).  The Costs for these items should not appear in Column C.												$   - 0		$   - 0		N/A

		1														$   - 0

		2												$   - 0		$   - 0

		3												$   - 0		$   - 0

		4												$   - 0		$   - 0

		5												$   - 0		$   - 0

		6												$   - 0		$   - 0

		7												$   - 0		$   - 0

		Architectural/Engineering Services														$   - 0

		General Conditions (Overhead & Profit)														$   - 0

		TOTAL BUILDING COST:												$   - 0		$   - 0		$   - 0

		Land and Building Shell Costs:														$   - 0

		Financing Costs:														$   - 0

		TOTAL PROJECT COST:												$   - 0		$   - 0		$   - 0

																		$   - 0





Exhibit B DFM - Grounds

		Exhibit B - Vendor's Proposed Lease Cost Submission Form

		Division of Facilities Management - Grounds Department

		PROPOSAL SUBMITTED BY:

		GENERAL INFORMATION

		Agency

		Proposed Address		='Exhibit B'!C5

		City Location (market)

		Lease Space (sq. ft.)		0

		Full Time Equivalency (FTE) employees

		Lease Begin Date (initial lease period)

		Lease End Date (initial lease period)

		Lease Term (in years, months)

				COST PROPOSAL

				PROPOSED LEASE RATES

				With Add Alternates										Without Add Alternates

				Cost/SF/Year		Cost/Year		1.3 M						Cost/SF/Year		Cost/Year

		LEASE COSTS - provided by 1st Party Landlord within the lease										$0.00

		Base Lease Cost				$0		$10.17		-$4,423,950.00		$0.00				$0

		Storage				$0		$0.00								$0

		Real Estate Taxes				$0		$1.78				$0.00				$0

		Insurance				$0		$0.24				$0.00				$0

		Major Maintenance				$0		$0.30				$0.00				$0

		Utilities - total				$0		not inc.								$0

		Electricity				$0		not inc.								$0

		Gas				$0		not inc.								$0

		Water/Sewer/etc.				$0		not inc.								$0

		Custodial/Janitorial				$0		$0.61				$0.00				$0

		Trash Pickup/Removal				$0		$0.13				$0.00				$0

		Pest Control				$0		$0.00								$0

		Snow Removal				$0										$0

		Grounds Maintenance				$0		$0.27				$0.00				$0

		Common Area				$0		$0.00								$0

		Additional Services (Please list below)

		1				$0		$0.45				$0.00				$0

		2				$0		$0.45				$0.00				$0

		SUBTOTAL - Lease Costs		$0.00		$0		$13.95				$0.00		$0.00		$0

												$43,500.00

		OTHER BUILDING OCCUPANCY COSTS - funded separate from the lease

		Building Operating Cost (not included in base rent)

		Utilities - total (estimated)

		Electricity				$0										$0

		Gas				$0										$0

		Water/Sewer/etc.				$0										$0

		Custodial/Janitorial				$0										$0

		Trash Pickup/Removal				$0										$0

		Pest Control				$0										$0

		Snow Removal				$0										$0

		Grounds Maintenance				$0										$0

		Security				$0										$0

		Total Other Bldg Optg Costs (not included in lease)		$0.00		$0		$2.85						$0.00		$0

		IMPROVEMENTS

		Improvements - Funded with upfront payment by Lessee		$0.00		$0								$0.00		$0

		Subtotal - Improvements		$0.00		$0								$0.00		$0

										10000

		Total Annual Cost of Occupancy (per sq. ft.)(est.)		$0.00		$0				$20,000.00				$0.00		$0

		Total Cost of Lease (estimated)		-		$0				$30,000				-		$0

		Comments
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