REQUEST FOR QUALIFICATIONS SAN ANTONIO RIVER

AUTHORITY SAN ANTONIO TEXAS

Project Title: Lake Medina Dam Modifications 

Project Description The San Antonio River Authority acting as project manager and contract administrator for the Bexar-Medina-Atascosa Counties Water Control and Improvement District No. 1 owner and operator of Lake Medina Dam is soliciting the submittal of qualifications from firms to provide complete construction services to correct dam stability and erosion protection deficiencies for Lake Medina Dam located in Medina County Texas. Scope of Work Construction to correct the identified deficiencies consists of two planned improvements. The first is installation of 32 Post-Tensioned Dam Anchors of approximately 50 strands each with an average depth of 117 feet installed on the crest of the dam. It is expected that this work will require at a minimum: concrete demolition bracing and shoring as needed drilling water pressure tests installation of steel strands and bearing plates a performance and proof test lock off structural concrete and grout. The second planned improvement is approximately 2,300 cubic yards of reinforced structural concrete and 1,000 cubic yards of backfill concrete for erosion protection installed at the downstream toe of the dam on the right and left abutments. It is expected that this work will require at a minimum: clearing and grubbing earthwork steel concrete passive anchors reinforcing steel forming placing and finishing concrete and grout. 

Qualifications Due Date and Time: March 30 2010 5 p.m. Mountain Time Address: URS Corporation 8181 E. Tufts Ave. Denver CO 80237 Attention: Chad Gillan P.E. Interested construction firms may obtain the SOQ documents by contacting: Chad Gillan P.E. URS Corporation 8181 E. Tufts Ave. Denver CO 80237 Direct: (303) 740 3884 Chad_Gillan@ urscorp.com
