Vendor Bid Proposal 
Specifications for Diesel 35 Passenger Type C School Bus

Chicago Metropolitan Region 

Due Date: August 20, 2010

General Instructions

1. The following Bid shall meet or exceed (1) Federal Motor Vehicle Safety Standards. (2) Criteria for Illinois State School Bus Specifications (3) 2007 Engine Requirements. 

2. Selected vendor must agree to correct faulty work or materials promptly and without cost to Cook Illinois Corporation. 

3. Must complete bid specification. 

4. Vendor must indicate total vehicle cost and total cost for all vehicles. 

5. Vendor may submit alternate bids 
6. Submit bids in PDF format to info@cleanaircounts.org 

7. The Metropolitan Mayors Caucus reserves the right to not award the bid. 

Please provide all requested information below: 
	Model Vehicle 2011
	VENDOR BID PROPOSAL

Specifications for Gas/Diesel, 35–77 Passenger

Type C School Bus
	For Vendor Use Only

	
	
	 FORMCHECKBOX 

This bid meets all district requirements as specified.

 FORMCHECKBOX 

This bid is an alternate to district requirements as specified.


Metropolitan Mayors Caucus/ Clean Air Counts Campaign/ 177 N State Street Suite # 500, Chicago IL 60601 info@cleanaircounts.org 
GENERAL INSTRUCTIONS

1. The following bid shall meet or exceed (1) Federal Motor Vehicle Safety Standards; (2) Illinois State Vehicle Requirements; and (3) 2007 Engine Emissions Requirements.

2. Delivery shall be considered complete when buses have been (1) Cook Illinois Corporation for inspection (2) are accepted as meeting bid specifications and district requirements by a duly authorized school district representative.

3. The basic bid specifications under the item and state-supported specifications columns are not to be altered in any way.

VENDOR INSTRUCTIONS

4. The selected vendor must agree to correct any faulty work or materials promptly and without cost to the school district.

5. The vendor must complete all information as requested on basic bid specifications and official bid summary and vehicle data.

6. The vendor must indicate two sets of costs figures on page 12.

a. A total vehicle base cost figure related only to the basic bid specifications (pages 2–6).

b. An adjusted total vehicle cost figure reflecting all deductions from, and/or additions to the base cost results from school district requirements or vendor alternates.

c. The total vehicle base cost or the total adjusted cost shall not reflect any allowance for trade-in.

7. The vendor may submit alternate bids, in which case, Items 1–3, 7, and 10–12 are to be followed.

	Vendor’s Company Name and Address

     
Telephone Number:
	CHASSIS

Make      

Model      


	BODY

Make      

Model      



Vendor:      

	
	Basic Bid Specifications

TYPE C—GAS/DIESEL

35–77 PASSENGER


	

	
	
	


	
	CHASSIS
	

	ITEM
	STATE-SUPPORTED SPECIFICATIONS

Vendor must meet or exceed these specifications.

Item bid shall be specified in column to right.
	VENDOR:  SPECIFICALLY IDENTIFY ITEM BID

	Maximum Design Capacity

 FORMCHECKBOX 

35





	As indicated in item column.
	Capacity      


	Engine

 FORMCHECKBOX 
 Diesel
Alternate Fuel:


 FORMCHECKBOX 
 B11
	
	Fuel type:   FORMCHECKBOX 
 Diesel
 FORMCHECKBOX 
 CNG


 FORMCHECKBOX 

LPG
 FORMCHECKBOX 
 B11

	
	
	Engine Mfr.      

Model or liters      


	
35-41 passenger
	175 H.P. minimum.
	Net torque      

@
     

R.P.M.

	Transmission


 FORMCHECKBOX 

Automatic


35-53 passenger
	Allison, PTS 2500 or equal.
	Mfr.      


	
	
	Model no.      



Vendor:      

	
	
	Basic Bid Specifications

TYPE C—GAS/DIESEL

35–77 PASSENGER


	

	
	
	
	


	
	CHASSIS
	

	ITEM
	STATE-SUPPORTED SPECIFICATIONS

Vendor must meet or exceed these specifications.

Item bid shall be specified in column to right.
	VENDOR:  SPECIFICALLY IDENTIFY ITEM BID

	Axles

Diesel Front

35-47 passenger
	7,000 lb. minimum.
	

	
	
	Mfr.      


	
	
	Capacity      


	
	
	

	Diesel Rear


35-47 passenger
	15,000 lb. minimum.
	Mfr.      


	
	
	Capacity      


	
	
	

	Axle Oil Seals
	Front and rear oil bath.
	Mfr.      


	Axle Ratio
	Must comply with power and gradeability formula.  Refer to Washington State School Bus Specifications Manual.
	Ratio      


	Alternator
	185 amp minimum with or without lift-equipped vehicle.
	Mfr.      


	
	
	Max. amps output w/o lift       

w/lift
     


	Battery(ies)
	
	Size or group      


	

	1200 CCA 12 volt to be mounted in body battery compartment.
	Number of batteries      


	
	1400 CCA 12 volt if lift-equipped vehicle is specified.  Mounted in body battery compartment.
	CCA      



Vendor:      

	
	
	Basic Bid Specifications

TYPE C—GAS/DIESEL

35–77 PASSENGER


	

	
	
	
	


	
	CHASSIS
	

	ITEM
	STATE-SUPPORTED SPECIFICATIONS

Vendor must meet or exceed these specifications.

Item bid shall be specified in column to right.
	VENDOR:  SPECIFICALLY IDENTIFY ITEM BID

	Brakes


35-47 passenger
	Hydraulic:  Drum or disc.  Refer to Washington State School Bus Specifications Manual.
	
 FORMCHECKBOX 

Hydraulic
 FORMCHECKBOX 

Air

Disc:
 FORMCHECKBOX 

Front
 FORMCHECKBOX 

Rear

Drum:
 FORMCHECKBOX 

Front
 FORMCHECKBOX 

Rear



	Engine Heater
	Engine manufacturer’s recommended in-block heater.
	Watts      

Volts      


	
	
	Mfr.      


	Engine Temperature
	To be controlled electronically, by fan clutch/drive, or shutters.
	Mfr.      

Electronic
 FORMCHECKBOX 

Fan clutch
 FORMCHECKBOX 


Shutters
 FORMCHECKBOX 


	Fuel Tank


35-41 passenger
	30 gallon minimum.
	Capacity      


	Hood
	Tilt.
	 FORMCHECKBOX 

Fiberglass

 FORMCHECKBOX 

Metal

	Tires
	7 first quality, radial ply tires.  (Tires must be equal to first-line tires manufactured by the five major U.S. tire companies.) 
	Mfr.      


	
	
	Size      


	
	
	Load range      



	Wheels
	7 to be compatible with tire size. 
	Size      


	
	
	Rim width      



Vendor:      

	
	
	Basic Bid Specifications

TYPE C—GAS/DIESEL

35–77 PASSENGER


	

	
	
	
	


	
	BODY
	

	ITEM
	STATE-SUPPORTED SPECIFICATIONS

Vendor must meet or exceed these specifications.

Item bid shall be specified in column to right.
	VENDOR:  SPECIFICALLY IDENTIFY ITEM BID

	Auxiliary Defroster Fans
	2 defroster fans, 6” maximum, mounted to defrost right and left windshield and service door.
	Mfr.      


	Back-up Lights
	All required backup lights to be LED (Light Emitting Diode). 
	Size:
 FORMCHECKBOX 

Square inches
     



 FORMCHECKBOX 

Diameter
     


	Battery Compartment
	Battery storage tray must be large enough to accommodate batteries as specified in chassis section.
	
 FORMCHECKBOX 

Swing out
 FORMCHECKBOX 

Roll out

	Heaters


35-47 passenger



	3 total: 2 front, 1 rear.  Total output must be 195,000 B.T.U. minimum.  Shut-off valves at engine for all heaters.  Two-speed motors.  Recirculating pump for diesel only.
	Left front B.T.U.      


	
	
	Right front B.T.U.      


	
	
	Total B.T.U.      


	P.A. System


35-53 passenger
	AM/FM/PA radio with 2 interior and 1 exterior speakers.
	
 FORMCHECKBOX 

2+1
 FORMCHECKBOX 

4+1

Mfr.      


	Seats
	To permit indicated passenger capacity (page 2 under item column) based on 21” seat spacing from S.R.P.
	Inside measurement from rear of

stepwell to appropriate point at rear of

passenger seating area:       

inches
Manufacturer’s C/C

seat measurement:       

inches




	Steering Wheel
	Tilt.
	Check if as specified
 FORMCHECKBOX 


	Toolbox
	Exterior, manufacturer standard.
	Size (cubic feet)
     


	Two-way Communications
	45-wall, VHF, mil. spec., narrow band/wide band capable.
	Mfr.      


	
	
	Model no.      



Vendor:      

	[image: image1.png]



	VALID

2008-09
ONLY
	Basic Bid Specifications

TYPE C—GAS/DIESEL

35–77 PASSENGER


	

	
	
	
	


	
	ADDITIONAL REQUIREMENTS—CHASSIS AND BODY
	

	ITEM
	STATE-SUPPORTED SPECIFICATIONS

Vendor must meet or exceed these specifications.

Item bid shall be specified in column to right.
	VENDOR:  SPECIFICALLY IDENTIFY ITEM BID

	Line Setting Ticket
	Legible copy of manufacturer’s Line Setting Ticket will be delivered with each vendor’s packet.
	As specified
 FORMCHECKBOX 


	Owner/Operator Handbook

	One copy of the chassis manufacturer’s owner/operator handbook or manual will be furnished with each bus at time of delivery.
	As specified
 FORMCHECKBOX 


	Repair Manuals
	A complete set of chassis, engine, transmission, and body repair manuals, including wiring diagram for all components, will be made available at time of delivery, with instructions available on accessing repair materials.
	As specified
 FORMCHECKBOX 


	Warranty
	A complete copy of all warranty agreements will be furnished at time of delivery.
	As specified
 FORMCHECKBOX 



:

	
	
	OFFICIAL BID SUMMARY

AND VEHICLE DATA

(must include district requirements)
	

	
	
	
	



	
	

	
	 FORMCHECKBOX 
  District requirement
Vendor shall furnish written warranty from chassis and body manufacturer

	REPRESENTATIVE’S SIGNATURE
     
	DATE

     
	 FORMCHECKBOX 
  Vendor alternate
defining areas of responsibility under warranty.

Estimated delivery date to school district:      

Firm where engine and chassis can be

serviced or repaired and parts obtained:      

	

	VENDOR’S COMPANY

     
	
	

	
	Firm where body can be serviced or repaired and parts obtained:      



	BODY

	MAKE
     
	Inside measurement from rear of stepwell 
to appropriate point at rear of passenger 
seating area:      
	C/C seat measurement based on district requirement       inches
	Mobile seating device lift:   FORMCHECKBOX 
  Yes     FORMCHECKBOX 
  No

	MODEL
     
	YEAR
     
	Manufacturer’s C/C seat measurement based on seat spacing 21” from S.R.P.       inches
	Capacity:      


	Warranty:
Years        
Overall vehicle length (inches):  

Miles       
     
	Capacity:      

	Radio
 FORMCHECKBOX 
  Citizen’s band


 FORMCHECKBOX 
  High frequency


	CHASSIS
	TRANSMISSION

	MAKE
     
	Brakes:
 FORMCHECKBOX 
  Hydraulic
Front axle capacity:
     

 FORMCHECKBOX 
  Air
Rear axle capacity:
     
	Make:      


	MODEL
     
	YEAR
     
	
 FORMCHECKBOX 
  Drum
GVWR:
     


 FORMCHECKBOX 
  Disc
Axle ratio:
     

	Model:      


	Warranty:
Years      
Wheel base:       

Miles       
	
 FORMCHECKBOX 
  Dual wheel
2 Speed:
 FORMCHECKBOX 
  Yes
 FORMCHECKBOX 
  No


 FORMCHECKBOX 
  Single wheel
	
 FORMCHECKBOX 
  Auto
 FORMCHECKBOX 
  Manual Speeds forward
     



	ENGINE
	BASE COST

	MAKE
     
	Torque:      

@
     
RPM

H.P.:      

@
     
RPM
	                                       F.O.B.  upon payment


within 30 days after delivery.
$     


	MODEL
     
	YEAR
     
	C.I.D.:      

Fuel type:      

	
Sales tax @      
$     


Total base cost
$     


	Warranty:
Years       

Miles       
Number of cylinders:      
Inline      
V-type       
	Alternator manufacturer: 

     

Max amps:      

Idle amps:      

Battery type/grp:      

Number batteries:      

Total CCA:      

	


