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			                         Request for Proposal (RFP)
Supply, Installation and Commissioning of Salt Refining Plant
for USAID/Partnership for Economic Growth Program 
Hargeisa, Somaliland

	RFP No:
	RFP-Partnership-2013/23

	Title:
	Supply, Installation and Commissioning of 2.5 TPH Salt Refining Plant

	Issuing Office:
	DAI/Partnership for Economic Growth
Head Office: Bada cas, Next to FAO
Kodbur District
Hargeisa, Somaliland 

	Date of Issue of RFP:
	January 30, 2013

	Date Proposal Due:   
	Time:  By 5:00 p.m. local time. Date: February 18, 2013

	Anticipated Type of Award:
	Firm Fixed Price Purchase Order

	Basis of Award:
	Award will be made on the basis of a tradeoff source selection process.  Bidders can bid on one or more components of the RFP, resulting in the award of one or more subcontracts. Award will be made to the offeror whose final offer represents the best value using a combination of cost/price and technical or non-cost/price factors.

	Attachments TO RFP:

All bidders are responsible to carefully review each attachment and follow any instructions that may be relevant to this procurement.
	1. Attachment “A” Instructions
2. Attachment “B” Specifications and SOW (includes Annex 1)
3. Attachment “C” Cover Letter
4. Attachment “D” Proposal Checklist
5. Attachment “E” Bidders company information
6. Attachment “F” Certifications of Compliance
7. Attachment “G” Agreement Terms & Conditions
8. Attachment “H” References and Past Performances

	Technical Specifications:
	USAID/Partnership for Economic Growth program is purchasing a 2.5 TPH salt refining plant on behalf of its grantee, Muliyo Salt Trading Company, in support of the company’s salt processing activities:
Production Process:
1. Unloading of salt into the Raw Salt Hopper either manually or with the help of Tractor trailer. 
2. Reclaiming of salt using a belt conveyor from hopper and discharge on to Roller crusher.  
3. Discharge Material from the crusher to Slurry formation tank from where the slurry passes through Wash Tank, Elutriation Tank and  Thickener for removing impurities like Ca, Mg, Sulphate, insoluble matters etc. 
4. Salt slurry formed in Thickener to be fed into Centrifuge for solid-liquid separation. 
5. Salt with about 3% moisture from to be discharged from centrifuge into screw conveyor and then volumetric cup fillers.
Process Sequence:
1. Crushing 
2. Removal of Insoluble, floating materials by elutriation process.
3. Removal of soluble impurities by washing.
4. Separation of solid and liquid by centrifuging.
5. Iodizing, Packaging in Pouches or sacks.


Attachment “A”
Instructions


DAI invites companies to submit a proposal to provide equipment for a salt refining plant to improve the salt mining of its grantee, Muliyo Salt Trading Company, under the USAID/Partnership for Economic Growth program (USAID Contract # AID-EEM-I-00-07-00009/AID-623-TO-11-00001).


I. Type of Subcontract

DAI anticipates awarding one (1) or more fixed price subcontract(s) as a result of this RFP.  
II. Contract Term

Delivery of goods required within 4 months or less of Purchase Order signing.


III. Submission of Proposals

A proposals must be in English and present costs in USD ($).  Proposals should be emailed to PartnershipProcurement@dai.com by 5 pm local Somaliland time on February 18th, 2013.  The subject of the email must include the title of the RFP.   The proposal must be submitted in one e-mail under separate documents clearly labeled: (1) Technical Proposal and (2) Price Proposal.

IV. Offeror’s Agreement with Terms and Conditions

The completion of all RFP requirements in accordance with the instructions in this RFP and submission to DAI/Partnership of the technical and price proposals will constitute an offer and indicate the Offeror’s agreement to the terms and conditions in this RFP. DAI reserves the right to award one or more subcontract(s) without discussion and/or negotiation; however, DAI also reserves the right to conduct discussions and/or negotiations, which among other things may require an Offeror(s) to revise its proposal (technical and/or price). Issuance of this RFP in no way obligates DAI to award a subcontract, nor does it commit DAI to pay any costs incurred by the Offeror in preparing and submitting the proposal.

V. Source, Origin, and Nationality Requirements

The authorized USAID Geographic Code (see AIDAR 752.225-70 Source, Origin and Nationality Requirements) is 937 for this procurement, which allows for procurement of goods/services from the United States of America, Somaliland, and developing countries other than advanced developing countries (complete list of allowed developing countries available here: http://transition.usaid.gov/policy/ads/300/310maa.pdf). Products may not be produced in or contain any part or ingredient manufactured in Cuba, Iran, North Korea, Sudan, and Syria.  

To be eligible for award under this RFP, a Vendor:
1. Must be incorporated or legally organized under the laws of a country in Code 937;
2. Must be operating as a going concern in a country in Code 937;
3. Must either:
a. Be managed by a governing body, the majority of whom are citizens or lawful permanent residents of countries in Code 937; or,
b. Employ citizens or lawful permanent residents of a country in Code 937.


VI. Composition of Proposal

The proposal is to be comprised of the following submission documents:

	

	Section 1 – Technical Proposal


a. Technical Approach- Offerors must describe the equipment and technical assistance to be provided, including:
a. List of plant machinery to be provided (please specify power (kW) and indicate if specifications differ at all from the list of machinery in Attachment B)
b. Model/manufacturer of machinery parts
c. Information requested under “Additional Information Required” section in Attachment B
d. Description of warranty and  maintenance services
e. Description of technical assistance for installation and verification of the equipment, as well as end-user training.  
f. CV of the proposed technician(s) who will travel to Somaliland.

Please see Attachment B for details on required information for the technical approach.

b. Delivery and Technical Assistance Timeline - Offerors must include a delivery timeline with their proposal that details the anticipated number of days needed for delivery from date of Purchase Order signing, as well as a timeline for the technician to come out to Boroma, Somaliland for installation, verification and end user training.  Please include the recommended number of days the technical will need to be on the ground (see Attachment B).

c. Summary of Relevant Work Experience – Offerors must submit evidence of previous experience with the equipment requested in this RFP, including names of locations where their product has been installed and contacts of their clients using their products as applicable.  Offerors should detail similar work completed with at least three other clients (Appendix I).






	Section 2 – Price Proposal

The Price Proposal must be under separate cover and clearly labeled as such.

a. Detailed Cost Breakdown – Offerers must provide a detailed cost breakdown of prices including:

a. Unit cost per piece of equipment. 
b. Shipping/Delivery
c. Warranty
d.  Maintenance and remote support
e. Technical assistance for installation, verification and training, including daily rate and travel costs (estimate $50 per day per person for lodging and boarding).)
f. Other

This must be submitted in Excel.   Packing/handling charges must be incorporated into the unit price for each line item.  Shipping charges may be shown as a separate line item.

b. Payment Schedule – DAI estimates that the subcontractor will be paid based on deliverables using the following percentage breakdown, or as otherwise negotiated in the Purchase Order. 

	No.
	Description
	Percentage of Cost

	1
	Provision of work-plan including equipment and plant design
	20%

	2
	Delivery of all equipment
	50%

	3
	Installation, verification and end-user training
	30%




VII. Evaluation of Proposals

DAI will use best value determination for the award of this purchase order.  A best value determination means that, in DAI’s estimation, the selected offer will provide the greatest overall benefit to the DAI/Partnership Program in response to the requirements stated in this RFP.  DAI will use the trade-off process to make a best value determination, which means that it may be in the interest of DAI to consider award to other than the lowest priced offeror or other than the highest technically rated offeror. The evaluation factors and allocated points are presented below.   


a. Technical Approach (50 points) – Points for this section will be awarded based on the information presented in the technical approach on the goods and technical assistance to be provided and the responsiveness of the approach to the requirements of this RFP.

b. Relevant Experience (25 points) – Points for this section will be based on information provided in the proposal around the company’s past experience with the work outlined in this RFP, specifically experience supplying its products to Africa and other similar developing countries, as well as availability of technicians on standby who can provide assistance in the English language.   

c. Timeline (25 points) – Points for this section will be based on whether the Offeror understands the activities to be undertaken, the order in which they should occur and timeline by which they should be completed.   This includes number of days for delivery after signing of Purchase Order and number of days for technician to be on the ground.

d. Cost– No points are assigned to the cost proposals evaluation. While the technical evaluation criteria are significantly more important than cost, cost remains important. 

Costs will primarily be evaluated for realism, if it is allowable, and for reasonableness. This will consist of a review of the cost proposal to determine if the overall costs proposed are realistic for the work to be performed, if the costs reflect the offeror understands of the requirements, and if the costs are consistent with the Technical Proposal.

VIII. Requirements for Bids to be Determined to be Responsive

a. The bid must conform to all the technical specifications listed in the SOW in Attachment B. Proposals which do not comply will be determined non-responsive and rejected.  
b. Bidder shall agree to delivery of all equipment listed in Attachment B within 4 months signing of Purchase Order (unless alternative schedule is provided in the Purchase Order). 
c. Vendor must agree to a warranty for defects as specified in Attachment B.
d. Vendor must not be included on the US Government EPLS/SDN blocked persons/organizations list 
e. Vendor must provide a DUNs number (if applicable)






Attachment “B”
Specifications & Statement of Works



I. Introduction

Development Alternatives Inc. (DAI) has been selected by the U.S. Agency for International Development (USAID) to implement the Partnership for Economic Growth (Partnership) program in Somaliland and Puntland. The Partnership program seeks to help local authorities and private sector groups improve the enabling environment for investment, generate more productive employment and improve other livelihood activities. One of the Partnership program’s initiatives is called the Partnership Fund, which is a matching grants program for local businesses in Somaliland. Muliyo Salt Trading Company has been selected for a grant to support the extraction of salt, and the establishment of a salt refining plant. 

Muliyo Salt Trading Company is a small business enterprise operating since 2009. It business so far has been to buy and resell salt procured from Tokhoshi in and around the Boroma, Awdal region.  A new venture and partnership has been established to form the Muliyo Salt Processing Project, which is an expansion of the Muliyo Salt Trading Company. This new venture will include activities like salt refining, packaging, and distributing to end users or salt traders. 

Muliyo’s manufacturing plant will be located in Boroma with the raw salt to be sourced from Tokhoshi. This salt producing village is located some 240Km north of Boroma, west of Zeila, and east of Loya’de (border town with Djibouti Republic).

The main activities of the business will encompass of following: 
•	To produce part of the salt in Tokoshi ,
•	Purchase of raw salt from the local producers,
•	Arrange transportation to Boroma
•	Refining and packaging raw salt
•	Distribution and marketing



II. Place of Performance:

Offeror is responsible for delivery of goods to Berbera Port, Somaliland.   Transport of goods from Berbera to Boroma will be done by the buyer.  The plant will be located in Boroma.  All Services shall be provided in Boroma, Somaliland.  











III. Equipment Specifications and Performance Requirements

The technical proposal should contain the specifications for equipment that can provide the following functions/meet the following requirements:


A. List of Plant Machinery: (For full details and specifications refer to section IX. Annex)


	LIST OF PLANT MACHINERY FOR 2.5 TPH SALT REFINERY

	Sr. No.
	Item Description
	Qty.
	MOC
	Ref Drg. / Datasheet No.
	POWER (kW)

	A.
	Raw Salt Feed Section
	
	
	
	

	1
	Feed Hopper
	1 No
	SS 316
	3a
	

	2
	Gate Valve
	1 No
	SS 316
	
	

	3
	Flat Raw Salt Belt Conveyor (300 mm wide, centre to centre distance = 10 mtrs. Approx, complete with Magnets, skirt, scrappers and discharge hood)
	1 No.
	Food Grade Rubber
	3b
	Pl. Specify

	4
	Raw Salt Roll Crusher (2.5 TPH, Feed 10 mm Max, Product below 3 mm)
	1 No
	CI Chilled Rolls
	3c
	Pl. Specify

	B.
	Wet Section
	
	
	
	

	1
	Slurry formation Tank Size 1.5 M High X750 mm Wide X 750 mm Long
	1 No.
	SS 316
	3ei
	

	2
	Slurry Pump-I (30% solids, 5 mlc, 10,000 LPH, SS 316 wetted parts, Mechanical seal, 1500 RPM)
	1 No.
	SS 316
	3d
	Pl. Specify

	3
	Wash Tank with Agitator
	1 No.
	SS 316
	3e
	Pl Specify

	4
	Slurry Pump-II (10% solids, 5 mlc, 25,000 LPH, SS 316 wetted parts, Mechanical seal, 1500 RPM)
	1 No.
	SS 316
	3d
	Pl. Specify

	5
	Elutriation Tank
	1 No.
	SS 316
	3e
	

	6
	Slurry Pump-III (20% solids, 5 mlc, 15,000 LPH, SS 316 wetted parts, Mechanical seal, 1500 RPM)
	1 No.
	SS 316
	3d
	Pl. Specify

	7
	Brine Pump (15 mlc, 25,00 LPH, SS 316 wetted parts, Mechanical seal, 1500 RPM)
	1 No.
	SS 316
	3d
	Pl. Specify

	8
	Brine Header
	1 No.
	SS 316
	
	

	C.
	Centrifuge Section
	
	
	
	

	1
	Thickener
	1 No.
	SS 316
	3e
	

	2
	Pusher Type Hydraulic, 2-stage Centrifuge 2.5 TPH (Process side SS 316)
	1 No.
	SS 316
	3g
	Pl Specify

	3
	Washed Salt Paddle Screw Conveyor (200 mm wide, centre to centre distance = 10 mtrs. Approx, with Cover and three discharge outlets)
	1 No.
	SS 316
	3f
	Pl Specify

	D.
	Dosing Section
	
	
	
	

	1
	Dosing Tank with Agitator (100 Lit)
	1 Nos.
	SS 316
	3i
	Pl Specify

	2
	Dosing Pump (SS 316, 5 LPH)
	1 Nos.
	SS 316
	3i
	Pl. Specify

	E
	Packaging Section
	
	
	
	

	1
	Volumetric Cup Fillers
	2 Nos
	SS 316
	3h
	Pl. Specify

	2
	Hand Sealers
	6 Nos
	Std
	3h
	Pl. Specify

	F
	Others
	
	
	
	

	1
	Magnets before Roller Crusher and after centrifuge
	1 No Each
	SS 316 Casing
	
	

	2
	Electrical Panel with capacitor bank, Indicator lights, Single phase preventer, Ammeter, Voltmeter and PF meter
	1 No
	Std
	
	

	3
	Local ON/OFF Push switches, Cables, Glands, Cable trays, Earthing plate, Earth Strip & Wire
	Al./ Cu
	
	
	

	4
	Piping, Hangers & Supports, Valves and Instrumentation
	1 Lot
	Food Grade PVC, HDPE, Std.
	
	

	5
	Lab Equipment
	1 lot
	Std.
	
	

	
	Total Connected Power
	
	
	
	Pl Specify



Notes:
1. Refer to all drawings and specification datasheets in annex, section IX.
	2. All equipment to be supplied with foundation bolts, lugs, supports, anti-vibrations pads, gaskets, sealants, 	    guards, dust covers and safeties.
3. All exposed MS parts shall be epoxy painted.


B. Additional Information Required:, 
i. Manufacturer and models of all components 
ii. Mass Balance Diagram
iii. List, Specifications of Equipment and Drawings of Fabricated Equipment.
iv. GA of the Plant
v. Specifications of the Final Product
vi. Utility Requirements
vii. Building & Structural Requirements
viii. List of deviations from the specifications mentioned in the document
ix. Supports required at site for installation
x. Items and their quantities needed for commissioning and operation of Plant but not included in the scope of supply
xi. List of Lab Equipment
xii. List of Spares for 2 years operation

Safety Requirements:
Please describe in detail the safety and reliability standards of the equipment.
Supporting Documentation:  
We strongly encourage each offeror to include in the submission photos, performance graphs, manuals, and any other useful supporting documentation.
IV. Warranty and Maintenance Requirements

The equipment shall be under warranty for one year from the date of commissioning OR 18 months from the date of Bill of Lading, whichever is earlier.. 

Remote support over phone / Skype, e-mails shall be provided during warranty period. Technicians should speak fluent English for support correspondence purposes.  

V. Shipping and Delivery

The offeror shall define a delivery period for the equipment.  Delivery is expected within 4 months or less of Purchase Order signing.  Equipment should be delivered to the Port of Berbera, Somaliland.


VI. Technical Assistance

A technician is to be sent from the offeror upon arrival of equipment in country to inspect, install and commission the plant, as well as provide end user training in operations and lab analysis.  The location for installation is Boroma, Somaliland.  The offeror should specify how long the installation and training will take (we estimate about a month, no later than July 15- August 15, 2013). The technician should plan to provide operating and maintenance manuals and a list of recommended spare parts.

The offeror will responsible for all travel-related costs for its technician and should account for these costs in their proposal. 



VII. Staffing

The offeror shall submit CV(s) consisting of qualified technician(s) and engineer(s).  Proposed staff should have a minim of ten years’ experience in the salt industry or a related sector.


VIII. Deliverables

The offeror shall submit the following deliverables as products under this SOW: 


Deliverable 1: Provision of work-plan including equipment and plant design

i. Details of Electric panel
ii. List of pipes and valves
iii. List of cables & cable trays
iv. Foundation Drawings
v. Drawings for Settling Pond

Deliverable 2: Delivery of Equipment 

i. All equipment as listed in the RFP Annex 1or as otherwise agreed to in the PO is delivered to Berbera, Somaliland
ii. Invoice & Packing List
iii. Certificate of Origin
iv. Bill of lading, marked clean, chipped on board

Deliverable 3: Installation, verification and end-user training

i. Operating & Maintenance Manuals
ii. Manual for Lab Analysis Protocols
iii. Inspection of equipment  by DAI Technical Specialist.
iv. Installation, commissioning, and final verification of equipment and performance testing according to the specifications by vendor technician and DAI Technical Specialist
v.  Training of Muliyo staff on system operations by vendor technician.


IX. Annex

See below Annex which includes the list of equipment, datasheets & drawings for various items under scope of supply, and specifications for raw salt. 










Attachment “C”
Cover Letter



PROPOSAL COVER LETTER
[On Firm’s Letterhead]


<Insert date>  	

TO:		Hirsi Farah 
Development Alternatives, Inc.
USAID Partnership for Economic Growth program
Next to FAO
Bada Cas, Kodbur District
Hargeisa, Somaliland


We, the undersigned, provide the attached proposal in accordance with RFP- Partnership-2013/23 dated January 30th, 2013. 

Our attached proposal is for the total price of <Sum in Words ($0.00 Sum in Figures) >. 

I certify a validity period of three months for the prices provided in the attached proposal.  Our proposal shall be binding upon us subject to the modifications resulting from any discussions.

We understand that DAI is not required to accept and/or evaluate proposals that do not conform to the instructions of this RFP, and additionally, DAI may reject all proposals and not award a subcontract for this RFP.


Sincerely yours, 


Authorized Signature:	

Name and Title of Signatory:	
				
Name of Firm:	

Address:	










Attachment “D”
Proposal Checklist

 
Please check all that apply and include this page in with the proposal submission.


Offeror: __________________________________________________________________________


Have you? 

|_|	Submitted your technical and financial proposal as separate documents to Partnership@dai.com by the required deadline?

Does your proposal include the following? 

|_|	Cover Letter (use template in Attachment C) 

|_|	Proposal Checklist (use template in Attachment D)

|_|	Bidder’s Company Information (use template in Attachment E)

|_|	Signed Certifications of Compliance (use template in Attachment F)

Technical Proposal

|_|	Technical Approach

|_|	Delivery and Technical Assistance Timeline 

|_|	Summary of Relevant Work Experience
 (use template in Attachment H) 

Cost Proposal

|_|	Detailed Cost Breakdown 













Attachment “E”
Bidder’s Company Information


To facilitate the evaluation and award process, please provide the following information about your company. This information is also required of all subcontractors included in your proposal. If an item is not applicable to your organization, please put “N/A” on the blank(s) provided.  Do not leave items unanswered.

	
CONTACT INFORMATION


	Company Name:


	Company Representative
Name:

Title/Position:

Phone:
Fax:
Email:

	Address 1:


	

	Address 2:

	

	City, State:

	Technical Representative
Name:

Title/Position:

Phone:
Fax:
Email:

	Zip Code:

	

	Country:

	

	Name of Parent Company:


	Parent Company Address:

	Web Page URL:

	

	
COMPANY PROFILE


	Type of Organization:
|_|  Non-profit	|_|  Government Entity 
|_|  For-profit		|_|  International Organization per 26 CFR 1.6049-4
|_|  Educational Institution	|_|  Other  	__________________________________________
|_|  Government-owned organization	


	CCR Registration: Yes |_|  No |_|
	Orca Registration: Yes |_|  No |_|   Orca Registration date:  


	DUNS Number:

	If Bidder is owned or controlled by a common parent:
Parent Name:
Parent EIN:













Attachment “F”
Representations and Certifications of Compliance


1. Federal Excluded Parties List - The Bidder Select is not presently debarred, suspended, or determined ineligible for an award of a contract by any Federal agency.

2. Executive Compensation Certification-  FAR 52.204-10 requires DAI, as prime contractor of U.S. federal government contracts, to report compensation levels of the five most highly compensated subcontractor executives to the Federal Funding Accountability and Transparency Act Sub-Award Report System (FSRS) 

3. Executive Order on Terrorism Financing- The Contractor is reminded that U.S. Executive Orders and U.S. law prohibits transactions with, and the provision of resources and support to, individuals and organizations associated with terrorism.  It is the legal responsibility of the Contractor/Recipient to ensure compliance with these Executive Orders and laws.  This provision must be included in all subcontracts/sub awards issued under this Prime Agreement.

4. Certification and Disclosure Regarding Payment to Influence Certain Federal Transactions – The Bidder certifies that it currently is and will remain in compliance with FAR 52.203-11, Certification and Disclosure Regarding Payment to Influence Certain Federal Transactions.

5. Organizational Conflict of Interest – The Bidder certifies that will comply FAR Part 9.5, Organizational Conflict of Interest.  The Bidder certifies that is not aware of any information bearing on the existence of any potential organizational conflict of interest.  The Bidder further certifies that if the Bidder becomes aware of information bearing on whether a potential conflict may exist, that Bidder shall immediately provide DAII with a disclosure statement describing this information.

6. Business Size and Classification(s) – The Bidder certifies that is has accurately and completely identified its business size and classification(s) herein in accordance with the definitions and requirements set forth in FAR Part 19, Small Business Programs.

7. Prohibition of Segregated Facilities - The Bidder certifies that it is compliant with FAR 52.222-21, Prohibition of Segregated Facilities.

8. Drug-Free Workplace – The Bidder certifies that it complies with the Drug-Free Workplace Act of 1988 (45 CFR Part 76, Subpart F) and, further, understands that any violation of the prohibitions of this Act is a breach of contract and can result in default action.

9. Federal Civil Rights Act – The Bidder certifies that it conforms to the provisions of the Federal Civil Rights Act of 1964, as amended and does not discriminate against any employee or applicant for employment because of race, religion, color, sex, national origin, or disabilities.

10. Americans with Disabilities Act – The Bidder certifies that it complies with the Americans with Disabilities Act.

11. Equal Opportunity – The Bidder certifies that it does not discriminate against any employee or applicant for employment because of age, sex, religion, handicap, race, creed, color or national origin.

12. Labor Laws – The Bidder certifies that it is in compliance with all labor laws, including but not limited to the Walsh-Healy Act and the Contract Work Hours and Safety Standards Act regarding overtime compensation.

13. Federal Acquisition Regulation (FAR) – The Bidder certifies that it is familiar with the Federal Acquisition Regulation (FAR) and is in not in violation of any certifications required in the applicable clauses of the FAR, including but not limited to certifications regarding lobbying, kickbacks, equal employment opportunity, affirmation action, and payments to influence Federal transactions.

14. Employee Compliance – The Bidder warrants that it will require all employees, entities and individuals providing services in connection with the performance of an DAI Purchase Order to comply with the provisions of the resulting Purchase Order and with all Federal, State, and local laws and regulations in connection with the work associated therein.

15. Special Restrictions – The Bidder certifies that it is not affiliated with, controlled by, or acting on behalf of excluded parties, including al Shabaab. The Bidder warrants that it will not knowingly make cash facilitation payments, purchase goods or services, or make payments to excluded parties as the de facto municipal authority using funds issued under any award resulting from this procurement.

The information contained in this offer is current, accurate and complete to the best of my knowledge and belief. Bidder further agrees to fully comply with the terms and conditions set forth in Agreement Terms & Conditions (Attachment G) and all applicable federal clauses included herein.


_______________________________________________________________________________________
Name of Authorized Official		Title			Signature		Date


























Attachment “G”
Agreement Terms & Conditions

DEVELOPMENT ALTERNATIVES, INC. - TERMS AND CONDITIONS
This Purchase Order ("Order") is an offer made by Development Alternatives, Inc. or its subsidiaries and affiliates	
(collectively, "DAI") to purchase goods or services on these terms and conditions, as may be modified by varying terms printed on the face of this Order (collectively, "Terms"). By acceptance of this Order and/or performance hereunder, Vendor agrees to comply fully with these Terms and any attachments to this Order. Any attachments referred to in this Order are hereby incorporated herein by reference. Acceptance of this Order is expressly limited to these Terms, and Vendor's terms and conditions in acknowledging or accepting this Order shall not apply. Acceptance by DAI of the goods and/or services under this Order is not acceptance of Vendor's terms and conditions. No employee, representative, or agent of DAI has any authority to bind DAI concerning this Order unless specifically stated herein or in a written amendment signed by an authorized representative of DAI's Procurement Department. When specified by DAI, Vendor shall comply with the geographic code requirements as set forth by the Client. Vendor will ensure that it does not engage in any procurement activity from the following countries: Cuban, Iran, Syria, Sudan and North Korea.
1. Definitions -
"Agreement" means the Purchase Order, these terms, and any other mutually executed agreement between Vendor
and DAI under which this Purchase Order is issued.
"Client" means the US government or another client of DAI.
"DAI" means Development Alternatives, Inc., with its principal place of business at 7600 Wisconsin Avenue, STE 200,
Bethesda, MD 20814 or its subsidiaries and affiliates.
"Goods" means goods specified by DAI in the Agreement.
"Order" means the Purchase Order issued by an authorized DAI representative.
"Services" means services specified by DAI in the Agreement.
"Taxes" means any and all applicable taxes, charges, fees, levies or other assessments applicable to the performance
of Services or the supply of Goods hereunder.
"Terms" means the terms and conditions specified in the Agreement.
"Vendor" means a party receiving a Purchase Order from DAI which references the Terms.
2. Acceptance - Final inspection and acceptance of goods and services shall be at the DAI receiving point
indicated in this Order. Nonconforming goods shall be returned to Vendor, freight collect, and Vendor shall be
debited for the transportation costs to DAI plus handling expenses. Such rejected goods shall be deemed to be
property of Vendor.
3. Price and Delivery - Vendor shall furnish the goods or services in accordance with the price and delivery terms
stated herein. TIME AND RATE OF DELIVERY ARE OF THE ESSENCE. Payments are due forty five (45)
days after DAI's receipt of a complete and correct invoice. Vendor certifies that each invoice issued by it shall be
based solely on Services actually performed by Vendor and Goods actually supplied by Vendor pursuant to a
PO, and that no part or portion of any invoice represents or is attributable to any payment, gift, gratuity or other
thing of value given to any person, organization, entity or governmental body (except for those payments
required by law).Unless otherwise stated, the price terms contained herein include all costs or charges of any
kind that will by paid by DAI, and DAI shall not be liable for any other costs or charges, all of which shall be
borne by Vendor, including, without limitation, unspecified charges for inspection, packaging and shipping; all
federal, state and municipal sales, use and other taxes and duties. Whenever any actual or potential event
occurs, including labor disputes, that delays or threatens to delay the timely performance of this Order, Vendor
shall give immediate notice thereof to DAI.
4. Packaging And Shipping - Vendor shall be responsible for packaging, marking and shipping the goods in
accordance with the terms hereof, good commercial practices and all applicable laws. Each package shall be
marked with handling instructions, shipping information, Order number and part or item number. An itemized
packing list shall accompany each shipment. DAI reserves the right to reject any shipment not meeting these
requirements.
5. F.O.B., Risk Of Loss - F.O.B. point shall be DAI's location unless otherwise stated in writing by DAI. Goods
purchased f.o.b. Vendor's plant or shipping point shall not be considered delivered until they have been
accepted at the DAI receiving point indicated herein; however, DAI assumes responsibility at the f.o.b. point for
carrier routing, transportation charges, and risk of loss or damage to goods in transit, if properly prepared and
packed. Vendor shall bear all risk of loss with respect to any goods rejected by DAI.
6. Warranty - Vendor warrants all goods and services delivered or provided hereunder to be non-infringing, free
from defect in title, material and workmanship, and fit for the purpose intended for a period of twelve (12)
months from delivery to DAI and to meet or exceed the specifications, drawings, or sample specified or
furnished and any supplementary documentation referenced herein. Vendor further warrants that all goods and
services delivered or provided hereunder comply with requirements of all applicable laws and regulations. This
warranty shall survive any inspection, delivery, or acceptance of the goods and services or payment therefore
by DAI.
7. Remedies/Waiver - If Vendor fails to timely perform its obligations under this Order, DAI reserves the right to
terminate this Order for default and purchase the goods or services elsewhere. If any goods or services covered
by this Order are defective or non-conforming or fail to meet applicable warranties ("Defective Material"), DAI
may, by written notice to the Vendor: (a) terminate this Order for default; (b) accept the Defective Material at an
equitable reduction in price; or (c) reject the Defective Material and (i) require the delivery of suitable
replacements or re-performance of services or (ii) repair such material, perform such services or purchase the
Defective Material elsewhere. DAI may hold Vendor accountable for any additional cost or damages incurred
by DAI. All Defective Materials replaced or re-performed by Vendor are subject to these Terms to same extent
as items initially furnished or originally ordered. This warranty provision shall survive any inspection, delivery,
acceptance, payment, expiration or earlier termination of this Order and such warranties shall run to DAI, its
successors, assigns, employees, students, and users of the goods or services. Rights and remedies of DAI
hereunder are cumulative and in addition to those which DAI has under law and equity. Any waiver by DAI of
any particular breach or default hereunder by Vendor shall not constitute a continuing waiver or a waiver of any
other breach or default. Approval by DAI of Vendor's proposed design, test plans, and/or procedures and
manufacturing process, methods, tooling, or facilities shall not relieve Vendor from meeting all requirements of
this Order.
8. Changes - At any time by written notice to Vendor, DAI may change the Order, including the specifications,
design, delivery, testing methods, packing, destination or any instructions. If any such required changes cause
an increase or decrease in the cost of or the time required for performance, an equitable adjustment shall be
made in the contract price or delivery schedule, or both. Vendor will give written notice to DAI of any proposed
equitable adjustment within ten (10) days of receiving notice from DAI of such changes. Vendor and DAI will
negotiate in good faith any proposed adjustments and upon agreement, DAI will incorporate issue an amended
Order incorporating the changes. Any change to be valid and binding upon DAI must be in writing and signed by
an authorized representative of DAI's Procurement Department.
9. Termination - DAI shall have the right to terminate this Order in whole or in part by providing 14 days prior
written notice to Vendor. DAI shall be liable for (a) the price of any items on this Order previously accepted by
DAI, and (b) reasonable costs incurred by Vendor for labor and materials for work in process and finished
conforming material plus a reasonable profit not to exceed 10% on such items. Such cost plus profit will not
exceed the cost of the goods ordered. DAI may elect to take possession of work in process and finished
conforming material.
10. Bankruptcy - If any bankruptcy, reorganization or insolvency proceedings, voluntary or involuntary, are
instituted by or against Vendor, or in the event of the appointment of an assignee for the benefit of creditors or
of a receiver, then DAI may cancel this Order and hold Vendor accountable for any costs or damages incurred
by DAI.
11. Assignment ?DAI and Vendor each binds itself and its successors and assigns to all warranties, covenants,
agreements, and obligations contained in this Order. Vendor may not assign or delegate all or any part any of its
rights (except to a lending institution in the normal course of business) or obligations hereunder without the prior
written consent of DAI, and no such assignment or delegation shall relieve Vendor of any such obligations. Any
such assignment or delegation shall be voidable at DAI's election.
12. DAI Property - All materials, tools, drawings, specifications and other items furnished or paid for by DAI shall be
identified as DAI property, removable by DAI at any time at no cost, used only in filling DAI Orders, inventoried
by Vendor, kept separate from other such materials, treated as DAI confidential information, and disposed of by
Vendor when and as DAI shall direct. Vendor shall be responsible for loss or damage to any such DAI property
excepting normal wear and tear. Vendor shall be responsible and accountable for all DAI or Client provided
property and, where applicable, Vendor shall comply with the requirements of 48 C.F.R. 45.5 with respect to
such property. Vendor assumes the risk of, and shall be responsible for, any loss or destruction of, or damage
to, DAI or Client property upon its delivery to Vendor employees. In the event of loss, damage or destruction of
DAI or Client property by Vendor, DAI may initiate an equitable adjustment to the Prices in favor of DAI. DAI
may direct changes to the Agreement in writing, and Vendor shall comply immediately with such direction. If DAI
directed changes increase or decrease the cost or time required Vendor's deliverables under the Agreement,
the parties shall negotiate an equitable adjustment in the price or schedule, or both, to reflect the increase or
decrease.
13. Information Disclosed - Information disclosed to Vendor by DAI contains DAI's confidential information, which
Vendor shall not disclose to any third party (except as required by law) without DAI's prior written consent.
Unless expressly agreed to in writing by DAI, no information or knowledge disclosed to DAI in the performance
of or in connection with this Order shall be deemed to be confidential or proprietary and any such information or
knowledge shall be free from restrictions as part of the consideration for this Order.
14. Publicity - Vendor shall not issue any public announcement regarding this Order or use the DAI name or
trademarks without prior written consent of DAI.
15. Indemnification - Vendor, at its sole expense, agrees to defend, indemnify and hold harmless DAI from and/or
against any and all claims, damages, costs, liability, and expenses, including reasonable attorneys' fees, that (i)
arise out of any breach of representation, agreement, or warranty made by Vendor; (ii) the performance of any
service or the delivery, installation, use or service of any item listed on this Order; (iii) are caused in whole or in
part by any act or omission of Vendor, Vendor's subcontractor, or anyone for whose acts Vendor may be liable;
or (iv) are attributable to bodily injury, sickness, or death; injury to or destruction of property including the loss of
use resulting therefrom; interference with the business or operations of any third party; or violation of any
governmental law or regulation. This paragraph shall survive the termination of this Order and shall continue in
effect until any hearing, litigation, or claims have been finally concluded and settled.
16. Insurance - As a minimum, Vendor shall, at its sole cost and expense, provide and maintain the following
insurance coverage and insurance coverage limits: (1) Worker's Compensation: Vendor shall provide and
maintain worker's compensation insurance as required by the laws of the applicable jurisdiction, as well as
employer's liability coverage with minimum limits of $1,000,000 (or an equivalent value in the local currency),
covering all of Vendor's employees who are engaged in any work under the Agreement; and if any work is
subcontracted, Vendor shall require the subcontractor to provide the same coverage for any of its employees
engaged in any work under the Agreement, (2) Commercial General Liability: Vendor shall maintain general
liability coverage on a comprehensive broad form on an occurrence basis in the minimum amount of $1,000,000
(or an equivalent value in the local currency) combined single limit (where the defense is in excess of the limit of
liability); (3) Automobile: Vendor shall maintain automobile liability insurance to include liability coverage,
covering all owned, hired and non-owned vehicles used in connection with the Agreement, and the minimum
combined single limit shall be $1,000,000 (or an equivalent value in the local currency) bodily injury and
property damage, including: (a) $500,000 (or an equivalent value in the local currency) uninsured/underinsured
motorist; and (b) $5,000 (or an equivalent value in the local currency) medical payment. Providing and
maintaining adequate insurance coverage is a material obligation of the Vendor under the Agreement. Such
insurance coverage shall be obtained from companies that are authorized to provide such coverage in
accordance with the governing jurisdiction(s). Vendor shall at all times comply with the terms of such insurance
policies, and all requirements of the insurer under any such insurance policies, except as they may conflict with
applicable laws or the Agreement. The limits of coverage under each insurance policy maintained by Vendor
shall not be interpreted as limiting the Vendor's liability and obligations under the Agreement.
17. Intellectual Property - Vendor grants DAI all rights and licenses necessary for DAI to use the Goods or
Services. The parties acknowledge and agree that all Services shall be deemed to be "works for hire", with all
intellectual property rights therein vesting in DAI, unless otherwise mutually agreed. Vendor agrees to
irrevocably transfer and assign all such rights to DAI, and comply with all reasonable requests by DAI to affect
such transfer and assignments. Vendor represents and warrants that the materials delivered hereunder and
their use by DAI will not infringe upon or misappropriate with any patent, copyright, trademark, trade secret or
other property right of Vendor or any third party or require any payment by DAI in respect of such rights to
Vendor or any third party. Vendor agrees to indemnify and hold harmless DAI for any breach of the foregoing
representation and warranty in accordance with the paragraph entitled "Indemnification."
18. Compliance - Vendor shall comply with all laws and regulations of Federal, State, or local governments, as well
as all U.S. statutes, regulations, and administrative requirements regarding relationships with non-U.S.
governmental and quasi-governmental entities including but not limited to the export control regulations of the
Department of State and the International Traffic in Arms Regulations ("ITAR"), the Department of Commerce
and the Export Administration Act ("EAA"), the anti-boycott and embargo regulations and guidelines issued
under the EAA, and the regulations of the U.S. Department of the Treasury, Office of Foreign Assets Control.
Vendor shall give all notices and obtain all permits and licenses required under such laws. The anti-bribery
provisions of the Foreign Corrupt Practices Act of 1977 ("FCPA"), 15 U.S.C. 78dd-2", et seq., make it unlawful
for U.S. concerns, as well as their officers, directors, employees, and agents, to corruptly offer or make a corrupt
payment of money or anything of value to a foreign official for the purpose of obtaining or retaining business.
Vendor acknowledges and understands that Vendor must comply fully with the anti-bribery provisions of the
FCPA. Specifically, Vendor understands and agrees that it shall be unlawful for Vendor to pay, promise to pay
(or authorize to pay or offer) money or anything of value to a foreign official in order to assist DAI in obtaining or
retaining business for or with, or directing business to, DAI. A "foreign official" means any officer or employee of
a foreign government, a public international organization, or any department or agency thereof, or any person
acting in an official capacity. Vendor understands all applicable laws relating to kickbacks. Vendor agrees to
periodically verify its compliance with such laws and to inform DAI immediately of any violations thereof. Vendor
shall maintain a Code of Business Ethics and Conduct in accordance with the provisions of FAR 52.203.13. The
provisions of 22 C.F.R. Part 140, Prohibition of Assistance to Drug Traffickers apply to Vendor and shall have
the same effect as if they were stated in their full text. Vendor shall take affirmative action in compliance with all
Federal and State requirements concerning fair employment, employment of the handicapped, employment of
veterans, and concerning the treatment of all employees without regard to discrimination by reason of race,
color, religion, sex, national origin, or physical handicap as described in 48 C.F.R. 52.222-26, Equal
Opportunity, 48 C.F.R. 52.222-35, Affirmative Action for Special Disabled Veterans, Veterans of the Vietnam
Era, and Other Eligible Veterans, and 48 C.F.R. 52.222-36, Affirmative Action for Workers with Disabilities. The
provisions of 48 C.F.R. 52.222-50, Combating Trafficking in Persons, apply to Vendor and have the same effect
as if they were stated in their full text. Vendor is reminded that U.S. Executive Orders and U.S. law prohibit
transactions with, and the provisions of resources and support to, individuals and organizations associated with
terrorism. It is the legal responsibility of Vendor to ensure compliance with these Executive Orders and laws.
The provisions of resources and support to, individuals and organizations associated with terrorism. It is the
legal responsibility of Vendor to ensure compliance with these Executive Orders and laws.
19. Exports - Vendor agrees to comply with all U.S. export control laws and regulations, specifically including but
not limited to, the requirements of the Arms Export Control Act, 22 U.S.C. 2751-2794, including the International
Traffic in Arms Regulation (ITAR), 22 C.F.R. 120 et seq.; and the Export Administration Act, 50 U.S.C. app.
2401-2420, including the Export Administration Regulations, 15 C.F.R. 730-774; including the requirement for
obtaining any export license or agreement, if applicable. Vendor agrees to notify DAI if any deliverable under the
Agreement is restricted by export control laws or regulations. Vendor shall immediately notify DAI if Vendor is,
or becomes listed in any Denied Parties List or if Vendor's export privileges are otherwise denied, suspended,
or revoked in whole or in part by any U.S. Government entity or agency. Vendor shall be responsible for all
losses, costs, claims, causes of action, damages, liabilities and expense, including attorney's fees, all expense
of litigation and/or settlement, and court costs, arising from any act or omission of Vendor, its officers,
employees, agents, or subcontractors at any tier, in the performance of any of its obligations under this section.
Vendor shall include the Terms of this section in all subcontracts issued when technical data is provided to such
subcontractors.
20. DAI Requirements - Vendor will ensure that its employees, agents, or designees, when in or upon DAI's
premises, shall obey all ethics and business conduct, workplace health, safety and security rules and
regulations established by DAI, regarding the conduct of its own employees and any additional rules and
regulations established by DAI for non-employees, including without limitation, security rules, and regulations.
21. Governing Law - This Order and the acceptance thereof shall constitute a valid, binding, and enforceable
contract governed by the laws of the State of Maryland, without regard to its principles of conflicts of law.
22. General - If any clause of this Order is held as a matter of law to be unenforceable or unconscionable, the
remainder of this Order shall be enforceable without such clause. This Order supersedes and replaces any
previous documents, correspondence, conversations, or other oral or written understandings between DAI and
Vendor related to the subject hereof. This Order cannot be amended, changed, or modified in any respect
unless each such, amendment, change, or modification shall have been agreed upon in writing, signed and
delivered by each party hereto.
23. Exclusion Of Damages - DAI shall not be liable for any consequential, punitive, exemplary, special or other
indirect damages, in contract, tort or otherwise in any action arising out of this Order. DAI will not be liable for
any amount in excess of the amounts paid to Vendor hereunder
24. Somalia Conditions
1. Consistent with the September 10, 2009 memorandum from the Department of State (State) to the Department of Treasury‘s Office of Foreign Assets Control (OFAC), and with the September 16, 2009 memorandum from OFAC to State, both relating to State/USAID Somalia Programs (such memoranda attached hereto at Tab 1), the Vendor agrees that it and/or its implementing partners (including contractors, grantees, sub-contractors and sub-grantees) will not knowingly and voluntarily make payments or provide any other benefits to al Shabaab, or to entities controlled by al Shabaab, or to individuals acting on behalf of al Shabaab (collectively, “excluded parties”). Such prohibited payments or other benefits would include:
a) cash facilitation fees or other similar fees at roadblocks, ports, warehouses, airfields or other transit points to excluded parties;
b) purchases or procurement of goods or services from excluded parties; and
c) payments to al-Shabaab as the de facto municipal authority
2. The Vendor and its implementing partners (including contractors, grantees, sub-contractors and sub-grantees) agree to exercise enhanced due diligence when providing assistance to Somalia under this agreement to avoid the accidental, unintentional or incidental provision of such payments or benefits to excluded parties.
3. In the event that the Vendor or its implementing partners (including contractors, grantees, sub-contractors and sub-grantees) becomes aware that it made a payment or provided a benefit to excluded parties, the Vendor shall, in accordance with 22 CFR 226.51(f) and within ten days after becoming aware of such payment or provision of benefit, notify the DAI Contracts Manager in writing, with a copy to the DAI Project Director, of such payment or provision of benefit. This notification shall include the following information:
a) Factual descriptions of each such event;
b) Amount of funds expended or other benefit provided for each event;
c) Safeguards and procedures, including management and oversight systems, that were in place to help avoid the occurrence of such event; and
d) Explanation of the reasons for each such payment or each such benefit provided, including whether it was made or provided knowingly, voluntarily, accidentally, unintentionally, incidentally, or forced.




Attachment “H”
References and Past Performance

A. List 3 current and/or former clients which your firm has provided similar equipment or service.

1.  Name and Location of Project:
___________________________________________________________________________________________
  ___________________________________________________________________________________________
 
Contract Amount: _________________

Percent Complete:_________________

Projected Completion Date:_________

Description of Services/Goods Provided: _________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________

Owner Reference Contact:
______________________________________________          _______________________
Name 								Telephone
______________________________________________
Address
_______________________________________________         _______________________
Name 								Telephone
_______________________________________________
Address


2.  Name and Location of Project: ___________________________________________________________________________________________
   ___________________________________________________________________________________________

Contract Amount: _________________

Percent Complete:_________________

Projected Completion Date:_________

Description of Services/Goods Provided: _________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________

Owner Reference Contact:
______________________________________________          _______________________
Name 								Telephone
______________________________________________
Address
______________________________________________          _______________________
Name 								Telephone
______________________________________________
Address

3. Name and Location of Project:
___________________________________________________________________________________________
___________________________________________________________________________________________

Contract Amount: _________________

Percent Complete:_________________

Projected Completion Date:_________

Description of Services/Goods Provided: _________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________

Owner Reference Contact:
______________________________________________          _______________________
Name 								Telephone
______________________________________________
Address
_______________________________________________         _______________________
Name 								Telephone
_______________________________________________
Address


B. Provide the following information on the current work portfolio of your company

1. Total number and dollar amount of contracts currently in progress:

Number____________________________________ $_____________________________

2. Largest single contract amount currently in-progress: $_____________________________

Project Name: _______________________________________________________________

Project Completion Date: ______________________________________________________

3.  Volume of work completed over 5 years: 

2012 $____________________
2011 $____________________
2010 $____________________
2009 $____________________
2008 $____________________
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3c. Datasheet-Roller Crusher.pdf

USAID APTECH DATA SHEET FOR DATA SHEET. NO: 3c
SOMALILAND ENGINEERS RAW SALT ROLLER CRUSHER
Vendor Name: Sheet 1 of 2 Sheets
Sr. No. Description Units

1. Item No.

o Type of Equipment Roller Crusher

3. Capacity MT/Hr. 3

4. Quantity 1 1

5 Purpose Crushing Raw Salt

6. Process Data:

6.1 Feed Material Salt Granules

a. Feed Input Size mm Below 5

b. Feeding System Belt Conveyor

. Discharge To Slurry Tank

d. Lumps Occasional

e. Moisture % 3-5

f. Output Size mm 05t 1

g. Temperature °C 50 °C max

h. Pressure ATM Atmospheric

7. Design Data

Mechanical Design
Requirements

a. Design Pressure ATM Atmospheric

b. Installation In Door

C. Operation Intermittent








USAID APTECH DATA SHEET FOR DATA SHEET. NO:3c
SOMALILAND | ENGINEERS RAW SALT ROLLER CRUSHER
Vendor Name: Sheet 2 of 2 Sheets
Sr. No. Description Units
8. Material of Construction ClI Chilled — Min. 20 mm thick Shell
a. Width mm 350
b. Diameter mm 250 min
C. Shaft type and MOC Solid, EN8
d. Shaft Diameter mm 80
e. Hopper size and MOC 400 x 400 with 3 mm SS316
f. Magnet To be at feed side
g. Motor Power HP *
h. Motor RPM 1440
j- Space reqd. for Machine *Mxmxm | *
Notes:
1. Supplier to submit duly filled in data sheet along with bid.
2. Blanks To be stated / confirmed by supplier.
3. Utility requirements to be specified by the vendor with the bid.
4. Supplier to provide all safety guards
5. All exposed parts to be epoxy painted












3d.Muliyo-2.5TPH-Pump-Datasheets.pdf

APTECH ENGINEERS,

DATA SHEET FOR SLURRY PUMP -I

DATA SHT.NO.3d

INDIA SHEET 1 OF 4 SHEETS
DAI CONTRACT NO.:
Main Item No. Plant : SALT PLANT
Total No. 1 \Working 1 \Stand by None Location: Indoor
1 |Service: Slurry Circulation Pump Drive : Motor
2 |Fluid : Brine Slurry 30% Area Classification : SAFE W R T ELECT HAZARDS
3 |Analysis/Solids content: - NaCl Crystals Pumping Temperature: Normal 80° C Max. 85°C Min.
4 |DUTY (each pump) Units Normal Rated |Specific Gravity : 1.2 Max. Min.
5 |Capacity m3/h 10 12 Viscosity, Centiposes 0.63 Max. Min.
6 |Discharge pressure kg/cm2A 2.5 35 Vapour pressure @ 42°C : 0.0815 Max. kg/cm2A Min.
7 |Suction pressure kg/cm2A Flooded Flooded |Shut-off Head Mtr
8 |Differential pressure kg/cm2 2 3.5 Max. pump Heat @ Rated capacity
9 |Total Head m/c. 5 mt 5.5 End-of curve power
10 |Hydraulic Power kw Recommended Driver power
11 |NPSH available m/c. Min. Continuous Flow
12 |Efficiency of pump % OPERATION CONTINUOUS
13 |Power absorbed at Norma kw NPSH required at Pump suction Mtr
14 |Vertical pump suction nozzle distance to support plate Drive : V Belt
15 |Specification Standard Motor: 400+ 10% volts 3 Phase: 50 + 3% cycles
16 |[Manufacturer: Perferred speed: 1450 RPM Make: Supplied by: Purchaser
17 |Size & Type No. of Stages : 01
18 |Rotation: Clockwise/Anti-clockwise Looking on Coupling
19 |From Driver End
20 Materials Specification
21 |Casing IASTM A 351 CF 8M
22 |Impeller ASTM A 351 CF 8M
23 |Impeller wear ring NA
24 |Casing wear ring ASTM A 351 CF 8M Couplings : Make : NA
25 |Lanternring ASTM A 351 CF 8M Pump Thrust on Driver Bearings
26 |Neck-Bush base frame MS FAB.
27 |Shaft AISI 316 Cooling Water : No
28 |Shaft sleeve AISI 316 Temperature
29 |Balance Piston NA Pressure
30 |Gasket PTFE Quantity per Pump:
31 |Packing/Mech PTFE PTFE (For Bearings, Pedestals packing box, Driver, oil cooler)
32 |Coupling NA BEING V BELT Flushing Fluid : Water
33 |Bearings: Type : Radial: YES Thrust: V BELT DRIVE Quantity : Pressure : Temp.:
34 |Lubrication : Oil
35 |Force Feed Fluid Thrust balance connection to: Suction Nozzle
36 |Shaft : Horizontal Suction Source: Suction Line/ Suction Nozzle - Feed Tank
37 |Casing support: Foot, Centre Line, Driver, Piping C'Line
38 |Suction : Flange Size : Rating : Recirculation - Flow Reqd. : Yes/No
39 End, Side, Top, Botom Office NA : By Purchaser/ Vendor
40 |Discharge: Flange Size: Rating : Quantity : NA
41 End, Side, Top, Bottom
42  |Impeller Type: Semi Open Imp Dia (Rated/Max.) mm Vendor to Supply : Pulleys
43 |Specific Speed: Suc. Sp. Speed : - US-Unit |Vendor/ Purchaser to mount driver on bedplate
44 |Clearance : Wear Ring Later Neck Bush : Vendor to supply foundation bolts
45 |Packing/Mechanical Seal : Mechanical Seal Weights : Pump & Bedplate
46 |Make NA Type: -- Size:-- Driver Maintenance Lift
47 |Arrangement : -- Driver Drg. No.
48 |Material : Seal :  Slilicon Carbide NA Seat : General Arrangement Drg. No.
49 |Screwed Conns.: NA Performance Curve No.
50 |Specifications: NA Protection:  Attached
51 |Type of Casing Split : VERTICAL Casing Design Temp. = 150°C
Made By : Remarks:
Checked By: Reference P.D.S. No.

Approved By:

Date :








APTECH ENGINEERS,

DATA SHEET FOR SLURRY PUMP -lI

DATA SHT.NO.3d

DAI INDIA CONTRACT NO.: SHEET 2 OF 4 SHEETS
Main Item No. Plant : SALT PLANT
Total No. 1 |Working 1 \Stand by None Location: Indoor
1 |Service: Slurry Circulation Pump Drive : Motor
2 |Fluid : Brine Slurry 10% Area Classification : SAFE W R T ELECT HAZARDS
3 |Analysis/Solids content: - NaCl Crystals Pumping Temperature: Normal 80° C Max. 85°C Min.
4 |DUTY (each pump) Units Normal Rated |Specific Gravity : 1.2 Max. Min.
5 |Capacity m3/h 25 27 Viscosity, Centiposes 0.63 Max. Min.
6 |Discharge pressure kg/cm2A 2.5 3.5 Vapour pressure @ 42°C : 0.0815 Max. kg/cm2A Min.
7 |Suction pressure kg/cm2A Flooded Flooded |Shut-off Head Mtr
8 |Differential pressure kg/cm2 2 Max. pump Heat @ Rated capacity
9 |Total Head m/c. 5mt 7 End-of curve power
10 |Hydraulic Power kw Recommended Driver power Kw
11 |NPSH available m/c. Min. Continuous Flow M3/HR
12 |Efficiency of pump % OPERATION CONTINUOUS
13 |Power absorbed at Norma kw NPSH required at Pump suction Mtr
14 |Vertical pump suction nozzle distance to support plate Drive : V Belt
15 |Specification Standard Motor: 400+ 10% volts 3 Phase: 50 + 3% cycles
16 |Manufacturer: Perferred speed: 1450 RPM Make: Supplied by: Purchaser
17 |Size & Type No. of Stages : 01
18 |Rotation: Clockwise/Anti-clockwise Looking on Coupling
19 |From Driver End
20 Materials Specification
21 |Casing ASTM A 351 CF 8M
22 |Impeller ASTM A 351 CF 8M
23 |Impeller wear ring NA
24 |Casing wear ring ASTM A 351 CF 8M Couplings : Make : NA
25 |Lantern ring ASTM A 351 CF 8M Pump Thrust on Driver Bearings
26 |Neck-Bush base frame MS FAB.
27 |Shaft AlSI 316 Cooling Water : NO
28 |Shaft sleeve AlSI 316 Temperature NA
29 |Balance Piston NA Pressure NA
30 |Gasket PTFE Quantity per Pump: NA
31 |Packing/Mech PTFE PTFE (For Bearings, Pedestals packing box, Driver, oil cooler)
32 |Coupling NA BEING V BELT Flushing Fluid : Water
33 |Bearings: Type : Radial: YES Thrust: V BELT DRIVE Quantity : Pressure : Temp.:
34 |Lubrication : Oil
35 |Force Feed Fluid Thrust balance connection to: Suction Nozzle
36 |Shaft : Horizontal Suction Source: Suction Line/ Suction Nozzle - Feed Tank
37 |Casing support: Foot, Centre Line, Driver, Piping C'Line
38 |Suction : Flange Size : Rating : Recirculation - Flow Reqd. : Yes/No
39 End, Side, Top, Botom Office NA : By Purchaser/ Vendor
40 |Discharge: Flange Size: Rating : Quantity : NA
41 End, Side, Top, Bottom
42 |Impeller Type: Semi Open Imp Dia (Rated/Max.) mm Vendor to Supply : Pulleys
43 |Specific Speed: Suc. Sp. Speed : - US-Unit |Vendor/ Purchaser to mount driver on bedplate
44 |Clearance : Wear Ring Later Neck Bush : Vendor to supply foundation bolts
45 |Packing/Mechanical Seal : Mechanical Seal Weights : Pump & Bedplate
46 |Make NA Type: -- Size:-- Driver Maintenance Lift
47 |Arrangement : -- Driver Drg. No.
48 |Material : Seal :  Slilicon Carbide NA Seat : General Arrangement Drg. No.
49 |Screwed Conns.: NA Performance Curve No.
50 |Specifications: NA Protection :  Attached
51 |Type of Casing Split : VERTICAL Casing Design Temp. = 150°C
Made By : Remarks:
Checked By: Reference P.D.S. No.

Approved By:

Date :








APTECH ENGINEERS,

DATA SHEET FOR SLURRY PUMP -llI

DATA SHT.NO.3d

DAI INDIA CONTRACT NO.: SHEET 3 OF 4 SHEETS
Main Item No. Plant : SALT PLANT
Total No. 1 |Working 1 \Stand by None Location: Indoor
1 |Service: Slurry Circulation Pump Drive : Motor
2 |Fluid : Brine Slurry 20% Area Classification : SAFE W R T ELECT HAZARDS
3 |Analysis/Solids content: - NaCl Crystals Pumping Temperature: Normal 80° C Max. 85°C Min.
4 |DUTY (each pump) Units Normal Rated |Specific Gravity : 1.2 Max. Min.
5 |Capacity m3/h 15 17 Viscosity, Centiposes 0.63 Max. Min.
6 |Discharge pressure kg/cm2A 2.5 3.5 Vapour pressure @ 42°C : 0.0815 Max. kg/cm2A Min.
7 |Suction pressure kg/cm2A Flooded Flooded |Shut-off Head 22 Mtr
8 |Differential pressure kg/cm2 3 Max. pump Heat @ Rated capacity
9 |Total Head m/c. 15 mt 20 End-of curve power
10 |Hydraulic Power kw Recommended Driver power Kw
11 |NPSH available m/c. Min. Continuous Flow M3/HR
12 |Efficiency of pump % OPERATION CONTINUOUS
13 |Power absorbed at Norma kw NPSH required at Pump suction Mtr
14 |Vertical pump suction nozzle distance to support plate Drive : V Belt
15 |Specification Standard Motor: 400+ 10% volts 3 Phase: 50 + 3% cycles
16 |Manufacturer: Perferred speed: 1450 RPM Make: Supplied by: Purchaser
17 |Size & Type No. of Stages : 01
18 |Rotation: Clockwise/Anti-clockwise Looking on Coupling
19 |From Driver End
20 Materials Specification
21 |Casing ASTM A 351 CF 8M
22 |Impeller ASTM A 351 CF 8M
23 |Impeller wear ring NA
24 |Casing wear ring ASTM A 351 CF 8M Couplings : Make : NA
25 |Lantern ring ASTM A 351 CF 8M Pump Thrust on Driver Bearings
26 |Neck-Bush base frame MS FAB.
27 |Shaft AlSI 316 Cooling Water : NA
28 |Shaft sleeve AlSI 316 Temperature : NA
29 |Balance Piston NA Pressure © NA
30 |Gasket PTFE Quantity per Pump: NA
31 |Packing/Mech PTFE PTFE (For Bearings, Pedestals packing box, Driver, oil cooler)
32 |Coupling NA BEING V BELT Flushing Fluid : Water
33 |Bearings: Type : Radial: YES Thrust: V BELT DRIVE Quantity : Pressure : Temp.:
34 |Lubrication : Oil
35 |Force Feed Fluid Thrust balance connection to: Suction Nozzle
36 |Shaft : Horizontal Suction Source: Suction Line/ Suction Nozzle - Feed Tank
37 |Casing support: Foot, Centre Line, Driver, Piping C'Line
38 |Suction : Flange Size : Rating : Recirculation - Flow Reqd. : Yes/No
39 End, Side, Top, Botom Office NA : By Purchaser/ Vendor
40 |Discharge: Flange Size: Rating : Quantity : NA
41 End, Side, Top, Bottom
42 |Impeller Type: Semi Open|Imp Dia (Rated/Max.) 249 mm Vendor to Supply : Pulleys
43 |Specific Speed: Suc. Sp. Speed : - US-Unit |Vendor/ Purchaser to mount driver on bedplate
44 |Clearance : Wear Ring Later Neck Bush : Vendor to supply foundation bolts
45 |Packing/Mechanical Seal : Mechanical Seal Weights : Pump & Bedplate
46 |Make NA Type: -- Size:-- Driver Maintenance Lift
47 |Arrangement : -- Driver Drg. No.
48 |Material : Seal :  Slilicon Carbide NA Seat : General Arrangement Drg. No.
49 |Screwed Conns.: NA Performance Curve No.
50 |Specifications: NA Protection :  Attached
51 |Type of Casing Split : VERTICAL Casing Design Temp. = 150°C
Made By : Remarks:
Checked By: Reference P.D.S. No.

Approved By:

Date :








APTECH ENGINEERS,

DATA SHEET FOR BRINE PUMP

DATA SHT.NO.3d

INDIA SHEET 4 OF 4 SHEETS
DAI CONTRACT NO.:
Main Item No. Plant : SALT PLANT
Total No. 1 \Working 1 \Stand by None Location: Outdoor
1 |Service: Slurry Circulation Pump Drive : Motor
2 |Fluid :Brine Area Classification : SAFE W R T ELECT HAZARDS
3 |Analysis/Solids content: - NaCl Crystals Pumping Temperature: Normal 40° C Max. 15°C Min.
4 |DUTY (each pump) Units Normal Rated |Specific Gravity : 1.2 Max. Min.
5 |Capacity m3/h 25 27 Viscosity, Centiposes 0.63 Max. Min.
6 |Discharge pressure kg/cm2A 2 2.5 Vapour pressure @ 42°C : 0.0815 Max. kg/cm2A Min.
7 |Suction pressure kg/cm2A 0.2 0.3 Shut-off Head ~ Mtr
8 |Differential pressure kg/cm?2 3 3.5 Max. pump Heat @ Rated capacity
9 |Total Head m/c. 15 20 End-of curve power
10 |Hydraulic Power kw Recommended Driver power
11 |NPSH available m/c. Min. Continuous Flow
12 |Efficiency of pump % OPERATION CONTINUOUS
13 |Power absorbed at Normalkw NPSH required at Pump suction
14 |Vertical pump suction nozzle distance to support plate Drive : V Belt
15 |Specification Standard Motor: 400+ 10% volts 3 Phase: 50 + 3% cycles
16 |Manufacturer: Perferred speed: 1450 RPM Make: Supplied by: Purchaser
17 |Size & Type No. of Stages : 01
18 |Rotation: Clockwise/Anti-clockwise Looking on Coupling
19 |From Driver End \
20 Materials Specification
21 |Casing ASTM CF 8M
22 |Impeller ASTM A 351 CF 8M
23 |Impeller wear ring NA
24 |Casing wear ring ASTM A 351 CF 8M Couplings : Make : NA
25 |Lanternring ASTM A 351 CF 8M Pump Thrust on Driver Bearings
26 |Neck-Bush base frame MS FAB.
27 |Shaft AISI 316 Cooling Water : No
28 |Shaft sleeve AISI 316 Temperature
29 |Balance Piston NA Pressure
30 |Gasket PTFE Quantity per Pump:
31 |Packing/Mech PTFE PTFE (For Bearings, Pedestals packing box, Driver, oil cooler)
32 |Coupling NA BEING V BELT Flushing Fluid : Water
33 |Bearings: Type : Radial: YES Thrust: V BELT DRIVE Quantity : Pressure:  Temp.:
34 |Lubrication : Oil
35 |Force Feed Fluid Thrust balance connection to: Suction Nozzle
36 |Shaft: Horizontal Suction Source: Suction Line/ Suction Nozzle - Sett. Pond
37 |Casing support: Foot, Centre Line, Driver, Piping C'Line
38 |Suction : Flange Size : Rating : Recirculation - Flow Reqd. : Yes/No
39 End, Side, Top, Botom Office NA : By Purchaser/ Vendor
40 |Discharge: Flange Size: Rating : Quantity : NA
41 End, Side, Top, Bottom
42 |Impeller Type: Semi Open/Imp Dia (Rated/Max.) mm Vendor to Supply : Pulleys
43 |Specific Speed: Suc. Sp. Speed : - US-Unit |Vendor/ Purchaser to mount driver on bedplate
44 |Clearance : Wear Ring Later Neck Bush : Vendor to supply foundation bolts
45 |Packing/Mechanical Seal : Mechanical Seal Weights : Pump & Bedplate
46 |Make NA Type: -- Size:-- Driver Maintenance Lift
47 |Arrangement : -- Driver Drg. No.
48 |Material : Seal :  Slilicon Carbide NA Seat : General Arrangement Drg. No.
49 |Screwed Conns.: NA Performance Curve No.
50 |Specifications: NA Protection:  Attached
51 |Type of Casing Split : VERTICAL Casing Design Temp. = 150°C
Made By : Remarks:
Checked By: Reference P.D.S. No.

Approved By:

Date :
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APTECH DATA SHEET FOR
USAID ENGINEERS WASH TANK DATA SHT.NO. 3e
SOMALILAND SHEET 1 OF 6 SHEETS
VENDOR NAME.:
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USAID APTECH ENGINEERS DATA SHEET FOR WASH TANK DATA SHT.NO. 3e

SOMALILAND SHEET 2 OF 6 SHEETS
VENDOR NAME.:
PROCESS DATA
FLUID SALT SLURRY UNITS  JAUXILIARY FOR HEAT / COOL
MASS FLOW | 15000 kg/hr
OP. TEMPERATURE 30° C FLUID
TEMP. MIN / MAX. 20 45/C MASS FLOW
ABS. OP. PRESSURE ATM. bar OP. TEMP. IN
ABS. PRESS. MIN / MAX | bar OouT
VAPOUR PRESSURE - ABS. OP. PRESS.
AT C bar ABS. PRESSURE
BOILING TEMP AT 1 bar 110 C MIN.
MAC VALUE glcm3  |MAX.
FLASH POINT C
DENSITY 1450 kg/m3
OPERATING VOLUME 5.5 m3
MECHANICAL DATA

VESSEL TYPE: CYLINDRICAL SHELL O.D 1500 MM
HORIZONTAL / VERTICAL: VERTICAL CYLINDRICAL LEN. 1500 MM
OPEN /CLOSED: OPEN CONICAL LEN. 1065 MM

MIXER: YES / NO: YES

TYPE OF HEADS

CONICAL / FLAT

MIXER TYPE: BLADE TYPE RPM 20 ‘

TOTAL VOLUME 6 M3 CORR. ALLOWANCE

DESIGN TEMPERATURE 40 C HEATING / COOLING

ABS. DESIGN PRESSURE ATM. bar ‘ JACKET |COIL
INSULATION YES / NO NO DESIGN TEMP. C C
WEIGHT OF EMPTY TANK MT ABS. DESIGN PRES

ELEVATION  MIN. GL

LOCAT. INDOOR/OUTDOOR: INDOOR

HAZ. CAT. VESSEL

DESIGN CODE ASME JACKET
MATERIAL OF CONSTRUCTION

VESSEL SS 316 | \
VESSEL LINING / PAINT. EPOXY JACKET / COIL

INSUATION

GASKETS SEE PIPE SPECS.
1) REFER DRAWING
2) AISI SS 316
3) STIFFENERS TO BE ADVISED BY THE VENDOR
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USAID APTECH ENGINEERS DATA SHEET FOR ELUTRIATION TANK DATA SHT.NO. 3e

SOMALILAND VENDOR NAME - SHEET 4 OF 6 SHEETS
PROCESS DATA
FLUID SALT SLURRY UNITS AUXILIARY FOR HEAT / COOL
MASS FLOW 30000 ka/hr
OP. TEMPERATURE 30° C FLUID
TEMP. MIN / MAX. 20 40 C MASS FLOW
ABS. OP. PRESSURE ATM. bar OP. TEMP. IN
ABS. PRESS. MIN / MAX bar ouT
VAPOUR PRESSURE - ABS. OP. PRESS.
AT C bar ABS. PRESSURE
BOILING TEMP AT 1 bar 110 C MIN.
MAC VALUE g/cm3 MAX.
FLASH POINT C
DENSITY 1450 kg/m3
OPERATING VOLUME 5.5 m3
MECHANICAL DATA

VESSEL TYPE: CYLINDRICAL SHELL O.D 1500 MM
HORIZONTAL / VERTICAL: VERTICAL CYLINDRICAL LEN. 1500 MM
OPEN /CLOSED: OPEN CONICAL LEN. 1144 MM

MIXER: YES / NO: NO
MIXER TYPE: BLADE TYPE
TOTAL VOLUME

DESIGN TEMPERATURE
ABS. DESIGN PRESSURE
INSULATION YES / NO
WEIGHT OF EMPTY TANK
ELEVATION  MIN.

LOCAT. INDOOR/OUTDOOR: INDOOR

RPM

6 M3
40 C
ATM. bar

TYPE OF HEADS CONICAL / FLAT
CORR. ALLOWANCE
HEATING / COOLING

JACKET COIL
DESIGN TEMP. C C
ABS. DESIGN PRES

HAZ. CAT. VESSEL

DESIGN CODE ASME JACKET
MATERIAL OF CONSTRUCTION

VESSEL SS 316

VESSEL LINING / PAINT. EPOXY JACKET / COIL

1) REFER DRAWING
2) AISI SS 316

3) STIFFENERS TO BE ADVISED BY THE VENDOR

INSUATION

GASKETS SEE PIPE SPECS.








DATA SHEET FOR
USAID APTECH ENGINEERS DATA SHT.NO. 3e

THICKNER
SOMALILAND SHEET 5 OF 6 SHEETS

VENDOR NAME.:
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USAID APTECH ENGINEERS DATA SHEET FOR THICKNER DATA SHT.NO. 3e

SOMALILAND SHEET 6 OF 6 SHEETS
VENDOR NAME.:
PROCESS DATA
FLUID SALT SLURRY UNITS  JAUXILIARY FOR HEAT / COOL
MASS FLOW | 20000 kg/hr
OP. TEMPERATURE 30° C FLUID
TEMP. MIN / MAX. 20 40/C MASS FLOW
ABS. OP. PRESSURE ATM. bar OP. TEMP. IN
ABS. PRESS. MIN / MAX | bar OouT
VAPOUR PRESSURE - ABS. OP. PRESS.
AT C bar ABS. PRESSURE
BOILING TEMP AT 1 bar 110 C MIN.
MAC VALUE glcm3  |MAX.
FLASH POINT C
DENSITY 1450 kg/m3
OPERATING VOLUME 9 m3
MECHANICAL DATA
VESSEL TYPE: CYLINDRICAL SHELL O.D 1500 MM
HORIZONTAL / VERTICAL: VERTICAL CYLINDRICAL LEN. 1500 MM
OPEN /CLOSED: OPEN CONICAL LEN. 955 MM
MIXER: YES / NO: NO TYPE OF HEADS CONICAL / FLAT
MIXER TYPE | RPM \
TOTAL VOLUME 9 m® CORR. ALLOWANCE
DESIGN TEMPERATURE 40 C HEATING / COOLING
ABS. DESIGN PRESSURE ATM. bar | JACKET | COIL
INSULATION YES / NO NO DESIGN TEMP. C C
WEIGHT OF EMPTY TANK MT ABS. DESIGN PRES
ELEVATION  MIN. M
LOCAT. INDOOR/OUTDOOR: INDOOR HAZ. CAT. VESSEL
DESIGN CODE | ASME JACKET
MATERIAL OF CONSTRUCTION
VESSEL SS 316 | \
VESSEL LINING / PAINT. EPOXY JACKET / COIL
INSUATION
GASKETS SEE PIPE SPECS.

1) REFER DRAWING

2) ABOVE CENTRIFUGE

3) AISI SS 316

4) STIFFENERS TO BE ADVISED BY THE VENDOR
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Title:

APTECH CLIENT:
engiINEERS | SLURRY  FORMATION TANK USAID-SOMALILAND

750

g 1_ {N1)
tA' d=—f ’Aj‘
{N2)
N2 100 NB | SLURRY DISCHARGE
N1 150 NB | SLURRY OVERFLOW
CONN. SIZE SERVICE
PLAN MARK NB.
BRINE INPUT THROUGH NOZZLE SCHEDULE

FLEXIBLE HOSE

- 2
He

1000

N
N

750

VIEW 'A'="A’

NOZZLE ORIENTATION ON HOLD

NOTES

1. ALL DIMENSIONS ARE IN MM.
2. 3MM THICK $S316 TO BE USED TO FABRICATE THE WALLS OF TANK UNLESS SPECIFIED.

Date Name Checked Date Q b C d e












3f.Datasheet-Screw Conveyor.pdf

DATA SHEET No

o ILAND Aptech Engineers DATASHEET FOR SCREW CONVEYOR af
SHEET 1of 1
Sr No Technical Parameters Data
Transport Salt from Centrifuge Discharge &
1 Application Blending Potassium lodate Soution to salt
2 Quantity 1No
3 Process Parameters
a. Product Common Salt
b. Function Blending & Conveying
c. Operation Continuous
d. Operating conditions Ambient, 50 °C, Closed Shed
e. Capacity (Operating) 2.5 Metric Tons / hr
Capacity (Max.) 3 MT/Hr
f. Feed (Input) Size All below 1 mm
g. Feeding System Centrifuge Discharge to the inlet Salt Hopper
h. Agglomerates May be present in soft cake form
i. Hard Lumps NIL
. Moisture 3.0t03.5%
k. Bulk Density 1200 kg/M®
l. Power Condition 400 Volts, 3-Ph, 50 Hz
4 Screw Design
Horizontal, Covered Paddle mixer and
a. Type Conveying Screw
b. MOC SS 316
c. Inclination Angle NIL
d. MoC SS 316
e. Length of Trough c/c 10 M Appox.
f. Screw Diameter 295 mm
g. Thickness of Flights Screw 5mm, Casing 3mm. Min.
h. Shaft Type & MOC Hollw, with shrink fit Stub Ends, EN 8
i. Shaft Diameter 75 mm
. Drive Motor
k. Gear Box Make Reputed
l. Gear Ratio 01:20
m. Transmission of Main Drive C-Section V-Belt & 2-Groove Pulley
n. Drive Arrangement Location On Product Discharge Side
o. Bearing type and Size
p. No of Discharge points 3
Two nos to feed pouch packing cup fillers and
one at the end with inverted Y chute for bulk
q. Dischage Ends bagging
5 MS Supports
a. To be painted with Epoxy paint.
6 Covers, Guards Safety Etc
a. Provide all safety & guards etc.
b. Bearig Blocks to be Covered

Please fill up Blanks in the sheet
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USAID Aptech Datasheet for Centrifuge Datasheet No 3g
SOMALILAND Engineers 2.5 TPH Capacity Sheet 1 of 4
Sr No. Item Particulars

1 Process Data:

a. Feed Material Salt Slurry in Brine

b. Mass Flow

i Normal 5 MT/Hr.

ii. Max. 7 MT/Hr.

C. Brine flow 2.5 M*/ hr

d. Temperature 40 °C

e. Pressure ATMr

f. Moisture Content 40%

g. Maximum size 1 mm

Particle size distribution

90% Below 1 mm, 10%
Between 1 — 2 mm

Overall Dimensions (LXBXH) mm
Filtration
Screen Design

Media
Area Outer Basket

Area Inner Basket

h.

i Slurry concentration (Min. / Max.) w/w 40/ 60 %

- Density 1450 Kg/M®

k. Viscosity 0.60 Centipoise
l. Feeding Device Thickener

m. Capacity 2.5 TPH

n. Discharge To lodisation Screw
0. Installation Indoor

p. Electricity 400 V, 3-Ph, 50 Hz
2 Machine Type

a. Type Hydraulic Pusher Centrifuge
b. Model No.

C. Quantity One

d. Design

€. No. of Stages Two

f. Moisture Content in the Discharge Product

3 Model Particulars

a. Capacity (Nor./Max) TPH 2.5/3 TPH

b. Feed Condition Required

C. Nominal Diameter

d. Height of centre of Rotor from the Base

e. Height of centre of gravity of machine from

f. Top of Qil level when full in the oil sump

a. Net Weight Kg Max

h.

4

a.

b.

C.

d.








USAID
SOMALILAND

Aptech Datasheet for Centrifuge
Engineers 2.5 TPH Capacity

Datasheet No 3g
Sheet 1 of 4

Cake Thickness (Max. / Min.) mm
Basket & Screens

2" Screen (Outer) Dia.

Length

Slot Width

1% Screen (Inner) Dia.

Length

Slot Width

Moment of Inertia (Unloaded Basket)

G — Value
Maximum
Normal

Basket Speed
Operating Speed
Maximum Speed

Pusher Device
Pusher Mechanism
Length of Stroke (Nor. / Max.) mm

No. of Strokes / Min
Diameter of Shaft

Bearings
Hydraulic Device
Oil Sump Capacity

No. of chambers in oil sump
Oil Pressure Max. / Op.
Oil Pump Type

Oil Cooler Type

MOC and construction of Oil Cooler
Operating Temp.

Cooling Water req. (Ipm)

TP HETe 0000 ROPR0TPONTRNTYOQ D 20T PO

Drive Details
Drive Motor
Pusher Motor








USAID Aptech Datasheet for Centritfuge Datasheet No 3g
SOMALILAND Engineers 2.5 TPH Capacity Sheet 1 of 4
11 Transmission
Main Drive

Pusher Drive

Main Drive- No. of Grooves on Pulley
Screw Pump Drive side - coupling etc.
Lubrication

N

Accessories — Control, indicators, alarms
Material of Construction

Bearing Housing
Process Housing
Basket

Pusher Plate
Pusher Ring
Slotted Screens

Feed Accelerator

Feed Cone
Pusher Shaft

Main Shaft

Volute Race
Scrapper Blades
Feed Pipe

Wash & Rinse Pipes
Flat Seals
Round Seal Rings

"eTos3—FAe-mTer0o00T 000 oo

Radial Shaft Sealing Rings
Sealing Discs

13 Surface Finish
a. CS

b. SS

14 Scope of Supply

Basic Machine
Base Frame

Anti Vibration Pads

Electrical Motors
Electrical Panel

Belts, Pulley, Guards etc.

Feed & Discharge Chutes








USAID
SOMALILAND

Aptech
Engineers

Datasheet for Centritfuge
3 TPH Capacity

Datasheet No 3g
Sheet 1 of 4

h.

Instrumentation
Spares
Tool Kit

i.
i
K.
l.
m

Erection Manual

Operating Manual

Maintenance Manual

Note: All blanks to be filled up by

Vendor
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USAID APTECH DATA SHEET FOR DATA SHEET. NO:3h
SOMALILAND ENGINEERS PACKING MACHINE
Vendor Name: Sheet 1 of 2 Sheets
Sr. No. Description Units
1. Item No.
o Type of Equipment Volumetric Feed Packing Machine
3. Model & Size
4. Quantity Nos 2
5 Purpose Packing Wet Salt
6. Process Data:
6.1 Feed Material Salt Granules
a. Mass Flow 2 MT/Hr
Normal | MT/Hr. 2 MT/Hr.
Design | MT/Hr. 2.2 MT/Hr.
b. Temperature °C 35 °C
C. Pressure ATM Atmospheric
d. Moisture Content v 3-4% Max
e. Particle size Max. mm 2
f. Maximum lump size mm Rare
7 Design Data
Mechanical Design
Requirements
a. Design Temperature °C 50 °C
b. Design Pressure ATM Atmospheric
C. Installation In Door








USAID APTECH DATA SHEET FOR DATA SHEET. NO:3h
SOMALILAND | ENGINEERS PACKING MACHINE
Vendor Name: Sheet 2 of 2 Sheets
Sr. No. Description Units
d. Operation Continuous
8. Material of Construction Contact Parts SS 316 , CS
a. Pedestal CS (Epoxy Painted)
b. Motor Power and RPM
9. Weight of Machine *Kg.
10. Weight of heaviest single piece | *Kg
*Mx
a. Space reqd. for Packing Machine
mxm
. Material coming from the
b. Feeding System screw conveyor will feed the
two Packing machines.
Notes:
1. Supplier to submit duly filled in data sheet along with bid.
2. Blanks To be stated / confirmed by supplier.
3. Inserts with the cups to be provided for packing 500 gram pouches
4. Supply to include 6 Nos hand sealers.
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USAID

SOMALILAND Aptech Engineers

Datasheet for lodate Dosing System

Datasheet
No 3i
Sheet 1 of 2

AGITATOR WITH
LEARED MDTDR\\\

I0DATE
SOLUTION TANK

HEATER

DOSING
PUMP

TO CENTRIFUGE








USAID

Datasheet

SOMALILAND Aptech Engineers Datasheet for lodate Dosing System No 3i
Sheet 1 of 2
Sr No Item Description

1 Application Dosing 2-3% Potassium lodate Solution to Salt

a. Product Potassium lodate Powder

b. Feed (Input) Size 0.5 mm Max.
Potassium lodate Holding Tank and Centrifugal

C. Feeding System Pump

d. Lumps No

e. Moisture 3.0t0 3.5%

f. Output Potassium lodate Solution in Water

g. Operation Continuous

h. Application Indoor

i. Ambient Conditions Maximum 35° C ambient

j- Power 400 Volts, 3-Ph, 50 Hz

2 System Components

2.1 Dosing Pump

a. Type of Pump Centrifugal (Reputed make)

b. Capacity Oto5ltr/hr

c. Contact Parts SS 316

d. Drive (Make) 3-Phase, 0.5 hp, 1440 rpm (Reputed)
The pump to feed Solution from the tank to the

e. Operation Nozzle at Centrifuge Discharge Chute
The Dischage to be regulated with Valve.
Excess Solution to be sent Back to Solution

f. By Pass Arrangement Tank

g. Filter In line filter to trap solids

2.2 K103 Tank (Cylindrical)

a. Type Cylindrical, with Openable Cover

b. MOC SS 316

C. Capacity 100 ltrs

d. Thickness 2mm

e. Heater & Thermostat 2 kW to be provided at the Bottom, 80° C

Agitator

Agitator to be provided with 0.5 HP Geared
Motor












3a.Feed Hopper.pdf

1500

350

50 x 10 MM SS PLATE ALL ARGUND

TO SUPPORT GRIZLY SCREEN BAR

900

150

200

200

150

50 x 10 MM SS PLATE ALL ARGUND

15MM THICK PLATE

TO SUPPORT GRIZLY SCREEN BAR

ELEVATION
1500
150,200, R 8| 200, |50
]
S
o~
150 150, 150
5 150 m
150 150
S
o~
2
£=J (=]
150] |200] ¥ @l [200] [150
PLAN
900
50, Y]
&l
S
o
a
VIEW 'C" - '(C

150 x 200

150

15MM THICK PLATES

S

i 1
15
N & 150 200
\ 5 A
d—dr 15MM THICK PLATE
R .>. D / q m 210
Eal ﬁ_w AN B \ o ShB BYs
B0} 15MM THICK PLATE rl o X
155 x 210 o ] &
5 200 5 .
s 51 100 155 4NOS. 22¢ HOLES FOR 20 ¢ BOLTS
DETAIL OF BRACKET VIEW ‘A" - "A’ VIEW 'B' - 'B’

’ ._
E

430

65

300 65

150 x 25 MM SS PLT

150

25

‘o
65

280
150

o |

65

5MM THK. (BOTH SIDES)

15 x 25MM SSPLT

lw _ \ 70MM THK.
” \ 65 x 3 MM THK. PLT 65, 1O 65
Q 12 ¢ DIA BOLT ALL AROUND 6 300 6 o [ A_\.H-hr 25
E h o] R 69 x 5 MM THK. SS PLT
I NUT FOR 12 @ DIA BOLT i A 4 \ ALL AROUND
WELDED WITH PLATE <l /ao x 140 MM SS PLT
” 3MM THK.
DETAIL GATE VALVE SECTION ‘D" - 'D’ SECTION 'E" - "E’
800
100 , 100 , 100 , 100 , 100 , 100 , 100 , 100
NOTES
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1. ALL DIMENSIONS ARE IN MM
2. MM THICK SS316 PLATE TO BE USED TO FABRICATE
THE WALLS OF FEED HOPPER UNLESS SPECIFIED.

10MM DIA SS ROD 3. STIFFENERS TO BE ADVISED BY VENDORS
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Aptech Datsheet for Raw Salt Belt Conveyor DATA SHT.NO. 3b
Engineers SHEET 1 OF 4
Vendor Name:
TECHNICAL PARAMETERS UNIT DATA
Quantity 1 No
Type Inclined
Purpose Transport
Operation Continuous
Operating Time Hr/Year 7000
Operating Environment Open to Air
Transfer One Way
No. of Feed Points One
No. of Unloading Points One
Feeding Device Hopper
Capacity
Nominal tph 3
Design tph 4
Characteristics of Material
Material Raw Salt
Nature - Flake/Prill/Granulate/Crystal/Lump Granulate
Maximum Grain Size mm 10
Average Grain Size mm 3to5
Presence of Lumps Rare/Occasional/Frequent Occasional
Maximum Lump Size mm 100
Moisture % wt 4-5%
Bulk Density Mt/Cumt. 996
Temperature Cc Ambient - 45
Pressure Sea Level
Abrasiveness High/Medium/Low Medium
Corrosiveness Severe When Wet
Flowability - Exellent/Good/Fair/Bad Good
Cohesiveness - High/Medium/Low Low
Static Angle of Repose 25 Degrees

Dynamic Angle of Repose

15 Degrees








Aptech Datsheet for Raw Salt Belt Conveyor DATA SHT.NO. 3b

Engineers SHEET 2 OF 4
Vendor Name

Structural Data

Centre to Centre Distance ' Mtr 10 Approx

Feed Point Salt Hopper Bottom 2.0 Mir below Ground
Delivery Point _ Salt Roller Crusher 2.0 Mtr above Ground
Supports to Rest on _ Ground Level

Belt Cover No

Provision for Belt Weigher No

Type of tensioning Device Screw

General

Belt Width mm 300

Belt Speed - Normal m/Sec 0.22 Approx

CI/C Distance _ m 10 Mtr | Approx
Skirtboard Length _ m 1

Skirtboard Thickness mm 100

Deck Plate Length m 1.2

Deck Plate Thickness mm 5

Idler Details

Carriying Idlers

Tube Dia X Thickness mm X mm 75 X3
Spacing m 0.75
Bearing Size, Type, Make Std
Spindle Type Std

Return Idlers

Tube Dia X Thickness mm X mm 75 X3

Spacing m 15 One near I_Each Drum
Pulley is must

Bearing Size, Type, Make Std

Spindle Type Std








Aptech Datsheet for Raw Salt Belt Conveyor DATA SHT.NO. 3e
Engineers SHEET 3 OF 4
Vendor Name
Belting
Material White, Rubber
Make Std
Type Flat
Rating 4 Ply Min
Grade (Food Grade) *
Top Cover Thickness mm 5
Bottom Cover Thickness mm 3
Drive Pulley Diameter | mm 300
Shaft Diameter at Hub _ mm 50
Bearing Type Ball
Tail Pulley Diameter mm 250
Shaft Diameter at Hub mm 50
Bearing Type Ball
Scrappers
Location At Discharge
Type Nylon/FG PVC

Magnets Enclosed in SS 316 Casing

No. of Magnets 1

Location of Magnets Middle
Size mm X mm 300 X 200
Max. size of object it can attract mm X mm 150
Distance of Attraction ' mm 100








Datsheet for Raw Salt Belt Conveyor

Aptech DATA SHT.NO. 3e
Engineers SHEET 4 OF 4
Vendor Name
Drive Details
Power at Pulley Shaft kW *
Motor Rating at 50 C HP *
Make Reputed
Applicable Standard IP55
Speed rpm 1440
Protection of Enclosure Cover
Gearbox Details
Type Worm / Spur Specify
Ratio 1:20
Make Reputed

Transmission

Type Chain & Sprocket
Make Std

Size As Required
Painting All CS Epoxy Painted
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			LIST OF PLANT MACHINERY FOR 2.5 TPH SALT REFINERY





			Sr. No.


			Item Description


			Qty.


			MOC


			Ref Drg. / Datasheet No.


			POWER (kW)





			A.


			Raw Salt Feed Section


			


			


			


			





			1


			Feed Hopper


			1 No


			SS 316


			3a


			





			2


			Gate Valve


			1 No


			SS 316


			


			





			3


			Flat Raw Salt Belt Conveyor (300 mm wide, centre to centre distance = 10 mtrs. Approx, complete with Magnets, skirt, scrappers and discharge hood)


			1 No.


			Food Grade Rubber


			3b


			Pl. Specify





			4


			Raw Salt Roll Crusher (2.5 TPH, Feed 10 mm Max, Product below 3 mm)


			1 No


			CI Chilled Rolls


			3c


			Pl. Specify





			B.


			Wet Section


			


			


			


			





			1


			Slurry formation Tank Size 1.5 M High X750 mm Wide X 750 mm Long


			1 No.


			SS 316


			3ei


			





			2


			Slurry Pump-I (30% solids, 5 mlc, 10,000 LPH, SS 316 wetted parts, Mechanical seal, 1500 RPM)


			1 No.


			SS 316


			3d


			Pl. Specify





			3


			Wash Tank with Agitator


			1 No.


			SS 316


			3e


			Pl Specify





			4


			Slurry Pump-II (10% solids, 5 mlc, 25,00 LPH, SS 316 wetted parts, Mechanical seal, 1500 RPM)


			1 No.


			SS 316


			3d


			Pl. Specify





			5


			Elutriation Tank


			1 No.


			SS 316


			3e


			





			6


			Slurry Pump-III (20% solids, 5 mlc, 15,00 LPH, SS 316 wetted parts, Mechanical seal, 1500 RPM)


			1 No.


			SS 316


			3d


			Pl. Specify





			7


			Brine Pump (15 mlc, 25,00 LPH, SS 316 wetted parts, Mechanical seal, 1500 RPM)


			1 No.


			SS 316


			3d


			Pl. Specify





			8


			Brine Header


			1 No.


			SS 316


			


			




















Annexure - 1 (Cont.)





			LIST OF PLANT MACHINERY FOR 2.5 TPH SALT REFINERY





			Sr. No.


			Item Description


			Qty.


			MOC


			Ref Drg. / Datasheet No.


			POWER (kW)





			C.


			Centrifuge Section


			


			


			


			





			1


			Thickener


			1 No.


			SS 316


			3e


			





			2


			Pusher Type Hydraulic, 2-stage Centrifuge 2.5 TPH (Process side SS 316)


			1 No.


			SS 316


			3g


			Pl Specify





			3


			Washed Salt Paddle Screw Conveyor (200 mm wide, centre to centre distance = 10 mtrs. Approx, with Cover and three discharge outlets)


			1 No.


			SS 316


			3f


			Pl Specify





			D.


			Dosing Section


			


			


			


			





			1


			Dosing Tank with Agitator (100 Lit)


			1 Nos.


			SS 316


			3i


			Pl Specify





			2


			Dosing Pump (SS 316, 5 LPH)


			1 Nos.


			SS 316


			3i


			Pl. Specify





			E


			Packaging Section


			


			


			


			





			1


			Volumetric Cup Fillers


			2 Nos


			SS 316


			3h


			Pl. Specify





			2


			Hand Sealers


			6 Nos


			Std


			3h


			Pl. Specify





			F


			Others


			


			


			


			





			1


			Magnets before Roller Crusher and after centrifuge


			1 No Each


			SS 316 Casing


			


			





			2


			Electrical Panel with capacitor bank, Indicator lights, Single phase preventer, Ammeter, Voltmeter and PF meter


			1 No


			Std


			


			





			3


			Local ON/OFF Push switches, Cables, Glands, Cable trays, Earthing plate, Earth Strip & Wire


			Al./ Cu


			


			


			





			4


			Piping, Hangers & Supports, Valves and Instrumentation


			1 Lot


			Food Grade PVC, HDPE, Std.


			


			





			5


			Lab Equipment


			1 lot


			Std.


			


			





			


			Total Connected Power


			


			


			


			Pl Specify








[bookmark: _GoBack]






4.Typical Raw Salt Specifications.pdf

TYPICAL RAW SALT SPECIFICATIONS

TEST UNIT RESULTS METHOD REF.
SALT (ON DRY BASIS) % 98.23 AOAC - 937.09
MOISTURE % 1.38 AOAC - 945.15
SULPHATE % 0.18 AOAC - 980.02
MAGNESIUM ppm 2715 AOAC - 2011.14
CALCIUM ppm 1286 AOAC - 2011.14
ACID INSLUBLE ASH % Not Detected AOAC - 920.72
IRON ppm Not Detected AOAC - 2011.14
COPPER ppm Not Detected AOAC-2011.14
ARSENIC ppb Not Detected AOAC - 2011.14
LEAD ppb Not Detected AOAC - 2011.14
MERCURY ppb Not Detected AOAC - 2011.14
PHYSICAL TEST NORMAL VISUAL
90% BETWEEN 3-5 MM, Lumps
PARTICLE SIZE % Occasional 25 mm max VISUAL
IMPURITIES % 0.34 GRAVIMETRIC
COLOR Grayish White (Not Refined) VISIBLE
SMELL OK SENSORY
TASTE TYPICAL SENSORY












1.Flow Chart.pdf
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2.Site Layout.pdf
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