
	                   STATE OF KANSAS           

	Quotation #:
	«PROP_NUM»

	    REQUEST FOR QUOTATION  
	Date Mailed:
Closing 2:00 PM:

	«MAIL_DATE»
«CLOSE_DATE»

	                                 SUBMIT BID TO        
                        DIVISION OF PURCHASES
                    900 SW JACKSON, ROOM 102N
                     TOPEKA, KANSAS  66612-1286            
It shall be the vendor’s responsibility to monitor this website
on a regular basis for any changes/addenda.
http://www.da.state.ks.us/purch/rfq/ 

        This Space for Bidder’s Name and Address











     THIS IS NOT AN ORDER                                             
	
1.     When communicating, always refer to the above quotation number.

2.     To receive consideration for award, one copy of the “Request for Quotation,”
        properly completed and signed, must be returned to and received by the Division of 
        Purchases no later than the specified closing time.

3.     All prices, terms, and conditions shall be shown. Prices, terms, and conditions
        not shown or presented after closing will not be considered in the evaluation.

4.     Prompt payment discounts will not be considered in determining the low bid.

5.     Prices quoted shall be less Federal Excise and State Sales tax.

6.     The Director of Purchases reserves the right to accept or reject any part of this 
        quotation.

7.     Bid results will not be given to individuals over the phone. Results can be obtained
        by attending the public bid opening.  If unable to attend the public bid opening, bid
        tabulations can be obtained in person for $3.00. Bid results can also be obtained by
        sending (do not include with bid) a check for $3.00 payable to the State of Kansas,
        with a self addressed, stamped envelope to the Kansas Division of Purchases, Attn:
        Bid Results/Copies, 900  SW  Jackson,  Room  102-N,  Topeka,  KS    66612. Please
        reference quote number on check. Copies of individual bids may be obtained under 
        the Kansas Open Records Act by calling  (785) 296-0002, requesting an estimate of 
        the cost to reproduce the documents, and remitting that amount to the above address.
        Upon receipt of the funds, the documents will be sent.

8.     Faxed bid responses are not acceptable for bids in excess of $25,000. 
        FAX: (785) 296-7240

9.   I hereby certify that I(we) do not have any substantial conflict of interest sufficient to 
        influence the bidding process on this bid.  A conflict of substantial interest is one 
        which a reasonable person would think would compromise the opening bidding process.


	Prices are to be delivered FOB Destination Prepaid & Allowed:
	 «BILL_TO»

	Purchase Requisition Number(s):
	«PR_NUM»

	
For Additional Information Contact:
	«CON_PER»
	«CON_PHONE»

	[image: ]
    QUANTITY
    AND UNIT
	
                              ITEMS AND SPECIFICATIONS
	
     UNIT
   PRICES
	
     TOTAL
     PRICE





	
	
	TRUCK ACCESSORIES

	
	
	

	
	
	Bidders shall submit one original and one copy of their bid response to the Division of Purchases. 

	
	
	

	
	
	

	
	
	Pricing to be based on the State being responsible for delivering the vehicles to the vendors installation location.  The truck dealer located in Shawnee, KS, charges $1.50 per mile to deliver the vehicles, this cost will be added to the bidder’s pricing to determine the lowest total cost.  The bidder will be responsible for delivering the completed trucks to the KDOT destination.

	
	
	

	
	
	Show installation location:___________________________________

	
	
	

	
	
	Show mileage from Shawnee, KS to the installation location:
________________ miles.

	
	
	

	
	
	

	
	
	As an Alternate Bid, show the amount to add per truck if the bidder is
responsible for transporting the KDOT trucks from the Ford truck dealer
in Shawnee, KS to the installation site: Add $___________________ per
truck.  The vendor will be responsible for inspecting the vehicles for
damage prior to transporting and not accepting any damage vehicles.

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	Transporting the trucks by the vendor may be accomplished by transport
truck or by driving the vehicle.  Vendor will provide coverage to cover loss or damage to the vehicle while in the vendor's possession prior to taking possession of the trucks.

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	Equipment to be furnished and installed in accordance with Specification
No. MS 217.01, dated 11/18/09, and shall be equipped with the features
noted on page 2 of the above referenced specifications and the items listed for each vehicle.

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	PR# 017736, KDOT PR# 476812

	
	
	Delivery to Topeka, KS.

	
	
	

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford
F-250 Cab, Fleetside Pick-up Truck.

	
	
	

	
	
	

	
	
	To include: Black Tool Box for Fleetside body, L-Shaped Fuel Tank, Grille Guard, Light Bar Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford F-250 Regular Cab, Fleetside Pick-up Truck.

	
	
	

	
	
	To include: Black Tool Box for Fleetside boy, Grille Guard, Light Bar
Rack, Light Bar.

	
	
	

	
	
	

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford F-250 Regular Cab, Fleetside Pick-up Truck.

	
	
	

	
	
	To include:  Black Tool Box, for Fleetside body, L-Shaped Fuel Tank,
Grille guard, Light Bar Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford F-250 Regular Cab, Fleetside Pick-up Truck.

	
	
	

	
	
	To include: Black Tool Box for Fleetside body, L-Shaped Fuel Tank,
Grille, Guard, Light Bar Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford F-250 Cab and Chassis Truck.

	
	
	

	
	
	To include Utility Bed,  Rectangular Fule Tank, Grille Guard, Light Bar
Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford F-250 Cab and Chassis Truck.

	
	
	

	
	
	To include:  Utility Bed, Grille Guard, Light Bar Rack, Light Bar.

	
	
	

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford F-250 Cab and Chassis Truck.

	
	
	

	
	
	To include:  Utility Bed, Rectangular Fuel Tank, Grille Guard, Light Bar
Rack, Light Bar, DMI Temperature Unit.

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	

	
	

	
	
	PR # 017754, KDOT PR #476303
Delivery to Salina, Kansas

	3
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford
F-250 Cab and Chassis Truck.

	
	
	

	
	
	

	
	
	To include:  Utility Bed, Rectangular Fuel Tank, Grille Guard, Light Bar
Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	
	
	PR# 017755, KDOT PR# 476415
Delivery to Chanute, Kansas

	4
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford
F-250 Cab and Chassis Truck.

	
	
	

	
	
	

	
	
	To include:  Utility Bed, Rectangular Fuel Tank, Grille Guard, Light Bar
Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	
	
	PR# 017757 KDOT PR# 479306
Delivery to Hutchinson, Kansas

	3
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford
F-250 Cab and Chassis Truck.

	
	
	

	
	
	

	
	
	To include:  Utility Bed, Rectangular Fuel Tank, Grille Guard, Light Bar
Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford F-250 Regular Cab, Fleetside Pick-up Truck.

	
	
	

	
	
	To include:  Tool Box, L-Shaped Fuel Tank, Grille Guard, Light Bar Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	
	
	PR# 017758 KDOT PR# 478976
Delivery to Garden City, Kansas

	1
	Each
	Vendor Furnished & Installed Accessories for KDOT Owned 2010 Ford
F-250 Regular Cab, Fleetside Pick-up Truck.

	
	
	

	
	
	

	
	
	To include:  Tool Box, L-Shaped Fuel Tank, Grille Guard, Light Bar
Rack, Light Bar, DMI, Temperature Unit.

	
	
	

	
	
	

	
	
	Show additional unit cost of the following options if not previously specified:

	
	
	

	
	
	Black color powder coat paint on toolboxes: $___________________

	
	
	

	
	
	10 inch step bumper in lieu of 8 ½ inch on utility bodies: $____________

	
	
	

	
	
	Grille guard mounting hardware required for trucks without tow hooks:
$__________________

	
	
	

	
	
	Bidders must return with the bid the attached specifications properly completed showing any and all exceptions.

	
	
	

	
	
	The brand names shown are given only to assist in identifying the type and quality of product required.  Bids on comparable brands are invited.






The specifications were written with the intent of permitting competitive bidding.  The Division of Purchases reserves the right to waive minor deviations in the specifications which inadvertently restrict bidding to a single manufacturer (or vendor) or when such deviations do not alter nor deter the Agency from accomplishing the intended use or function.  However, it shall be the bidder's responsibility to advise the Division of Purchases of any specifications, language, other requirements, or any combinations thereof, which restricts or limits bidding.  Such notification must be submitted in writing and must be received by the Division of Purchases no later than five (5) days prior to the bid closing.  Each bid shall include descriptive literature and specifications on the product bid.  However, the providing of this material shall not be considered a substitute for listing deviations.

	
	
	

	
	
	POLITICAL SUBDIVISION USAGE
Political Subdivisions throughout the State (City, County, School District, etc.) are permitted to utilize contracts administered by the Division of Purchases if agreed to by the contractor.

	
	
	

	
	
	The State has no responsibility for payments owed by the political sub-divisions.  The vendor must deal directly with the political subdivision.

	
	
	

	
	
	Awards shall not be based on which of these statements is selected.  However, conditions included in this contract shall be the same for political subdivisions unless stated otherwise below:

	
	
	

	
	
	Indicate below, by checking () one of the boxes, if you will or will not extend pricing to Political Subdivisions.  Refusal will not be a determining factor in the award of this contract.

	
	
	

	
	
	· Yes, pricing is available to Political Subdivisions of the State of 	Kansas.

· No, pricing is not available to Political Subdivisions of the State 	of Kansas.

	
	
	

	
	
	If yes, for what time period and are there any additional restrictions or conditions?

_________________________________________________________________

_________________________________________________________________

_________________________________________________________________




	                   STATE OF KANSAS           

	Quotation #:
	12731

	    REQUEST FOR QUOTATION  
	Date Mailed:
Closing 2:00 PM:

	12/16/2009
1/5/2010

	                                 SUBMIT BID TO        
                        DIVISION OF PURCHASES
                    900 SW JACKSON, ROOM 102N
                     TOPEKA, KANSAS  66612-1286            
It shall be the vendor’s responsibility to monitor this website
on a regular basis for any changes/addenda.
http://www.da.ks.gov/purch/ 

        This Space for Bidder’s Name and Address











     THIS IS NOT AN ORDER                                             db
	
1.     When communicating, always refer to the above quotation number.

2.     To receive consideration for award, one copy of the “Request for Quotation,”
        properly completed and signed, must be returned to and received by the Division of 
        Purchases no later than the specified closing time.

3.     All prices, terms, and conditions shall be shown. Prices, terms, and conditions
        not shown or presented after closing will not be considered in the evaluation.

4.     Prompt payment discounts will not be considered in determining the low bid.

5.     Prices quoted shall be less Federal Excise and State Sales tax.

6.     The Director of Purchases reserves the right to accept or reject any part of this 
        quotation.

7.     Bid results will not be given to individuals over the phone. Results can be obtained
        by attending the public bid opening.  If unable to attend the public bid opening, bid
        tabulations can be obtained in person for $3.00. Bid results can also be obtained by
        sending (do not include with bid) a check for $3.00 payable to the State of Kansas,
        with a self addressed, stamped envelope to the Kansas Division of Purchases, Attn:
        Bid Results/Copies, 900  SW  Jackson,  Room  102-N,  Topeka,  KS    66612. Please
        reference quote number on check. Copies of individual bids may be obtained under 
        the Kansas Open Records Act by calling  (785) 296-0002, requesting an estimate of 
        the cost to reproduce the documents, and remitting that amount to the above address.
        Upon receipt of the funds, the documents will be sent.

8.     Faxed bid responses are not acceptable for bids in excess of $25,000. 
        FAX: (785) 296-7240

9.   I hereby certify that I(we) do not have any substantial conflict of interest sufficient to 
        influence the bidding process on this bid.  A conflict of substantial interest is one 
        which a reasonable person would think would compromise the opening bidding process.


	Prices are to be delivered FOB Destination Prepaid & Allowed:
	 Department of Transportation, *VARIOUS LOCATIONS

	Purchase Requisition Number(s):
	017736, 017754, 017755, 017757, 017758

	
For Additional Information Contact:
	John T. Lowe
	785-296-3126

	[image: ]
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	Page 4 of 33
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Federal Employer Identification Number (F.E.I.N) or Social Security Number:
	

	
Show Payment Terms:
	
	
Signed by:
	

	Delivery To Be:
	
	days after receipt of order.
	Print Name:
	
	Title:
	

	
Date:
	
	
Toll Free or Phone #:
	
	
Fax #:
	

	
	
	
	Email Address:
	
	
















Request for Quotation No.: 12731
Page 5 of 33

TAX CLEARANCE
PLEASE NOTE:  THIS INFORMATION HAS CHANGED EFFECTIVE 10/27/09

Per KSA 75-3740-(c), the Director of Purchases may reject the bid of any bidder who is in arrears on taxes due the State of Kansas.  The Secretary of the Kansas Department of Revenue is authorized to exchange such information with the Director of Purchases as is necessary to determine a bidder’s tax clearance status, notwithstanding any other provision of law prohibiting disclosure of the contents of taxpayer records or information.

A “Tax Clearance” is a comprehensive tax account review to determine and ensure that the account is compliant with all primary Kansas Tax Laws administered by the Director of Taxation.  Information pertaining to a Tax Clearance is subject to change(s), which may arise as a result of a State Tax Audit, Federal Revenue Agent Report, or other lawful adjustment(s).

Bidders (and their subcontractors) are expected to submit a current Tax Clearance Certificate with every event response.  Bidders can obtain a Kansas Tax Clearance Certificate through the Kansas Department of Revenue’s secure website (http://www.ksrevenue.org/taxclearance.htm).  

Please Note:  For applications entered prior to 5:00 PM Monday through Friday, results typically will be available the following business day.  Individual and business applications are available.  Tax clearance requests may be denied if the request includes incomplete or incorrect information. 

Information about Tax Registration can be found at the following website:
http://www.ksrevenue.org/busregistration.htm

The Division of Purchases reserves the right to confirm tax status of all potential contractors and subcontractors prior to the release of a purchase order or contract award.  

In the event that a current tax certificate is unavailable, the Division of Purchases reserves the right to notify a bidder (one that has submitted a timely event response) that they have to provide a current Tax Clearance Certificate within ten (10) calendar days, or the Division may proceed with an award to the next lowest responsive bidder, whichever is determined by the Director of Purchases to be in the best interest of the State.

Contact Information:  Please provide the attached contact information for use should the State of Kansas need to contact the appropriate officials within your company to discuss your tax clearance / registration status.

CONTRACTOR
Contact Person for Tax Issues:	
Company Name:			
FEIN / Tax Number:			
CAUTION:  If your tax number is the same as your Social Security Number (SSN), you must leave this line blank.  DO NOT enter your SSN on this Tax Clearance Form.  If your SSN is required to process a contract award, including any tax clearance requirements, you will be contacted by an authorized representative of the Division of Purchases at a later date.

Mailing Address	
City & State	Zip Code	
Toll Free Telephone	Local	  Cell:  		Fax	
E-Mail	


SUBCONTRACTOR(S)
Contact Person for Tax Issues:	
Company Name:	Tax Number:	
Mailing Address	
City & State	Zip Code	
Toll Free Telephone	Local	  Cell:  		Fax	
E-Mail	
Additional pages may be added, as required, indicating the same information for multiple subcontractors.



Request for Quotation No.: 12731
Page 6 of 33




CERTIFICATION REGARDING
IMMIGRATION REFORM & CONTROL


All Contractors are expected to comply with the Immigration and Reform Control Act of 1986 (IRCA), as may be amended from time to time.  This Act, with certain limitations, requires the verification of the employment status of all individuals who were hired on or after November 6, 1986, by the Contractor as well as any subcontractor or sub-subcontractor.  The usual method of verification is through the Employment Verification (I-9) Form.  With the submission of this bid, the Contractor hereby certifies without exception that Contractor has complied with all federal and state laws relating to immigration and reform.  Any misrepresentation in this regard or any employment of persons not authorized to work in the United States constitutes a material breach and, at the State’s option, may subject the contract to termination and any applicable damages.  

	Contractor certifies that, should it be awarded a contract by the State, Contractor will comply with all applicable federal and state laws, standards, orders and regulations affecting a person’s participation and eligibility in any program or activity undertaken by the Contractor pursuant to this contract.  Contractor further certifies that it will remain in compliance throughout the term of the contract.  

	At the State’s request, Contractor is expected to produce to the State any documentation or other such evidence to verify Contractor’s compliance with any provision, duty, certification, or the like under the contract.  

	Contractor agrees to include this Certification in contracts between itself and any subcontractors in connection with the services performed under this contract.




____________________________________________	______________________
	Signature, Title of Contractor	Date






















Request for Quotation No.: 12731
Page 7 of 33
State of Kansas
Department of Administration
 Division of Purchases

Supplier Diversity Survey Form

Why is the Division of Purchases requesting this information?

Current statutes governing the activities of the Kansas Division of Purchases do not include preferences or set-asides for Small Business Enterprises (SBEs).  The Division of Purchases is interested in determining to what extent purchase orders and contracts are awarded to SBEs under existing work efforts.  Please Note:  You must submit this form with each bid opportunity.

Persons or concerns wishing to receive a Purchase Order or Contract Award resulting from this bid opportunity must provide the information contained in this document before the award is made.  To help expedite this procurement, it is requested that you submit this form with your bid.

COMPANY DATA

Legal Company Name 	
Doing Business As (if applicable)	
Federal Tax ID Number  / FEIN 	
Diversity Program Contact Name	Title	
Phone Number 	Fax Number 	
E-Mail Address 	Company Web 	
Address 	
City 	State 	Zip Code 	
Legal Structure:	□ Corporation	□ Partnership	□ Non-Profit	□ Sole Proprietorship	□ LLC

Signature 	Date:	

COMPANY DIVERSITY DATA  

 (A)	Business Classification   (See Appendix A for definitions):
Is your business a Small Business Enterprise (SBE) as defined by the SBA?
□ Yes	□ No	□ Don’t Know
Check all that Apply:	□ Disabled (DIS) 	□ SBA-Small Disadvantage Business (SDB)
□ Veteran-Owned (VBE)	□ Women-Owned (WBE)	□ Service-Disabled Veterans-Owned (DVBE)
□ African American	□ Native American	□ Minority-Owned Business Enterprise (MBE)
□ Hispanic American  	□ Asian Pacific American	□ Disadvantaged Business Enterprise (DBE)
□ Asian Subcontinent American 	□ Other: __________________________________________________________

 (B)	Has your Business Classification Status been certified by a state, municipal, federal or other certifying agency?
	□ No	□ Yes	Certifying Entity:	



Other State of Kansas Resources for Small Business Enterprises (SBE)

Kansas Department of Commerce
Office of Minority/Women Business Development
http://www.kansas.gov/ksbdc/

Request for Quotation No.: 12731
Page 8 of 33

State of Kansas
Department of Administration
 Division of Purchases
Supplier Diversity Survey Form

Appendix A
Definition of Terms

Small Business Enterprise / Concern (SBE)
SBEs are businesses that do not exceed the size standard for the product or service it is providing as measured by its employment and/or business receipts in accordance with the U.S. SBA numerical size standards.  These standards are defined as FAR 52.219-8, 13 CFR Part 121 and 13 CFR 121.410.

Disadvantaged Business Enterprise (DBE) 
DBEs are defined as a business which are (a) owned by socially disadvantaged individuals who have been subjected to racial or ethnic
prejudice or cultural bias because of their identity as a member of a group without regard to their individual qualities; or (b) owned by economically disadvantaged individuals whose ability to compete in the free enterprise system has been impaired due to diminished opportunities to obtain capital and credit as compared to others in the same line of business who are not socially disadvantaged.

Disabled Business Enterprise (DIS)
DIS businesses are at least 51% owned and controlled by one or more U.S. citizens who has a physical or mental impairment which substantially limits one or more of such person’s major life activities.

Small Disadvantage Business Concern (SDB)
SDB businesses are certified by the SBA as meeting the following criteria: (1) they are small business concern and (2) must be at least 51% owned and controlled by one or more U.S. citizens who are socially and economically disadvantaged.  African Americans, Asian Pacific Americans, Asian Subcontinent Americans, Hispanic Americans and Native Americans are presumed to qualify as being socially disadvantaged.  Other individuals can qualify if they show by a preponderance of the evidence that they are socially disadvantaged.  In addition, the personal net worth of each eligible owner applicant must be less than $750,000, excluding the values of the applicant’s ownership interest in the business seeking certification and the owner’s primary residence.  Successful applicants must also meet applicable size standards for small businesses in their industry.  SDB regulations can be found in FAR 52.219-8 and 13 CFR parts 121 & 124.

Veterans-Owned Business Concern (VBE)
VBE businesses are at least 51% owned and controlled by one or more U.S. citizens who are Veterans of the U.S. Armed Forces.  In the case of any publicly owned business, at least 51% of the stock is owned by one or more veterans and one or more veterans must control the management and daily business operation.  The term “Veteran” means a person who served in the active military, naval or air service and who was discharged or released there from under conditions other than dishonorable.  VBE regulations can de found in FAR 52.219-9 & 38 USC 101 (2).

Service-Disabled Veterans-Owned Business Concern (DVBE)
DVBE businesses are at least 51% owned and controlled by one or more U.S. citizens who are service-disabled Veterans of the U.S. Armed Forces.  In the case of any publicly owned business, at least 51% of the stock is owned by one or more service-disabled veterans and one or more veterans must control the management and daily business operation.  The term “Veteran” means a person who served in the active military, naval or air service and who was discharged or released there from under conditions other than dishonorable.  The term “Service-Disabled” means a veteran of the U.S. Military Service has a service-connected disability with a disability rating of 0%-100%.  In the case of permanent or severe disability, the spouse of caregiver of such a service-disabled veteran may control the management and daily operations.  DVBE regulations can be found in FAR 52.219-9 & 38 USC 101 (2) & USC 101 (16).

Women-Owned Business Concern (WBE)
WBE businesses are at least 51% owned and controlled by one or more U.S. citizens who are female gender.  In the case of any publicly owned business, at least 51% of the stock is owned by one or more women and one or more women must control the management and daily business operations.  For Federal contracting regulations see FAR 52-219-8.

Minority-Owned Business Enterprise (MBE)
MBE businesses are at least 51% owned and controlled by one or more U.S. citizens belonging to certain ethnic minority groups.  In the case of any publicly owned business, at least 51 % of the stock is owned by one or more minorities, and one or more minorities must control the management and daily business operations.  “Ethnic Minority Groups” are people of Asian Pacific American, Asian Subcontinent American, African American, Hispanic American and Native American descent.  
· African Americans: People whose origins lay in any of the Black racial groups of Africa.
· Asian Pacific Americans: People whose origins lay in Brunei, Burma, China, Guam, Indonesia, Japan, Kampuchea (Cambodia), Korea, Laos, Malaysia, Northern Mariana Islands, Republic of the Marshall Islands, Federated States of Micronesia, Republic of Palau (U.S. Trust Territory of the Pacific Islands), the Philippines, Samoa, Singapore, Taiwan, Thailand and Vietnam.
· Asian Subcontinent Americans: People whose origins lay in Bangladesh, Bhutan, India, Pakistan, Sri Lanka or Nepal.
· Hispanic Americans: People whose origins are in the South and Central America, Mexico, Puerto Rico, Cuba or the Iberian Peninsula (including Portugal).
· Native Americans: American Indians, Inuit (Eskimos), Aleuts, and native Hawaiians of Polynesian ancestry.

Date of Last Update:  March, 2007




Request for Quotation No.: 12731
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VENDOR ACCESSORIZED
MAINTENANCE PICKUPS

STATE OF KANSAS
KANSAS DEPARTMENT OF TRANSPORTATION

SPECIFICATION FOR A
VENDOR ACCESSORIZED 3/4 TON MAINTENANCE PICKUP

The following specifications and dimensions shall apply to a VENDOR ACCESSORIZED 3/4 TON MAINTENANCE PICKUP for the Kansas Department of Transportation. The State reserves the right to waive minor technicalities under this specification. Federal and State laws supersede any conflicting part of this specification.

[bookmark: OLE_LINK3][bookmark: OLE_LINK4]Each accessory described in this specification shall be new and unused, and, with the exception of the lightbar support racks, shall be a current model under standard production by the manufacturer, with parts stocked at one or more locations in Kansas or the greater Kansas City area. The requirement for parts to be stocked at locations in Kansas or the greater Kansas City area may be waived if the bidder provides an alternative parts availability plan acceptable to the Agency. ALTERNATIVE PARTS AVAILABILITY PLANS MUST BE APPROVED PRIOR TO CLOSING OF BID.

The bidder agrees, if his proposal is accepted, to warrant all parts, materials and labor supplied including the design of the unit bid for a period of one year. Such warranty shall be in addition to any manufacturer’s warranties on the cab, chassis, engine, etc. and shall include 100% of all costs to repair or replace any defective material or workmanship. A copy of the warranty shall accompany the bid. Warranty coverage shall include costs of transporting the unit to and from dealer's shop, when outside a 150 mile radius of the delivery point.

Complete specifications and literature on the unit bid shall accompany the bid. Any exceptions to these specifications shall be indicated on the bid or on a separate attachment to the bid, labeled as such.

Any “equal” or “equivalent” items for brand specified components shall be listed with the bid package. Complete description and literature on the “equal”/“equivalent” components shall be supplied for consideration by the KDOT. The burden of proof regarding “equal”/“equivalent” items shall be upon the vendor. Note that some equipment in this specification must be evaluated prior to the bid closing to be considered “equivalent” to accepted components.

PRE-DELIVERY SERVICE:  Each vendor accessorized pickup shall be delivered complete and fully operational. It shall be properly serviced, free of leaks, and all mechanical adjustments made prior to delivery. A minimum of three days notice prior to delivery shall be given to the person to whom the unit is to be shipped. Delivery shall be between the hours of 9 AM and 3:30 PM.





This specification is divided into three major sections:
1) Accessories to be installed on KDOT owned fleetside pickup.
2) Accessories to be installed on KDOT owned cab and chassis pickup.
3) Accessories to be installed on both a fleetside and cab and chassis pickup.

PICKUP TRUCK SUPPLIED TO VENDOR  Pickup year, make, and model is SPECIFIED on the Request for Quotation (RFQ). The types of pickup truck(s) that may be supplied to the vendor are as follows:

FLEETSIDE BODY TRUCK:  KDOT may supply a new ¾ ton pickup truck(s) with standard fleetside pickup bed to the vendor. The number of fleetside pickups supplied to the vendor will be SPECIFIED on the Request for Quotation (RFQ).  and if SPECIFIED on the Request for Quotation (RFQ), a fuel tank, distance measuring instrument (DMI) and/or a temperature sensor, all as described in this specification. A receiver hitch, combination pintle with 2" ball, and trailer wiring and connector will be delivered with the truck.
OR
MAINTENANCE CAB AND CHASSIS TRUCK:  KDOT may supply a new ¾ ton cab and chassis pickup truck(s) with fuel cap and hose kit to the vendor. The number of cab and chassis only pickups supplied to the vendor will be SPECIFIED on the Request for Quotation (RFQ). Each truck is to be equipped by the vendor with a utility body, an adjustable pintle hook mount with four pairs of holes, hitch and trailer connector, lightbar support rack, light bar, grille guard, and if SPECIFIED on the Request for Quotation (RFQ), a fuel tank, distance measuring instrument (DMI) and/or a temperature sensor shall also be installed on the truck as described in this specification. A receiver hitch, combination pintle with 2" ball, and trailer wiring and connector will be delivered with the truck.

INSURANCE  The successful vendor will be responsible to supply full replacement cost insurance for each pickup while in the possession of the vendor and to remain in force until final delivery and acceptance by KDOT at each location specified. The vendor shall supply a copy of the policy declaration page to the KDOT Equipment Section no later than 10 days after notification of award at:

	Equipment Section
	Bureau of Construction and Maintenance
	Kansas Department of Transportation
	Eisenhower State Office Building, 6th Floor
	Topeka, Kansas  66603-3745
Attn: KDOT Equipment Engineer

PRINTED MANUALS: One shop manual, parts manual, and operator manual shall be supplied with each accessory unit, with one additional set of each manual supplied to each delivery point. The manuals shall fully and clearly cover all components of the unit.
[bookmark: OLE_LINK7][bookmark: OLE_LINK8]
SECTION 1
ACCESSORIES TO BE INSTALLED ON A FLEETSIDE PICKUP
- - Adjustable Pintle Hook Mount - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

GENERAL:

			A receiver hitch, combination pintle with 2" ball, and trailer wiring and connector will be delivered with the truck.

_____________	_____________	Truck hitch is to be equipped with an adjustable pintle hook mount with four pairs of holes.



- - Light Bar Support Rack - -

SHOW MFG. & MODEL OFFERED _________________________________________

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

GENERAL:

_____________	_____________	Light bar rack is to be fabricated as described in the drawing on the next page of this specification.

_____________	_____________	Light bar rack is to support a light bar specified elsewhere in this specification.

_____________	_____________	Entire unit shall be painted with black powdercoat paint.

_____________	_____________	Expanded metal utilized on the unit shall be ¾" No. 13 carbon steel, diamond pattern.

_____________	_____________	Example unit shall be fabricated, painted and approved by KDOT prior to remaining units being produced.

* * See drawing next page * *
[image: Fleetside Lightbar Rack]
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ACCESSORIES TO BE INSTALLED ON A FLEETSIDE PICKUP 
- - Light Bar Support Rack (Continued) - -


SHOW MFG. & MODEL OFFERED _________________________________________

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

GENERAL:

_____________	_____________	The dimensions given below are approximate and shall be adjusted as necessary for individual manufacturers. In every case, the tool boxes offered by the bidder shall be designed to fit a full size (8 ft) bed.

_____________	_____________	The set shall include two Weatherguard Model R-174, or approved equal, low profile side mounted utility boxes.

		The boxes shall be constructed of 3003 aluminum diamond plate:

_____________	_____________	0.058" thick minimum, for the body and cover;

_____________	_____________	0.100" thick minimum, for the bottom,

_____________	_____________	with fully welded joints.

_____________	_____________	The boxes shall be supported by steel support legs, one front and one rear, between the underside of the box and the body floor.

_____________	_____________	The boxes shall be approximately 54 inches in length; with a 12 inch depth; and 15 inch width, across the top.

_____________	_____________	The deep tool storage bin shall run the length of the box with a minimum 8 inch width.

_____________	_____________	Each box shall have a minimum of 4 cubic feet of storage area.

_____________	_____________	Each sidebox shall have a parts tray.
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ACCESSORIES TO BE INSTALLED ON A FLEETSIDE PICKUP 
- - Toolboxes - -


GENERAL (Continued):

_____________	_____________	The set shall also include one cross box Weatherguard Model R-127, or approved equal, with a minimum 11 cubic foot capacity and a single, full length lid shall be provided.

_____________	_____________	The cross box shall have approximate dimensions of 6 foot length, 20 inch width, and 15 inch height.

_____________	_____________	The top of truck bed sides to bottom of tool box (when box is installed properly) shall be an absolute maximum of 11" to allow for auxiliary equipment to be mounted in the truck bed under the tool box.

_____________	_____________	Lid shall be able to be locked and unlocked from either side and shall be capable of being opened and closed from either side. Boxes that require the operator to walk to both sides of the truck to open/close the lids are unacceptable.

_____________	_____________	Each crossbox shall have a parts tray.

_____________	_____________	The top, bottom and front and back sides shall be constructed of rib-formed panels or shall have longitudinal cover channels for reinforcing.

_____________	_____________	The lid shall overlap the box and shall be weather stripped to provide full weather-proofing.

_____________	_____________	The lid shall have a full-length aluminum piano type hinge or at least 4 heavy duty hinges; and self-locking supports to prevent accidental closing.

_____________	_____________	The lids shall have push-button latches and locks or stainless steel paddle latches.

_____________	_____________	All locks in a set shall be keyed the same. Three keys shall be provided for each set.

OPTIONAL PRICING FOR POWDERCOATING:

_____________	_____________	Please provide optional pricing for black color powder coat paint.
			Cost:  $_____________
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ACCESSORIES TO BE INSTALLED ON A FLEETSIDE PICKUP 
- - Toolboxes (Continued) - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS


SHOW MFG. & MODEL OFFERED _________________________________________

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

_____________	_____________	When SPECIFIED on the Request for Quotation (RFQ), an auxiliary fuel tank shall be installed.

GENERAL:

_____________	_____________	All painted surfaces are to be properly primed and painted white or an approved factory color.

_____________	_____________	The unit shall be an L-shaped single compartment with baffles.

_____________	_____________	Approximate dimensions shall be 26 inches high, 30 inches wide with an absolute maximum length of 55 inches.

_____________	_____________	The bottom leg of the "L" shall have an absolute maximum overall height of 7.75 inches.

_____________	_____________	The upright portion of the "L" shall be a maximum of 11 inches wide.

_____________	_____________	The unit shall hold 88 gallons of fuel, minimum allowing for 10% expansion of tank contents.

_____________	_____________	A two inch reinforced pump/fill opening shall be provided on the top of each outside end of the tank. One 2 inch fill cap shall be provided with each tank.

_____________	_____________	Each tank shall have a two - 1/2 inch minimum diameter drain openings, one in each lower, rear facing corner.

_____________	_____________	The unit shall have brackets at the bottom of the tank to secure the tank to the vehicle. (A minimum of one in each corner of the tank.)
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ACCESSORIES TO BE INSTALLED ON A FLEETSIDE PICKUP 
- - L-Shaped Single Compartment Fuel Tank - -

_____________	_____________	Reinforce area of tank to which bracket is welded.
GENERAL (Continued):
_____________	_____________	Each tank shall have a minimum of two lifting lugs, one at each end of the tank, to aid in installation and removal.

FUEL TRANSFER PUMP:
		The fuel transfer pump shall be:
_____________	_____________	12-volt DC powered,

_____________	_____________	self priming,

_____________	_____________	U.L. listed, and

_____________	_____________	provide a minimum flow rate of 10 gallons per minute.

		The fuel transfer pump shall be equipped with a:
_____________	_____________	check valve,

_____________	_____________	continuous duty solenoid,

_____________	_____________	spin-on fuel filter housing, example Wix #24034,

_____________	_____________	spin-on 10 micron fuel filter, example Wix #24006,

_____________	_____________	strainer,

_____________	_____________	totally enclosed switch,

_____________	_____________	sealed explosion proof and weather proof motor compartment,

_____________	_____________	meter and totalizer,

_____________	_____________	adjustable suction pipe,

_____________	_____________	12 foot hose and lockable manual nozzle, and

_____________	_____________	¾ inch double jointed swivel to relieve stress on the nozzle end of the hose, example Husky VI Model 0350 multi-plane swivel.
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ACCESSORIES TO BE INSTALLED ON A FLEETSIDE PICKUP 
- - L-Shaped Single Compartment Fuel Tank (Continued) - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS


SHOW MFG. & MODEL OFFERED	_________________________________________

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

GENERAL:

_____________	_____________	Utility body is to be Stahl Model 96-CVS, Knapheide Model 796, Reading 967AB, Omaha Standard 96VH or approved equivalent with standard compartments and shelving.

_____________	_____________	Depth of side compartments shall be a minimum of 14.5 inches.

_____________	_____________	Body length shall be a minimum of 96 inches.

_____________	_____________	Body shall be mounted with U-Bolts or brackets bolted in the existing bolt holes of the truck frame. Units welded to any part of frame will not be accepted. The integrity of the truck frame shall not be diminished by any drilling, cutting, or welding.

_____________	_____________	All painted surfaces shall be painted to match cab color, except bottom side of body may be painted black.

_____________	_____________	All compartments must lock securely, using the same key to all compartments. Two keys shall be provided.

_____________	_____________	Compartments shall have rotary style paddle latches and spring loaded door retainers. A “T-handle” latching system which latches the doors in 3 locations is also acceptable.

_____________	_____________	All lights and reflectors shall conform to the Motor Vehicle Laws of the State of Kansas.

_____________	_____________	All added wiring shall be a minimum of 14-gauge SJTO primary cable.
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SECTION 2
ACCESSORIES TO BE INSTALLED ON A CAB & CHASSIS PICKUP 
- - Utility Body - -


GENERAL (Continued):

_____________	_____________	All added wire splices and connections shall be soldered with plastic or resin type solder (acid not approved) and then covered with moisture proof shrink tubing for complete encapsulation.

_____________	_____________	Rear lights shall be mounted same height, both sides, and shall include back up lights and directional signals. Rear lights shall be recessed.

_____________	_____________	Stop/tail/turn lights shall be LED.

_____________	_____________	Light guards shall be installed inside compartment to provide protection to the back side of the recessed lights.
REAR BUMPER:

_____________	_____________	Install heavy duty trailer towing type step bumper, minimum of 8 ½ inch, mounted to the main frame of the truck, bumper and hitch shall be rated for a minimum of 4000 lb. gross trailer weight and 500 lb. tongue weight.

_____________	_____________	Provide OPTIONAL PRICING for same bumper as above except with a step bumper, minimum of 10 inch.
			Cost:  $___________

LOW PROFILE OPTION: (Shall be included in bid price WHEN SPECIFIED on the Request for Quotation [RFQ].)

_____________	_____________	WHEN SPECIFIED, the unit shall be a low profile body meeting all prior specifications except for height dimensions.
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ACCESSORIES TO BE INSTALLED ON A CAB & CHASSIS PICKUP 
- - Utility Body (Continued) - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS


EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

GENERAL:

			A receiver hitch, combination pintle with 2" ball, and trailer wiring and connector will be delivered with the truck.

_____________	_____________	Truck hitch is to be equipped with an adjustable pintle hook mount with four pairs of holes.

_____________	_____________	Truck/utility body is to be equipped with a hitch, combination pintle with 2" ball, and trailer wiring and connector supplied with truck.





- Light Bar Support Rack - -

SHOW MFG. & MODEL OFFERED _________________________________________

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

GENERAL:

_____________	_____________	Light bar rack is to be fabricated as described in the drawing on the next page of this specification.

_____________	_____________	Light bar rack is to support a light bar specified elsewhere in this specification.

_____________	_____________	Entire unit shall be painted with black powdercoat paint.

_____________	_____________	Expanded metal utilized on the unit shall be ¾" No. 13 carbon steel, diamond pattern.

_____________	_____________	Example unit shall be fabricated, painted and approved by KDOT prior to remaining units being produced.

* * See drawing next page * *
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ACCESSORIES TO BE INSTALLED ON A CAB & CHASSIS PICKUP 
- - Adjustable Pintle Hook Mount - -




	Request for Quotation No.: 12731
Specification No.: MS 217.01
	Page: 21 of 21

ACCESSORIES TO BE INSTALLED ON A CAB & CHASSIS PICKUP 
- - Light Bar Support Rack (Continued) - -

[image: Utility Lightbar Rack]
SHOW MFG. & MODEL OFFERED _________________________________________

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

_____________	_____________	When SPECIFIED on the Request for Quotation (RFQ), an auxiliary fuel tank shall be installed.

GENERAL:

_____________	_____________	All painted surfaces are to be properly primed and painted white or an approved factory color.


_____________	_____________	The unit shall be a rectangular single compartment tank with baffles.

_____________	_____________	Dimensions shall be approximately 24 inches high by 29 inches wide with an absolute maximum length of 48 inches.

_____________	_____________	The unit shall have a capacity of 98.5 gallons of fuel, minimum, allowing for 10% expansion of tank contents.

_____________	_____________	Each tank shall have a two inch reinforced pump/fill opening on the top of each end of the tank. The two openings shall be located at the outside edges of the tank for easy access. One 2 inch fill cap shall be provided with each tank.

_____________	_____________	Each tank shall have a two - 1/2 inch minimum diameter drain openings, one in each lower, rear facing corner.

_____________	_____________	The unit shall have brackets at the bottom of the tank to secure the tank to the vehicle. (A minimum of one in each corner of the tank.)

_____________	_____________	Reinforce area of tank to which bracket is welded.

_____________	_____________	Each tank shall have a minimum of two lifting lugs, one at each end of the tank, to aid in installation and removal.
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ACCESSORIES TO BE INSTALLED ON A CAB & CHASSIS PICKUP 
- - Rectangular Single Compartment Fuel Tank - -


FUEL TRANSFER PUMP:
		The fuel transfer pump shall be:
_____________	_____________	12-volt DC powered,

_____________	_____________	self priming,

_____________	_____________	U.L. listed, and

_____________	_____________	provide a minimum flow rate of 10 gallons per minute.

		The fuel transfer pump shall be equipped with a:
_____________	_____________	check valve,

_____________	_____________	continuous duty solenoid,

_____________	_____________	spin-on fuel filter housing, example Wix #24034,

_____________	_____________	spin-on 10 micron fuel filter, example Wix #24006,

_____________	_____________	strainer,

_____________	_____________	totally enclosed switch,

_____________	_____________	sealed explosion proof and weather proof motor compartment,

_____________	_____________	meter and totalizer,

_____________	_____________	adjustable suction pipe,

_____________	_____________	12 foot hose and lockable manual nozzle, and

_____________	_____________	¾ inch double jointed swivel to relieve stress on the nozzle end of the hose, example Husky VI Model 0350 multi-plane swivel.
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ACCESSORIES TO BE INSTALLED ON A CAB & CHASSIS PICKUP 
- - Rectangular Single Compartment Fuel Tank (Continued) - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS


SHOW MFG. & MODEL OFFERED _________________________________________

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

GENERAL:

_____________	___________	The light bar shall measure approximately 2.7 inches high x 12 inches wide x a maximum of 47 inches long (excluding mounting brackets) to mount to the lightbar support rack called out elsewhere in this specification and to match the pickup model(s) listed in the Request for Quotation.

_____________	_____________	Example light bar meeting this specification: Whelen LFL Liberty light bar model KDOTLIB2, PSE light bar model 2747A-CC-KDOT, Federal Signal LGD45-01149-KDOT, or equivalent. All other light bars must be evaluated and approved by KDOT prior to closing of bid to be considered “equivalent”.

_____________	_____________	The light bar must meet all Federal Motor Vehicle Safety Standards and Society of Automotive Engineers (SAE) Class I requirements.

_____________	_____________	For strength and durability, the framework of the light bar must be made of extruded aluminum.

_____________	_____________	The light bar must contain one control module I/O board which must control all internal light heads.

_____________	_____________	The I/O Board shall produce a minimum flash rate of seventy five flashes per minute.

_____________	_____________	There shall be a minimum of ten flash patterns from which to choose.

_____________	_____________	Each set of two light-emitting diode (LED) lamps must be capable of operating in a different flash pattern.
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SECTION 3
ACCESSORIES TO BE INSTALLED ON
BOTH FLEETSIDE AND UTILITY BODY TRUCKS
- - Light Bar - -


GENERAL (Continued):

_____________	_____________	Light bars with more than one internal electronic module control to control all internal lights is not acceptable.

_____________	_____________	The light bar must operate on a voltage range of 10 – 16 VDC.

_____________	_____________	The component configuration shall correspond to the “Light Bar Diagram” in this section of the specification.

_____________	_____________	The wiring configuration (if applicable) shall correspond to the “Light Bar Diagram” in this section of the specification.


WARRANTY:

_____________	_____________	All components of the light bar shall be warranted free from defects for a minimum period of five years from the date of installation.

_____________	_____________	All components of the light bar shall have a lifetime warranty against hail damage.

LED MODULES:

_____________	_____________	The light bar must contain a minimum of 96 “Whelen ‘Super-LEDs’, ‘Generation 3.5’, or equivalent.”

_____________	_____________	The light bar must have a maximum of four Whelen “ ‘Linear-LED’ or equivalent” modules, one in each corner.

_____________	_____________	Each corner Linear module must consist of a minimum of twelve Whelen high output LEDs or equivalent permanently mounted within a single “removable” highly mirrored parabolic reflector for maximum light output.

LED MODULES (Continued):

_____________	_____________	The forward and rear facing LED modules shall be mounted in a straight line.

_____________	_____________	The LED modules shall have a single diffuser panel mounted in front of them for maximum light output.

_____________	_____________	Light bars that utilize individual reflectors for each LED or that use mirrors to reflect light are not acceptable.

_____________	_____________	All front-facing LED panels shall be the same design as the corner “Linear-LEDS” described above, but shall contain a minimum of six high output LEDs.

_____________	_____________	The rear “Linear-LED” panels shall contain a minimum of six high output LED’s within the light head.

_____________	_____________	All rear LEDs must produce a minimum of a 90 degree light pattern.

_____________	_____________	LED panels that do not produce significant light output at 45 degrees are not acceptable.

		The light bar shall be designed to have:

_____________	_____________	a minimum of seven modules to the front (including corners),

_____________	_____________	a minimum of seven modules to the rear (including corners),

_____________	_____________	and one (empty module slot) on each end.

_____________	_____________	The light bar LED colors will be amber; all with clear polycarbonate lenses.

LED MODULES (Continued):

_____________	_____________	The light bar shall also be capable of low power, to reduce the brightness for night time operation.

_____________	___________	The LED panel must be mounted within the light bar.

_____________	___________	Systems in which the LED panel/lens assembly makes up the outside configuration of the light bar are not acceptable.

FACTORY IN-DASH SWITCH CONNECTIONS

_____________	___________	The light bar shall be connected to and controlled by four factory installed in-dash switches.

		The four switches shall operate the light bar as follows:

_____________	_____________	Switch #1 – on/off master switch. When initially turned “on”, the light bar will operate in random rapid flash mode for front, rear, and sides.

_____________	_____________	Switch #2 – “left” arrow.

_____________	_____________	Switch #3 – “right” arrow.

_____________	_____________	Switch #4 – “dim” the light bar.

WIRING HARNESS:

_____________	_____________	The harness shall be wired on the passenger side.


WIRING HARNESS (continued):

		The harness shall have:

_____________	_____________	a single harness containing hot, ground, and switching wires
			or
_____________	_____________	a separate hot/ground harness and switching harness.

_____________	_____________	The harness shall be wired directly to a fused link at the battery.

MOUNTING BRACKETS:

_____________	_____________	Each light bar must be supplied with two slide bolts for mounting on rear headache racks.

MODULE CONFIGURATION (See diagram):

_____________	_____________	Front:	Two Whelen “Linear12 Super-LED or equivalent” modules [amber].
			Two Whelen “Linear6 Super-LED or equivalent” modules [amber].

_____________	_____________	Rear:	Two Whelen “Linear12 Super-LED or equivalent” modules [amber].
			Six Whelen “Linear6 Super-LED or equivalent” modules [amber]
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ACCESSORIES TO BE INSTALLED ON
BOTH FLEETSIDE AND UTILITY BODY TRUCKS
- - Light Bar (Continued) - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS
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ACCESSORIES TO BE INSTALLED ON
BOTH FLEETSIDE AND UTILITY BODY TRUCKS
- - Light Bar (Continued) - -
[image: Light Bar Diagram]
SHOW MFG. & MODEL OFFERED _________________________________________

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS

GENERAL:

_____________	_____________	The unit shall be a Perry Company Renegade, Go Industries Rancher or approved equal.

_____________	_____________	The unit shall be custom designed and manufactured to fit a ¾ ton pickup. Specific pickup year, make, and model is SPECIFIED on the Request for Quotation (RFQ).

_____________	_____________	The unit shall mount to the frame of the pickup truck using existing factory holes. Bumper mounts are not acceptable.

_____________	_____________	State the cost of OPTIONAL mounting hardware required for trucks without tow hooks.
			Cost:  $_____________

_____________	_____________	The unit shall not interfere with mounting and use of factory tow hooks.

_____________	_____________	The unit's main frame shall be constructed of steel pipe or tubing having an outside diameter of at least 1.3" and weighing at least 1.6 pounds per foot. Larger diameters and weights will be given preference.

_____________	_____________	The unit shall be continuously welded leaving no unwelded seams.

_____________	_____________	The unit shall incorporate a steel mesh or punched plate center grille of at least 16 gauge thickness.

_____________	_____________	The unit shall be finished with black powder coat.

_____________	_____________	The unit shall extend the full width of the grille, protecting the lights.
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ACCESSORIES TO BE INSTALLED ON
BOTH FLEETSIDE AND UTILITY BODY TRUCKS
- - Grille Guard - -

GENERAL (Continued):


_____________	_____________	The unit shall be designed such that light from headlights or turn/parking lamps is not obstructed or reflected from the unit toward the operator or other vehicles on the roadway.

_____________	_____________	Three copies of descriptive literature including size and thickness or gauge of pipe or tubing shall be provided.

_____________	_____________	The name and location of a dealer or distributor having this model in stock for inspection shall be provided.

_____________	_____________	Detailed photos of the bid unit installed on the specific pickup listed on the Request for Quotation (RFQ) shall be provided.
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ACCESSORIES TO BE INSTALLED ON
BOTH FLEETSIDE AND UTILITY BODY TRUCKS
- - Grille Guard (Continued) - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS


SHOW MFG. & MODEL OFFERED _________________________________________

_____________	_____________	When SPECIFIED on the Request for Quotation (RFQ), a distance measuring instrument (DMI) shall be installed as described below.

_____________	_____________	When SPECIFIED on the Request for Quotation (RFQ), the unit is to be equipped with an RS-232 port for inventory survey uploading to a personal computer.

_____________	_____________	When SPECIFIED on the Request for Quotation (RFQ), the unit is to be equipped with an electronic interface and cable kit that is universally compatible between make and models of vehicles.

GENERAL:

[bookmark: OLE_LINK9][bookmark: OLE_LINK10]_____________	_____________	Unit is to be obtained according to existing KDOT contract found at:
			http://prodnet2/FiscalContracts/Default.aspx

WIRING:

_____________	_____________	Interface shall be installed and wiring shall be run by the vendor so that head can be installed on any part of the dashboard.

_____________	_____________	Distance Measuring Instrument head will be provided by the vendor with the truck but will be installed by KDOT.
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ACCESSORIES TO BE INSTALLED ON
BOTH FLEETSIDE AND UTILITY BODY TRUCKS
- - Distance Measuring Instrument - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS
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ACCESSORIES TO BE INSTALLED ON
BOTH FLEETSIDE AND UTILITY BODY TRUCKS
- - Distance Measuring Instrument - -

EXCEPTIONS TO
MFG. CODE	SPECIFICATION		SPECIFICATIONS


SHOW MFG. & MODEL OFFERED _________________________________________

		When SPECIFIED on the Request for Quotation (RFQ), a pavement temperature sensor shall be installed:

GENERAL:

[bookmark: OLE_LINK5][bookmark: OLE_LINK6]_____________	_____________	An infrared pavement temperature sensor shall be properly mounted per the manufacturer’s recommendations. 

_____________	_____________	The gauge shall be mounted in the location shown in the dash layout diagram, below.


_____________	_____________	The gauge shall display both air and pavement temperature simultaneously

_____________	_____________	The infrared pavement temperature sensor shall be a Sprague Roadwatch or Quixote Transportation Technologies Surface Patrol or approved equal.
[image: TEMP GAGE border]
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ADDENDUM

December 29, 2009

Addendum Number:	1

RFQ Number:	12731

PR Numbers:	017736, 017754, 017755, 017757, 017758

Closing Date:	January 5, 2010, 2:00 P.M.	(SEE BELOW)

Procurement Officer:  	John T. Lowe
Telephone:	785-296-3126
E-Mail Address:  	john.lowe@da.ks.gov 
Web Address:  	http://da.ks.gov/purch

Item:	Truck Accessories

Agency:	Department of Transportation
	Topeka, KS


Conditions:  

1. Closing Date has been extended to January 12, 2010.

2. 
Please see attached .pdf	

There are no other changes at this time.


A signed copy of this Addendum must be submitted with your bid.  If your bid response has been returned, submit this Addendum by the closing date indicated above.

I (We) have read and understand this addendum and agree it is a part of my (our) bid response.

NAME OF COMPANY OR FIRM:	

SIGNED BY:	

TITLE:	 DATE:	
	

It shall be the vendor's responsibility to monitor this website on a regular basis for any changes/addenda.
http://da.ks.gov/purch/rfq/rfqdata/12731.doc 
	

[image: 7595 Larned header gray.eps][image: 93508 Letterhead Chris Howe Footer Black]
ADDENDUM

January 6, 2010

Addendum Number:	2

RFQ Number:	12731

PR Numbers:	017736, 017754, 017755, 017757, 017758

Closing Date:	January 12, 2010	(SEE BELOW)

Procurement Officer:  	John T. Lowe
Telephone:	785-296-3126
E-Mail Address:  	john.lowe@da.ks.gov 
Web Address:  	http://da.ks.gov/purch

Item:	Truck Accessories

Agency:	Department of Transportation
	Topeka, KS

Conditions:  

1. Closing Date has been extended to January 14, 2010.

2. The following Item is added to PR# 017758 (KDOT PR# 478976) for delivery to Garden City, KS:

1 Each     	Vendor Furnished & Installed Accessories for KDOT 		$___________
	Owned 2010 Ford F-250 Cab and Chassis Truck.
			
	To include Utility Bed, Grille Guard, Light Bar Rack, Light 
	Bar, and Rectangular fuel tank

There are no other changes at this time.


A signed copy of this Addendum must be submitted with your bid.  If your bid response has been returned, submit this Addendum by the closing date indicated above.

I (We) have read and understand this addendum and agree it is a part of my (our) bid response.

NAME OF COMPANY OR FIRM:	

SIGNED BY:	

TITLE:	 DATE:	
	

It shall be the vendor's responsibility to monitor this website on a regular basis for any changes/addenda.
	http://da.ks.gov/purch/rfq/rfqdata/12731.doc	
	
	

	
Federal Employer Identification Number (F.E.I.N) or Social Security Number:
	

	
Show Payment Terms:
	
	
Signed by:
	

	Delivery To Be:
	
	days after receipt of order.
	Print Name:
	
	Title:
	

	
Date:
	
	
Toll Free or Phone #:
	
	
Fax #:
	

	
	
	
	Email Address:
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BUREAU OF FISCAL SERVICES 
Rhonda J Seitz, Chief 


Dwight D. Eisenhower State Office Building 
700 S.W. Harrison Street; Topeka, KS 66603-3745 • (785) 296-3545 • Fax: (785) 296-7927 


Hearing Impaired - 711 • e-mail: publicinfo@ksdot.org • Public Access at North Entrance of Building 
 


 
 
 
 


CONTRACT AWARD 
 
 
Date of Award:  April 10, 2009 
 
Contract Number:  75568 
 
Item: Distance Measuring Instruments 
 
Period of Contract: Date of Award through March 31, 2010, with one, one year 


renewal option. 
     
Contractor:   John Thomas, Inc. 
    1560 Lovett Dr. 
    Dixon, IL  61021 
 
Phone:   888-447-7263 
 
FEIN:    34-1857196 
 
Contact Person:  Larry Hageman, CFO 
 
Procurement Officer: Charlie Woldt 
Phone:   785-296-3313 
E-Mail:   charlesw@ksdot.org 


 
 
 
 
 
  
 







 


 


Kansas Department of Transportation 
Pricing Page, Distance Measuring Instrument 


 
 
Specify brand and model:  _____Nu-Metrics NiteStar NS-50______________ 
 
Statewide estimated annual quantity:  40 
 
Quantity ordered 1 – 5 units per location order:  Cost per each:  $__613.00___________ 
Note:  The above price includes the electronic interface and cable kit priced below.  If ordering the head 
only, deduct $205.00 from the cost. 
 
Quantity ordered 6 – 10 units per location order:  Cost per each:  $_592.00___________ 
Note:  The above price includes the electronic interface and cable kit priced below.  If ordering the head 
only, deduct $205.00 from the cost. 
 
Quantity ordered 11 or more per location order:  Cost per each:  $__573.00___________ 
Note:  The above price includes the electronic interface and cable kit priced below.  If ordering the head 
only, deduct $205.00 from the cost. 
 
Show Optional pricing for unit to be equipped with an RS-232 port for inventory survey uploading to a 
personal computer:  $___792.00_______ 
 
Show Optional pricing Electronic interface and cable kit. Interface shall be universally compatible 
between make and models of vehicles.  An example of an acceptable interface is Nu-Metrics SS-10:  
$__205.00________ 
 
List all vehicle Makes that interface is not compatible with:  NONE 
 
Show payment terms:  __Net 30 days_________________ 
 







 


 


Kansas Department of Transportation 
Special Provisions for 


Distance Measuring Instrument 
 


1. This contract shall be established to provide Distance Measuring Instruments for the Kansas 
Department of Transportation (KDOT).  
 


2. Period of Contract:  The contract shall begin Date of Award through March 31, 2010, with one year 
renewal option. 


 
3. Termination for Cause:  The Procurement Officer may terminate this contract, or any part of this 


contract, for cause under any one of the following circumstances: 
 


a. The Contractor fails to make delivery of goods or services as specified in this contract; or 
 


b.The Contractor fails to perform any of the provisions of this contract, or so fails to make progress 
as to endanger performance of this contract in accordance with its terms. 


 
4. The Procurement Officer shall provide Contractor with written notice of the conditions endangering 


performance.  If the Contractor fails to remedy the conditions within ten (10) days from the receipt 
of the notice (or such longer period as State may authorize in writing), the Director of Purchases 
shall issue the Contractor an order to stop work immediately.  Receipt of the notice shall be 
presumed to have occurred within three (3) days of the date of the notice. 


 
5. Termination for Convenience:  The Procurement Officer may terminate performance of work under 


this contract in whole or in part whenever, for any reason, the Procurement Officer shall determine 
that the termination is in the best interest of the State of Kansas.  In the event that the Procurement 
Officer elects to terminate this contract pursuant to this provision, it shall provide the Contractor 
written notice at least thirty (30) days prior to the termination date.  The termination shall be 
effective as of the date specified in the notice.  The Contractor shall continue to perform any part of 
the work that may have not been terminated by the notice. 


 
6. For good cause, and consideration for executing this contract, the contractor, acting herein by and 


through its authorized agent, hereby conveys, sells, assigns, and transfers to the State of Kansas all 
rights, title, and interest in and to all causes of action it may now or hereafter acquire under the 
anti-trust laws of the United States and the State of Kansas, relating to the particular product or 
services purchased or acquired by the State of Kansas pursuant to this contract. 


 
7. Quantities:  Quantities indicated herein are estimated and will be used to evaluate bids.  Quantities 


ordered will be those actually purchased. 
 


8. Delivery:  Deliveries must be completed with 30 calendar days after receipt of order. 
 


Delivery locations will be to District Headquarters located at:  Topeka, KS  66612; Salina, KS  
67402, Norton, KS  67654; Chanute, KS  66720; Hutchinson, KS  67504 and  
Garden City, KS  67846. 







 


 


 
 


Contract No. 75568 
 


9. Prices:  Prices will be guaranteed during the contract period.  All prices to be F.O.B. 
Destination, freight paid by the contractor to the ordering locations.  Price 
Adjustments:  On the yearly anniversary date of this contract, prices as bid may 
remain at the price bid or may be based on a price adjustment, either upward or 
downward, keyed to industry and changes. Contractor shall furnish figures at least 
thirty (30) days prior to expiration date to substantiate any claim for increase. Price 
increases shall not exceed five percent (5%) of the existing contract. If parties to the 
contract cannot agree on renewal terms, it is hereby understood that the contract 
will be re-bid.  


 
10. Orders and Payment:  Orders will be issued by telephone or fax using the Purchase 


Authority form #DOT 455A.  Payment will be made within 30 days upon receipt 
and acceptance of material and a copy of the invoice indicating the order number. 


 
11. Bidders shall return with the bid, the attached Specification properly completed 


showing any and all deviations and the pricing page. 
 


12.  To be in accordance with Specification No.: MS 44.8, Dated  03-06-09, attached 
for reference. 


 







 


 


Specification No.: MS 44.8 
Date: 3-6-09 
Page 1 of 3 


DM/DME/DIST 
 


KANSAS DEPARTMENT OF TRANSPORTATION 
DIVISION OF OPERATIONS 


 
SPECIFICATIONS 


FOR 
DISTANCE MEASURING INSTRUMENT 


 
 The following specifications and dimensions shall apply to purchases of 
DISTANCE MEASURING INSTRUMENT for the Kansas Department of 
Transportation. The KDOT reserves the right to waive minor technicalities under 
this specification. Federal and State laws supersede any conflicting part of this 
specification. 
 
 The unit shall be a current model, new and unused and under standard 
production by the manufacturer.  All parts utilized on the unit shall be new and 
unused. 
 
 The bidder agrees, if his proposal is accepted, to guarantee the design, 
material and workmanship of the unit bid according to the standard factory 
warranty, or for one year from date of acceptance, whichever is greater.  A copy 
of the warranty shall accompany the bid. Warranty coverage shall include costs 
of transporting the unit to and from dealer's shop, when outside a 150 mile radius 
of the delivery point. 
 
 Complete specifications and literature on the unit shall accompany the bid.  
Any exceptions to these specifications shall be indicated on the bid or on a 
separate attachment to the bid, labeled as such. 
 
 Any "or equal" or "equivalent" items for brand specified components shall 
be listed with the bid package.  Complete description and literature on the "or 
equal" components shall be supplied for consideration by the KDOT.  The burden 
of proof regarding "or equal" items will be upon the vendor. 
 
PRE-DELIVERY SERVICE:  The unit shall be delivered complete and fully 
operational.  It shall be properly serviced and all out of vehicle adjustments 
made prior to delivery.  A minimum of three days notice prior to delivery shall 
be given to the person to whom the unit is to be shipped. 
 
PRINTED MANUALS:  One operators manual shall be supplied with each unit.  
One additional set consisting of a shop manual, parts manual and operators 
manual shall be furnished to each delivery point.  The manuals shall fully and 
clearly cover all components of the unit and attachments.  Complete instructions 
for installation of the unit and sensors shall accompany each unit. 







Specification No.:  MS 44.8 
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  ITEM:   DISTANCE MEASURING INSTRUMENT 
 
SHOW MFG. & MODEL OFFERED ___________________________________ 
 
  EXCEPTIONS TO 
MFG. CODE SPECIFICATIONS                        SPECIFICATIONS 
 
GENERAL DESCRIPTION: 
 
_____________ _____________ Unit is to be a microprocessor based 


Distance Measuring Instrument for 
mounting in vehicles. 


 
POWER REQUIREMENTS: 
 
_____________ _____________ Unit shall operate from approximately 9 


to 16 volts DC with negative ground. 
 
OPERATING TEMPERATURE: 
 
_____________ _____________ 0 C. to 70 C. 
 
ACCURACY: 
 
_____________ _____________ Plus or minus one foot per mile. 
 
OPERATING FEATURES (The unit shall be equipped with the following): 
 
_____________ _____________ Lighted display panel.  Display shall 


allow for 6 digit distance and 3 digit 
speed.   


 
_____________ _____________ Unit shall be capable of automatically 


converting the distance on the display to 
English or S.I. units with the push of a 
key. 


 
_____________ _____________ Automatic calibration with 4 vehicle 


memory. 
 
_____________ _____________ Pre-distance entry function. 
 
_____________ _____________ Display hold without loss of 


accumulating distance. 
_____________ _____________ Bi-Directional Counting (Up or Down)
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  EXCEPTIONS TO 
MFG. CODE SPECIFICATION  SPECIFICATIONS 
 


 


OPERATING FEATURES (Cont.) 
 
_____________ _____________ Unit shall include a keypad with 15 keys. 
 
_____________ ____________ Shall include internal memory for up to 


99 locations. 
 
ACCESSORIES: 
 
_____________ _____________ Optional pricing for unit to be equipped 


with an RS-232 port for inventory survey 
uploading to a personal computer. 


 
_____________ _____________ Optional pricing Electronic interface 


and cable kit. Interface shall be 
universally compatible between make 
and models of vehicles.  An example of 
an acceptable interface is Nu-Metrics 
SS-10. List all Makes that interface is 
not compatible with.  


 
EXAMPLE: 
 
_____________ _____________ Unit shall be Nu-Metrics Model 


NITESTAR NS-50 or approved equal. 
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