Idaho Transportation Department
ITB03543
Aluminum Sheets and Sign Blanks

 

The Division of Purchasing is seeking bids for the Idaho Transportation Department (ITD) from qualified vendors for the purchase of Aluminum Sheets and Sign Blanks.  Estimated quantities and sizes provided on Attachment 1 – Pricing Sheet.  All Aluminum Sheets and Sign Blanks must meet the technical specifications detailed below.

Please Note:  ASTM Specification for Conversion Coating is:
“ ASTM B921 - 08 Standard Specification for Non-hexavalent Chromium Conversion Coatings on Aluminum and Aluminum Alloys”

1	Projected Timeline

1.1	Questions Due							November 19, 2009
1.2	Questions Answered (approximate)				November 27, 2009
1.3	Bid Closing Date						December 11, 2009

2		Standard Terms and Conditions 

The State's Standard Contract Terms and Conditions and Solicitation Instructions to Vendors are incorporated by reference into this solicitation as if set forth herein in their entirety.  The Terms and Conditions and Instructions to Vendors are located on the Internet at http://www2.state.id.us/adm/purchasing/index.htm.  The Terms and Conditions and Instructions to Vendors shall apply to this solicitation and the State of Idaho Standard Contract Terms & Conditions shall apply to any contract resulting from this solicitation.  Failure by any submitting vendor to obtain copies of these documents shall in no way constitute or be deemed a waiver by the State of either document, or any part of them.  No liability will be assumed by the Division of Purchasing for a submitting vendor's failure to consider the Terms and Conditions and Solicitation Instructions to Vendors in its response to the solicitation.

3	Correspondence, Questions and Addenda

All correspondence will be in writing.  In the event that it becomes necessary to revise any part of this ITB, addenda will be posted at www.sicomm.net.  It will be the responsibility of the Bidder to monitor www.sicomm.net for any updates or amendments.  Any oral interpretations or clarifications of this ITB shall not be relied upon.  All changes to this ITB must be in writing and posted at www.sicomm.net to be valid.  






This solicitation is issued by the Division of Purchasing via the state’s e-procurement provider, Sicomm.  The Division of Purchasing is the only contact for this solicitation.  Written questions must be submitted via e-mail to:

Diane Robinson, Purchasing Officer
Phone (208) 332-1631
State of Idaho, Division of Purchasing
E-mail: Diane.Robinson@adm.idaho.gov
 
The deadline for receipt of questions is November 19, 2009.  To be considered, questions must be received via e-mail by 5:00 p.m. Mountain Time, on that date.  Answers to timely received vendor questions will be posted at www.sicomm.net.

4	Bid Submission

4.1    Bids are to be submitted manually and must be received at the office of the Division of Purchasing and time stamped using the Division’s time stamp, no later the than the date and time set forth for the Bid Closing.  Bids must include a completed Pricing Sheet (Attachment #1).  Do not fax or e-mail your response.

4.2       Bids must be sealed, and the outer package clearly labeled to identify the solicitation.  One (1) original hardcopy and two (2) hardcopies of the Bid, marked “Technical Bid - Original” along with two (2) exact electronic (soft) copy in Excel format (on CD or USB).  

4.3       State of Idaho Signature Page

Bids must include a completed State of Idaho Signature Page, with an original signature.  Failure to include a signed, complete original State of Idaho Signature Page will result in a finding that the Bid is non-responsive, and no further consideration will be given to the Bid. If you have a web site, please write it on the State of Idaho Signature Page.

5	Invoicing and Payment

Invoices shall be submitted as instructed by the individual purchase orders. Invoices are to reference the purchase order number and the contract number.  Payment terms shall be Net 30 after receipt of order. 

6	FOB Destination

All unit prices bid must include all shipping charges FOB Destination to address noted on ITB. 

7          Contract Award

Contract will be awarded ALL OR NONE to the responsible responsive bidder with the lowest “Total Cost”.


8	Specifications

8.1	All aluminum shall conform to ASTM B-209, Alloy-Temper 6061-T6 Or 5052-H38,            and conform to flatness tolerances listed in Table 7.18 of the Aluminum
 Standards and Data Book published by the Aluminum Association, Inc.

8.2	In addition to the above requirements, the allowable deviation from the flatness of the sign blanks, including all sizes through 48"x 48", shall be no more than 1/16" per foot (longitudinal and transverse) when the blank is positioned on a flat horizontal surface.

8.3 All aluminum shall be conversion coated per sheeting manufacturer’s recommendations, conforming to ASTM B921 - 08 Standard Specification for Non-hexavalent Chromium Conversion Coatings on Aluminum and Aluminum Alloys.  The optimum coating weight will be 25 milligrams per square foot of aluminum, applied in a uniform manner with no excessive buildup on the edges.  Any other coating or electrochemical process proposed to be used must be approved by the Idaho Transportation Department (ITD).

8.4 Sign blanks shall be 0.080 gauges with mounting holes per attached drawing titled “Punching Schedule for Type ‘B’ or Type ‘E’ Signs.”  All edges, corners, and holes shall be smooth, burr-free, and not sharp from manufacturing.

8.5 Flat, uncut, sheets shall be 0.063 or 0.080 gauge as specified when ordered.

8.6 All mounting holes shall be 3/8" diameter.

8.7 Corner radii for vertical rectangle, horizontal rectangle, square and diamond sign blanks shall be 1 1/2".  Blanks 48" x 48" and larger shall have 3" radii.

8.8 All other blanks, equilateral triangle (yield), interstate shield, U.S. shield, pentagon (school), county shield, national forest shield, and isosceles triangle (no passing zone), shall have radii which conforms to FHWA standard highway sign layouts (http://mutcd.fhwa.dot.gov/ser-shs_millennium_eng.htm).

8.9 Aluminum sheets and sign blanks shall be packaged and received free of contaminants (dirt, grease and moisture, excessive traffic marks, or other foreign matter).

8.10 Sign blanks shall be staggered in quantities of ten and banded securely to pallets (one size per pallet).  Pallets will be clearly marked displaying quantities and sizes and shall not exceed 2,000 lbs. per pallet.  Note:  Signs staggered in quantities OTHER THAN 10 shall be rejected.

8.11 Aluminum flat sheets and sign blanks will be tested at point of delivery for conformance to specifications.  All material that fails testing procedures will be rejected and returned to the contractor at no expense to ITD.



9         Other Contract Provisions

9.1       MATERIAL CERTIFICATION
A Certificate of Conformance shall accompany each sign lot shipped to ITD certifying the materials proposed to be supplied will meet or exceed the requirements of ASTM B-209 and ASTM B921 specifications.  

9.2	LEADTIME
Delivery time to ITD after receipt of order shall not exceed 30 business days.  

9.3	CONTRACT TERM
Contract term will be for one (1) year with the option to renew for three (3) additional one-year renewals.  

9.4	ESTIMATED QUANTITIES
The quantities provided are estimated and are provided for bidding purposes only.   Actual quantities ordered may vary.

9.5	PRICE ADJUSTMENT CLAUSE
The contractor may request an adjustment at annual intervals from the date of the contract.  The percentage increase is not to exceed the latest annual increase in the Table 6. Producer price indexes and percent changes for commodity groupings and individual items, not seasonally adjusted, Aluminum, Commodity Code 1025-0105.  Such adjustment may be allowed only after:

· The vendor has submitted a written request to the Department at least 30 calendar days prior to the proposed implementation date and provided detailed justification for such an adjustment is given, and

· The Department has given written approval of the requested adjustment effective on the next annual adjustment date.
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