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Technical Specifications For Dell Server R720
· Rack mount type 

· Bezel

· Default Power Management BIOS Setting:  Performance BIOS Setting

· Risers with 4, x8 PCIe Slots + 2, x16 PCIe Slots

· 1x Integrated Dell Remote Access Controller (iDRAC) 7 Enterprise Embedded System Management 

· 2x  750W Hot-plug, Redundant Power Supply (1+1)

· 2x NEMA5-15P to C13 Wall Plug, 15-amp Power Cord (24 inch) 

· 1x Intel Ethernet X540 + I350 Network Daughter Card

· 2x 10GbE RJ-45 Interfaces

· 2x 1GbE RJ-45 Interfaces

· Single Root Input/Output Virtualization (SR-IOV) capable

· 2x Intel Xeon E5-2670 (2.6GHz/8-core/115W)

· 6x 16GB (96 GB total) Dual Rank x4 PC3-12800R (DDR3-1600) Registered CAS-11 Memory

· 1x PERC H710P Integrated RAID Controller configured for RAID-1

· 2x 300GB 6G SAS 10K rpm SFF (2.5-inch) SC Enterprise 3yr Warranty Hard Drive

· 1x QLogic 2462, Dual Port 4Gb Optical Fibre Channel Host Bus Adapter

· 1x SATA DVD ROM Internal Drive

· ReadyRails Sliding Rails (without Cable Management Arms)

· 1x Microsoft Windows Server 2008 R2 Service Pack 1, Standard Edition, License 

· Not Pre-installed 

· 32 GB Memory Limit of Standard Edition is understood

· 5 Year ProSupport and Next Business Day On-Site Service

· Keep your Hard Drive, 5 years
Other Abbreviations/Acronyms Used:

BIOS – Basic Input Output System

DVD – Digital Versatile Disk

GbE – Gigabit Ethernet

Gb – Gigabit

GB – Gigabyte

PCIe - Peripheral Component Interconnect Express

ROM – Read Only Memory

SATA – Serial Advanced Technology Attachment
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