MOHAVE COUNTY COMMUNITY COLLEGE DISTRICT
Kingman, Arizona

REQUEST FOR QUOTE
RFQ 15-1213
Mobile Technology Systems 
MOBILE CLASSROOM FIFTH WHEEL TRAILER
Responses will be received at:
Office of the President
Attn:  Amy Curley
Mohave County Community College

Kingman Campus - Building 100
1971 Jagerson Ave 

Kingman, AZ 86409
Quotes must be received at the above location by 
2:00 PM local time Monday, April 8, 2012
For inquiries regarding this Quote Contact:

Christine Van Vleet
Procurement Manager
Mohave County Community College
1971 Jagerson Avenue

Kingman AZ  86409

Voice:  928-757-0819
FAX:  928-757-0814
cvanvleet@mohave.edu
This is a Notice of a procurement process which may result in an award; however it is not intended to be and should not be construed to be an offer to contract.

April 1, 2013
I.  SCOPE OF SERVICES
Mohave County Community College invites interested companies to submit a quote for a Fifth Wheel Travel Trailer to be used as a Mobile Technology Classroom as described below. 
Any equipment quoted which is not listed on the below table must be of equal or better quality and functionality to that which is listed in the below table.
Quotes should provide the name of the make and model of equipment in addition to a per item cost and a total cost based on listed quantities.

All quotes should list shipping, tax and all related installation and implementation fees at the end of the quote.
Quoted prices must be signed and dated by an authorized signer.
	 
	FIFTH WHEEL TRAVEL TRAILER
	
	QTY
	MAKE & MODEL
	UNIT PRICE
	TOTAL

	
	Equipment for operation similar or at least equal to:
	
	 
	
	
	

	1
	38 FT. Goose Neck Travel Trailer
	
	
	
	
	
	

	
	To be used for mobile classroom 
	
	
	
	
	
	

	
	STANDARD FEATURES:
	
	
	
	
	
	

	
	102” Body Width
	
	
	
	
	
	

	
	6’6” Interior Height (See option for extra height)
	
	
	
	
	
	

	
	96” Interior Width
	
	
	
	
	
	

	 
	82” between wheel wells
	
	
	
	
	
	

	
	1 piece aluminum roof
	
	
	
	
	
	

	
	.030 Aluminum Exterior
	
	
	
	
	
	

	
	Heavy Duty 8” tubular Main Frame Rails
	
	
	
	
	
	

	
	Wall Construction: 1”x1 ½ steel box tube sidewalls w/dust shield
	
	
	
	
	
	

	
	White Vinyl Walls and Ceiling
	
	
	
	
	
	

	
	¾” Plywood Floor w/Darco moisture barrier
	
	
	
	
	
	

	
	16” On Center Walls, Ceiling and Floor
	
	
	
	
	
	

	
	All Wheel Electric Brakes
	
	
	
	
	
	

	 
	Dexter E-Z Lube Torsion Axles
	
	
	
	
	
	

	
	15” Radial Tires with Silver Mod Rims
(See option for larger 16” tires)
	
	
	
	
	
	

	 
	Chrome Center Caps w/ 6 lug nuts
	
	
	 
	
	
	

	 
	48” Side Door w/ flush lock, deadbolt & Piano hinge
(See option for extra side door)
	
	
	 
	
	
	

	
	Turn Signals Over Fenders
	
	
	
	
	
	

	
	L.E.D. Taillights in Uprights
	
	
	
	
	
	

	
	Painted Under Carriage – Z-Tech Undercoating
	
	
	
	
	
	

	
	ATP Stoneguard
	
	
	
	
	
	

	
	Spring Asst. Ramp Door A.B.S. Spring Cover & 16’ Flap
	
	
	
	
	
	

	
	2 Cambar Locks on Ramp Door W/2 Grab Handles
	
	
	
	
	
	

	
	Ramp Door Trimmed W/Mill Finish Aluminum
(See option for additional height on ramp door)
	
	
	
	
	
	

	
	4’ Sculpted Beavertail
	
	
	
	
	
	

	
	4-D- Rings Loose
	
	
	
	
	
	

	
	1 Non-Powered Roof Vent
	
	
	
	
	
	

	
	Automotive Style Weather Stripping
	
	
	
	
	
	

	
	2- 12V Lights with Switch
	
	
	
	
	
	

	
	Three Year Factory Warranty
	
	
	
	
	
	

	
	OPTIONAL FEATURES: 
	
	
	
	
	
	

	1
	Fifth Wheel Hitch
	
	
	
	
	
	

	3
	3/5200# Axles Upgrade to 3/6000# Axles

 (16” Tires) 
	
	
	
	
	
	

	1
	12” Extra Height 
	
	
	
	
	
	

	1
	.040 Smooth Side Exterior 7’6” High
(Must add extra height to trailer)
	
	
	
	
	
	

	2
	Large Grab Handle @ RV Door
	
	
	
	
	
	

	1
	Roof Vent: Wired & Framed for Future A/C
	
	
	
	
	
	

	1
	Deluxe Light Package:
2- 4’ Defused Fluorescent Lights

2- 500 Watt 110 V Quartz Lights in Recessed Cast Aluminum boxes

2- 12V Loading Lights

2- 110V Wall Switches

1- 12 V Wall Switch

1-30 Amp Panel W/Life Line

3-110 V Interior Receps

1-12V Dome Light
	
	
	
	
	
	

	1
	50 Amp Panel w/ Life Line in lieu of 30 Amp
	
	
	
	
	
	

	2
	4’ Defused Fluorescent Light
	
	
	
	
	
	

	1
	110V GFI Receptacle
	
	
	
	
	
	

	1
	15,000 BTU Coleman A/C with 12,700 Heat Pump & Remote Thermostat
	
	
	
	
	
	

	2
	12V Dome Light
	
	
	
	
	
	

	 2
	12V Porch Light with Switch
	
	
	
	
	
	

	1
	12V Converter
	
	
	
	
	
	

	1
	12V Battery & Bax
	
	
	
	
	
	

	1
	LED Turn Signals Above Fender (Set of 2)
	
	
	
	
	
	

	1
	LED Running Lights (17) 30Ft. and Larger
	
	
	
	
	
	

	1
	LED Tail Lights (set)
	
	
	
	
	
	

	1
	12V Hitch Light for G N Trailer
	
	
	
	
	
	

	38
	Rubber Black Coin Flooring
	
	
	
	
	
	

	8
	Black Marine Grade Carpeting on Gooseneck Riser
	
	
	
	
	
	

	1
	A T P Ramp Door & Flap 7’6” High
	
	
	
	
	
	

	74
	E-track: Surface Mounted
	
	
	
	
	
	

	1
	Heavy Duty D-Rings:  4 Loose installed
	
	
	
	
	
	

	4
	Heavy Duty Floor D- Rings Installed (4)
	
	
	
	
	
	

	1
	24” Tall Straight Overhead Cabinet
	
	
	
	
	
	

	1
	48” Side Door w/ Flush Lock & Deadbolt
	
	
	
	
	
	

	2
	R V Step
	
	
	
	
	
	

	1
	Recessed Spare-Tire compartment w/ hinged Lid 36”x36”
	
	
	
	
	
	

	3
	30”x22” Radius Slider Window
	
	
	
	
	
	

	1
	30”x22” Egress Window (Roadside)
	
	
	
	
	
	

	1
	Heavy Duty Skid Wheels
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	This Quote includes 2- AC’s
2 Side Doors

(1) 7.0 Generator
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	BASE PRICE:
	
	
	
	
	
	

	
	TOTAL OPTIONS:
	
	
	
	
	
	

	
	LESS DISCOUNT:
	
	
	
	
	
	

	
	BID SUBTOTAL:
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	SHIPPING/FREIGHT:
	
	
	
	
	
	

	
	TAX:
	
	
	
	
	
	

	
	BID TOTAL:
	
	
	
	


Authorized signer approving above pricing 

Signature ___________________________________________________Date__________________________
COMPANY NAME: _________________________________________________________________________

ADDRESS:  ________________________________________________________________________________

CITY:  __________________________________________STATE: _________________ ZIP: ______________

PHONE #:  _______________________________________     FAX #: _________________________________                 
II. REQUEST FOR QUOTE REQUIREMENTS 

1. Communications with the Owner: All communication with the Owner shall comply with the following guidelines.  All communications shall be in writing.  Address all communications (other than DELIVERY of the QUOTE) to the Owner’s project manager at the address noted below. Written communications, including the QUOTE, may also be emailed to cvanvleet@mohave.edu.
Christine Van Vleet, Procurement Manager
Mohave County Community College
1971 Jagerson Avenue

Kingman AZ  86409

Voice:  928-757-0819
FAX:  928-757-0814
cvanvleet@mohave.edu
From the date of issuance of this RFQ, and until a binding contractual agreement is executed with a selected firm, all communications between the Owner and the Bidders or any of their individual members, shall be formal.  Formal communications shall include, but are not be limited to:  (1) general written inquiries,   (2) written questions and answers, (3) written addenda.  

No informal communication shall occur regarding this procurement, including requests for information, comments, speculation, etc., between a Bidder (and any of its individual members,) and any Owner employee or official.  Failure to comply with this provision may result in the rejection of the Quote.
5

