STATE OF NEW HAMPSHIRE

DEPARTMENT OF TRANSPORTATION
7 HAZEN DRIVE

JOHN O. MORTON BUILDING







POST OFFICE BOX 483

CONTRACT SECTION                                              INVITATION FOR BIDS 


CONCORD, NH   03302

Sealed proposals are to be received and deposited in the Bid Box in Room 112 (small conference room) at the John 0. Morton Building, at the address above by 2:00 o'clock PM, Eastern Time, on THURSDAY, JANUARY 7, 2010 for the following project:

GREENLAND

X-A000(825), 15618

THIS SAFETY IMPROVEMENT PROJECT IS LOCATED ON NH ROUTE 33 IN GREENLAND.  THE WORK INVOLVES WIDENING AND OVERLAYING NH ROUTE 33, ADDING LEFT TURN LANES TO NH ROUTE 33, GUARDRAIL WORK, MINOR DRAINAGE IMPROVEMENTS AND THE INSTALLATION OF A TRAFFIC SIGNAL

CERTIFIED CHECK/BID BOND: $50,000.00

A schedule of the minimum wages for all labor classifications as determined by the Secretary of Labor pursuant to Section 115 of the Federal Aid Highway Act of 1956 is included in the proposal. Unskilled labor may be hired from lists prepared by the NH Dept. of Employment Security designated in the proposal.

BIDDERS SHOULD ACT PROMPTLY AND SUBMIT ALL QUESTIONS ON THE PROJECT TO CRAIG GREEN AT (603) 271-2171 AT LEAST FIVE (5) DAYS BEFORE THE HOUR AND DATE SET FOR THE BID OPENING

Plans and specifications (NOT FOR BIDDING PURPOSES) may be seen at the at the Office of Const. Industries of MA, 1500 Providence Hwy., Suite 14, Norwood, MA; at the office of Assoc. General Contractors of NH, 48 Grandview Rd, Bow, NH; FW Dodge Corp. 880 Second Street., Manchester, NH, Construction Summary of NH, Inc., 734 Chestnut St., Manchester, NH, Const. Summary of ME, c/o Cross Insurance Bldg., 2331 Congress St., Portland, ME, Works in Progress, 20 Farrell Street, Suite 103, So. Burlington, VT, Minuteman Press, 109 Gosling Road, Newington, NH, Signature Press & Blueprinting, Inc., 45 Londonderry Turnpike, Hooksett, NH, and Infinite Imaging. 30 International Drive, Suite 6, Portsmouth NH.

NH specifications and proposals forms, FOR BIDDING PURPOSES, shall only be obtained at the Contract Office of the Department of Transportation for THIRTY-FIVE DOLLARS ($35.00) for Plans and specifications NON-REFUNDABLE. An additional FIVE Dollars ($5.00) will be charged for shipping fees NON‑REFUNDABLE.  Bidders must obtain a proposal form from the Department of Transportation to be eligible for bidding. Checks should be made payable to "Treasurer, State of New Hampshire".  Send check with project name and No. to the Dept. of Transportation, c/o Finance & Contracts, P.O. Box 483 Hazen Drive, Concord, NH 03302. 

Proposals must be completed in both words and figures on forms furnished by the Department, or on previously approved substantially‑identical forms generated by computer software, which shall be submitted in a sealed envelope marked "Proposal for:  (GREENLAND X-A000(825), 15618)”  and received by the Department of Transportation as specified above no later than the date and time mentioned above, at which time they will be publicly opened and read aloud. Proposals must be accompanied by a certified check or bid bond in the amount listed above, payable to, "Treasurer, State of New Hampshire," as security for the execution of the contract.

All individuals, firms, partnerships or corporations intending to bid, must file with the Dept. of Transportation on forms prepared for that purpose at least ten (10) days prior to opening of bids, a statement showing their qualifications.  No valid bidding proposal will be issued to a prospective bidder not prequalified.

If contract price is $35,000 or more, the successful bidder will be required to furnish a contract bond in the amount of One hundred (100) percent of their bid on forms furnished by the Department.

All bidders will be required to execute a sworn statement pursuant to Section 112(c) of Title 23 USC, certifying that he or she has not either directly or indirectly, entered into any agreement, participated in any collusion or otherwise taken any action in restraint of free competitive bidding in connection with such contract. Civil Rights Act of 1964,78 Stat. 252, USC 2005d to 2005d‑4 and Title 49, Code of Federal Regulations, Dept. of Transportation, Subtitle A, Office of the Secretary, Part 21, Nondiscrimination in Federally‑assisted programs of the Dept. of Transportation issued pursuant to such Act, hereby notifies all bidders that it will affirmatively insure that in any contract entered into pursuant to this advertisement, minority business enterprises will be afforded full opportunity to submit bids in response to this invitation and will not be discriminated against on the grounds of race, color or national origin in consideration for an award.

The right is reserved to waive any informalities in or to reject any or all proposals.

DECEMBER 8, 2009                         








F                                                                  William J. Cass, P.E. Director of Project Development

                                       STATE OF NEW HAMPSHIRE   

                                  DEPARTMENT  OF  TRANSPORTATION

                                         INFORMATION REPORT 

          PROJECT:                GREENLAND 

                                  X-A000(825), 15618

          COUNTY AND CODE:        ROCKINGHAM 015

          DATE BIDS OPEN:         January 7, 2010   

          SCOPE OF WORK:          ROADWAY REHABILITATION

          LOCATION:               NH ROUTE 33 IN GREENLAND  

          COMPLETION DATE:        August 20, 2010   

          PROPOSAL GUARANTEE:     50,000.00 

          FEDERAL PARTICIPATION:  90%   

                             ESTIMATED QUANTITIES   

                   HWY SAFETY PROG  

                  ITEM               ITEM   

                 NUMBER          DESCRIPTION         UNIT    QUANTITY   

                 202.41    REMOVAL OF EXISTING PIPE 

                            0-24" DIAMETER            LF          210.  

                 202.5     REMOVAL OF CATCH BASINS, 

                            DROP INLETS, AND

                            MANHOLES                  EA            1.  

                 202.7     REMOVAL OF GUARDRAIL (F)   LF          762.5 

                 202.85    REMOVAL OF FLASHING  

                            BEACON                    U             1.  

                 203.1     COMMON EXCAVATION          CY        1,250.  

                 203.5555  GUARDRAIL 25'EAGRT   

                            PLATFORM                  U             4.  

                 203.6     EMBANKMENT-IN-PLACE (F)    CY          212.  

                 206.1     COMMON STRUCTURE 

                            EXCAVATION                CY          500.  

                 209.4     GRANULAR BACKFILL (GRAV)   CY           75.  

                 214.      FINE GRADING               U             1.  

                 304.1     SAND (F)                   CY          547.  

                 304.32    CRUSHED GRAVEL FOR   

                            SHOULDER LEVELING         TON          40.  

                 304.35    CRUSHED GRAVEL FOR DRIVES  CY           10.  

                 304.4     CRUSHED STONE (FINE  

                            GRADATION) (F)            CY          277.  

                 304.5     CRUSHED STONE (COARSE

                            GRADATION) (F)            CY          188.  

                                         1  

                                            15618   

                 403.11    HOT BITUMINOUS PAVEMENT, 

                            MACHINE METHOD            TON       1,150.  

                 403.1109  HOT BITUMINOUS PAVEMENT  

                            MACHINE METHOD, HIGH

                            STRENGTH                  TON         810.  

                 403.12    HOT BITUMINOUS PAVEMENT, 

                            HAND METHOD               TON          80.  

                 403.6     PAVEMENT JOINT ADHESIVE    LF        5,650.  

                 403.99    TEMPORARY BITUMINOUS 

                            PAVEMENT                  TON          10.  

                 417.      COLD PLANING BITUMINOUS  

                            SURFACES                  SY        4,100.  

                 570.4     MORTAR RUBBLE MASONRY (F)  CY            1.7 

                 585.3     STONE FILL, CLASS C        CY           15.  

                 593.411   GEOTEXTILE; PERM CONTROL 

                            CL.1, NON-WOVEN           SY           40.  

                 603.00218 18" R.C. PIPE, 2000D       LF           20.  

                 603.34118 18" STEEL END SECTIONS     EA            1.  

                 603.83218 18" PLASTIC PIPE (SMOOTH 

                            INTERIOR)                 LF          250.  

                 604.12    CATCH BASINS TYPE B        U             4.  

                 606.120   BEAM GUARDRAIL (STANDARD 

                            SECTION-STEEL POST)       LF          762.5 

                 606.1455  BEAM GUARDRAIL (TERM.

                            UNIT EAGRT 25 FT.)        U             4.  

                 608.12    2" BITUMINOUS

                            SIDEWALK (F)              SY            6.  

                 609.01    STRAIGHT GRANITE CURB      LF          130.  

                 611.90001 ADJUSTING WATER GATES AND

                            SHUTOFFS SET BY OTHERS    EA            1.  

                 614.331   3" STEEL CONDUIT           LF           15.  

                 614.522   MOLDED PULL BOX 13"X24"    EA           15.  

                 614.7414  4" PVC PLASTIC CONDUIT,  

                            SCHEDULE 40               LF        1,100.  

                 614.7418  4" PVC PLASTIC CONDUIT,  

                            SCHEDULE 80               LF          250.  

                 615.03    TRAFFIC SIGN TYPE C (F)    SF           69.  

                 615.06    TRAFFIC SIGN TYPE CC (F)   SF            8.  

                 616.101   TRAFFIC SIGNALS            U             1.  

                 618.61    UNIFORMED OFFICERS WITH  

                            VEHICLE                        AS SHOWN IN  

                                                             PROPOSAL   

                 618.7     FLAGGERS                   HR          800.  

                 619.1     MAINTENANCE OF TRAFFIC     U             1.  

                 619.25    PORTABLE CHANGEABLE  

                            MESSAGE SIGN              U             2.  

                 619.253   PORTABLE CHANGEABLE  

                            MESSAGE SIGN (UNIT WEEK)  UWK           4.  

                 621.2     RETROREFLECTIVE BEAM 

                            GUARDRAIL DELINEATOR      EA           15.  

                 621.31    SINGLE DELINEATOR WITH   

                            POST                      EA           35.  

                 622.1     STEEL WITNESS MARKERS      EA            5.  

                 628.2     SAWED BITUMINOUS PAVEMENT  LF        1,550.  
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                 632.0104  RETROREFLECTIVE PAINT

                            PAVE. MARKING, 4" LINE    LF       49,100.  

                 632.3104  RETROREFLECT. THERMOPLAS.

                            PAVE. MARKING, 4" LINE    LF          300.  

                 632.3106  RETROREFLECT. THERMOPLAS.

                            PAVE. MARKING, 6" LINE    LF          130.  

                 632.3118  RETROREFLECT. THERMOPLAS.

                            PAVE. MARKING, 18" LINE   LF          110.  

                 632.32    RETROREFLECT. THERMOPLAS.

                            PAVEMENT MARKING, SYMBOL

                            OR WORD                   SF          130.  

                 632.9118  OBLITERATE PAVEMENT  

                            MARKING, 18" LINE         LF           50.  

                 641.      LOAM                       CY          400.  

                 645.3     EROSION STONE              TON         250.  

                 645.43    TEMPORARY SLOPE  

                            STABILIZATION TYPE C      SY        5,000.  

                 645.46    PERMANENT CHANNEL

                            STABILIZATION TYPE B      SY          550.  

                 645.531   SILT FENCE                 LF        1,300.  

                 645.7     STORM WATER POLLUTION

                            PREVENTION PLAN           U             1.  

                 645.71    MONITORING SWPPP AND 

                            EROSION AND SEDIMENT

                            CONTROLS                  HR          110.  

                 646.31    TURF ESTABLISHMENT WITH  

                            MULCH AND TACKIFIERS      SY        5,100.  

                 647.1     HUMUS                      CY          160.  

                 692.      MOBILIZATION               U             1.  

                 698.14    FIELD OFFICE TYPE D        MON          10.  

                 699.      MISCELLANEOUS TEMPORARY  

                            EROSION AND SEDIMENT           AS SHOWN IN  

                            CONTROL                          PROPOSAL   

                1008.11    ALTERATIONS AND ADDITIONS

                            AS NEEDED-                     AS SHOWN IN  

                            UNANTICIPATED WORK               PROPOSAL   

                1010.15    FUEL ADJUSTMENT  

                                                           AS SHOWN IN  

                                                             PROPOSAL   
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